IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition[CoordinationView_V2.0, QuantityTakeOffAddOnView]"
Description: "Option [BaseQuantities:On]"
Description: "Option [GridExport:Off]"
Description: "Option [Assemblies:Off]"
Description: "Option [Bolts:On]"
Description: "Option [Rebars:On]"
Description: "Option [PourObjects:Off]"
Description: "Option [Welds:Off]"
Description: "Option [SurfaceTreatments:On]"
Description: "Option [LocationBy:0]"
Description: "Option [ViewColors:Off]"
Description: "Option [SectionedSpine:Off]"
Description: "Option [PropertySets:On]"
Description: "Option [Export all:Off]"
File name: "MHBT3_RIB.ifc"
Time stamp: "2024-04-25T14:01:47"
Author: "CORETECH\anders"
Organization: "Structural Designer"
Preprocessor: "IFC Database Version: Work"
Originating system: "Tekla Structures 2020 Service Pack 13, IFC Export Version: 4.0.0.0 May 4 2022"
Application: "Tekla Structures" version "2020 Service Pack 13" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation"

People and organizations
  Person "Undefined" id "CORETECH\anders" of Organization "Trimble Solutions Corporation"
  Owner history of Person "Undefined" id "CORETECH\anders" of Organization "Trimble Solutions Corporation" | application "Tekla Structures" version "2020 Service Pack 13" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | change NOCHANGE | created 1714046499 (2024-04-25T12:01:39Z)
  Owner history of Person "Undefined" id "CORETECH\anders" of Organization "Trimble Solutions Corporation" | application "Tekla Structures" version "2020 Service Pack 13" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | change NOCHANGE | created 1714053600 (2024-04-25T14:00:00Z)
  Owner history of Person "Undefined" id "CORETECH\anders" of Organization "Trimble Solutions Corporation" | application "Tekla Structures" version "2020 Service Pack 13" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | change NOCHANGE | created 1713974400 (2024-04-24T16:00:00Z)
  Owner history of Person "Undefined" id "CORETECH\anders" of Organization "Trimble Solutions Corporation" | application "Tekla Structures" version "2020 Service Pack 13" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | change NOCHANGE | created 1713852000 (2024-04-23T06:00:00Z)
  Owner history of Person "Undefined" id "CORETECH\anders" of Organization "Trimble Solutions Corporation" | application "Tekla Structures" version "2020 Service Pack 13" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | change NOCHANGE | created 1713816000 (2024-04-22T20:00:00Z)
  Owner history of Person "Undefined" id "CORETECH\anders" of Organization "Trimble Solutions Corporation" | application "Tekla Structures" version "2020 Service Pack 13" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | change NOCHANGE | created 1713258000 (2024-04-16T09:00:00Z)
  Owner history of Person "Undefined" id "CORETECH\anders" of Organization "Trimble Solutions Corporation" | application "Tekla Structures" version "2020 Service Pack 13" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | change NOCHANGE | created 1712667600 (2024-04-09T13:00:00Z)
  Owner history of Person "Undefined" id "CORETECH\anders" of Organization "Trimble Solutions Corporation" | application "Tekla Structures" version "2020 Service Pack 13" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | change NOCHANGE | created 1643112000 (2022-01-25T12:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  PLANEANGLEUNIT: RADIAN
  SOLIDANGLEUNIT: STERADIAN
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Project"
  IFCSITE "Hillevågsveien 24"
    IFCBUILDING "Bygningens navn"
      IFCBUILDINGSTOREY "02" | elevation 17420.
        contains 91 elements
          7 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*200" | object type "3000*200" | names: "BETONGVEGG" | descriptions: "3000*200" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 200.); layers "Wall: Insitu CONCRETE/B45" ("CONCRETE/B45" 200.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*220" | object type "3000*220" | names: "BETONGVEGG" | descriptions: "3000*220" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 220.) | property sets: Tekla Common, Pset_WallCommon, Tekla Quantity, BaseQuantities
          4 x IFCWALL | type IFCWALLTYPE "3000*200" | object type "3000*200" | names: "BETONGVEGG" | descriptions: "3000*200" | material: "CONCRETE/B30"; "CONCRETE/B45" | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "250*2202" | object type "250*2202" | FLOOR | names: "BALKONG" | descriptions: "250*2202" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 250.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          5 x IFCSLAB | type IFCSLABTYPE "250*2160" | object type "250*2160" | FLOOR | names: "BALKONG" | descriptions: "250*2160" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 250.) | property sets: Pset_SlabCommon, Tekla Quantity, Tekla Common, BaseQuantities
          3 x IFCWALL | type IFCWALLTYPE "3000*220" | object type "3000*220" | names: "BETONGVEGG" | descriptions: "3000*220" | material: "CONCRETE/B30"; "CONCRETE/B45" | property sets: Tekla Common, Pset_WallCommon, Tekla Quantity, BaseQuantities
          7 x IFCCOLUMN | type IFCCOLUMNTYPE "RHS200*100*16" | object type "RHS200*100*16" | names: "STÅLSØYLE" | descriptions: "RHS200*100*16" | material: "STEEL/S355J0" | property sets: Pset_ColumnCommon, Tekla Quantity, Tekla Common, BaseQuantities
          10 x IFCCOLUMN | type IFCCOLUMNTYPE "CFRHS200X100X12.5" | object type "CFRHS200X100X12.5" | names: "STÅLSØYLE" | descriptions: "CFRHS200X100X12.5" | material: "STEEL/S355J0" | property sets: Pset_ColumnCommon, Tekla Quantity, Tekla Common, BaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "UPE270" | object type "UPE270" | names: "STÅLBJELKE" | descriptions: "UPE270" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          10 x IFCBEAM | type IFCBEAMTYPE "HD320" | object type "HD320" | names: "HULLDEKKE" | descriptions: "HD320" | material: "CONCRETE/B45" | property sets: Pset_BeamCommon, Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCSLAB | type IFCSLABTYPE "220*2100" | object type "220*2100" | FLOOR | names: "Forsenket dekke" | descriptions: "220*2100" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 220.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "250*12420" | object type "250*12420" | FLOOR | names: "Betongdekke" | descriptions: "250*12420" | material: layers "Floor: Insitu CONCRETE/B30" ("CONCRETE/B30" 250.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "D20-400" | object type "D20-400" | names: "Deltabjelke" | descriptions: "D20-400" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Quantity, Tekla Common, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "120*2065" | object type "120*2065" | FLOOR | names: "Bad" | descriptions: "120*2065" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 120.) | property sets: Pset_SlabCommon, Tekla Quantity, Tekla Common, BaseQuantities
          2 x IFCSLAB | type IFCSLABTYPE "120*1817" | object type "120*1817" | FLOOR | names: "Bad" | descriptions: "120*1817" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 120.) | property sets: Pset_SlabCommon, Tekla Quantity, Tekla Common, BaseQuantities
          2 x IFCSLAB | type IFCSLABTYPE "120*1780" | object type "120*1780" | FLOOR | names: "Bad" | descriptions: "120*1780" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 120.) | property sets: Pset_SlabCommon, Tekla Quantity, Tekla Common, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "120*1700" | object type "120*1700" | FLOOR | names: "Bad" | descriptions: "120*1700" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 120.) | property sets: Pset_SlabCommon, Tekla Quantity, Tekla Common, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "250*200" | object type "250*200" | names: "Konsoll" | descriptions: "250*200" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 200.) | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "270*21040" | object type "270*21040" | FLOOR | names: "BETONGDEKKE" | descriptions: "270*21040" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          10 x IFCCOLUMN | type IFCCOLUMNTYPE "RHS200*100*12.5" | object type "RHS200*100*12.5" | names: "STÅLSØYLE" | descriptions: "RHS200*100*12.5" | material: "STEEL/S355J0" | property sets: Pset_ColumnCommon, Tekla Quantity, Tekla Common, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "270*2170" | object type "270*2170" | FLOOR | names: "BALKONG" | descriptions: "270*2170" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "270*2280" | object type "270*2280" | FLOOR | names: "BALKONG" | descriptions: "270*2280" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          3 x IFCBEAM | type IFCBEAMTYPE "IPE240" | object type "IPE240" | names: "STÅLBJELKE" | descriptions: "IPE240" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Quantity, Tekla Common, BaseQuantities
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*250" | object type "3000*250" | names: "BETONGVEGG" | descriptions: "3000*250" | material: layers "Wall: Insitu CONCRETE/B45" ("CONCRETE/B45" 250.) | property sets: Pset_WallCommon, Tekla Quantity, BaseQuantities, Tekla Common
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*300" | object type "3000*300" | names: "BETONGVEGG" | descriptions: "3000*300" | material: layers "Wall: Insitu CONCRETE/B45" ("CONCRETE/B45" 300.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCWALL | type IFCWALLTYPE "3000*250" | object type "3000*250" | names: "BETONGVEGG" | descriptions: "3000*250" | material: "CONCRETE/B45" | property sets: Pset_WallCommon, Tekla Quantity, BaseQuantities, Tekla Common
      IFCBUILDINGSTOREY "Hav" | elevation 0.
        contains 109 elements
          10 x IFCFOOTING | object type "400*1000" | names: "B2" | descriptions: "400*1000" | material: "CONCRETE/B30" | property sets: Tekla Common, Tekla Quantity, BaseQuantities
          3 x IFCFOOTING | object type "300*1500" | names: "B1", "Bankett" | descriptions: "300*1500" | material: "CONCRETE/B30" | property sets: Tekla Common, Tekla Quantity, BaseQuantities
          15 x IFCFOOTING | object type "1400*1400" | names: "F1" | descriptions: "1400*1400" | material: "CONCRETE/B30" | property sets: Tekla Common, Tekla Quantity, BaseQuantities
          4 x IFCFOOTING | object type "1750*1750" | names: "F2" | descriptions: "1750*1750" | material: "CONCRETE/B30" | property sets: Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCFOOTING | object type "2300*3000" | names: "Heisgrube" | descriptions: "2300*3000" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity, BaseQuantities
          7 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "1220*300" | object type "1220*300" | names: "Heisgrube" | descriptions: "1220*300" | material: layers "Wall: Insitu CONCRETE/B35" ("CONCRETE/B35" 300.); layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 300.) | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          1 x IFCPLATE | type IFCPLATETYPE "10*62145" | object type "10*62145" | names: "X-Sprengenivå" | descriptions: "10*62145" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Tekla Common, Tekla Quantity, Pset_PlateCommon, BaseQuantities
          1 x IFCFOOTING | object type "10000*4000" | names: "X-Sprengenivå" | descriptions: "10000*4000" | material: "CONCRETE/B30" | property sets: Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCPLATE | type IFCPLATETYPE "10*2000" | object type "10*2000" | names: "X-Sprengenivå" | descriptions: "10*2000" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Tekla Common, Tekla Quantity, Pset_PlateCommon, BaseQuantities
          1 x IFCPLATE | type IFCPLATETYPE "10*11327" | object type "10*11327" | names: "X-Sprengenivå" | descriptions: "10*11327" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Tekla Common, Tekla Quantity, Pset_PlateCommon, BaseQuantities
          1 x IFCPLATE | type IFCPLATETYPE "10*1999" | object type "10*1999" | names: "X-Sprengenivå" | descriptions: "10*1999" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Tekla Common, Tekla Quantity, Pset_PlateCommon, BaseQuantities
          48 x IFCBEAM | type IFCBEAMTYPE "D75" | object type "D75" | names: "KORR.RØR Ø75" | descriptions: "D75" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Tekla Quantity, Tekla Common, Pset_BeamCommon, BaseQuantities
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "D5" | object type "D5" | names: "Koordpunkt" | descriptions: "D5" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity, Pset_ColumnCommon, BaseQuantities
          10 x IFCFOOTING | object type "2000*2000" | names: "F3" | descriptions: "2000*2000" | material: "CONCRETE/B30" | property sets: Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCFOOTING | object type "4600*3400" | names: "Heisgrube" | descriptions: "4600*3400" | material: "CONCRETE/B30" | property sets: Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "1220*250" | object type "1220*250" | names: "Heisgrube" | descriptions: "1220*250" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 250.) | property sets: Tekla Common, Pset_WallCommon, Tekla Quantity, BaseQuantities
          1 x IFCFOOTING | object type "500*7580" | names: "Bunnplate" | descriptions: "500*7580" | material: "CONCRETE/B30" | property sets: Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCFOOTING | object type "500*1200" | names: "Bankett" | descriptions: "500*1200" | material: "CONCRETE/B30" | property sets: Tekla Common, Tekla Quantity, BaseQuantities
      IFCBUILDINGSTOREY "01" | elevation 14420.
        contains 183 elements
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3050*220" | object type "3050*220" | names: "BETONGVEGG" | descriptions: "3050*220" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 220.) | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3050*200" | object type "3050*200" | names: "BETONGVEGG" | descriptions: "3050*200" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 200.) | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          2 x IFCWALL | type IFCWALLTYPE "3050*200" | object type "3050*200" | names: "BETONGVEGG" | descriptions: "3050*200" | material: "CONCRETE/B30" | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3350*300" | object type "3350*300" | names: "BETONGVEGG" | descriptions: "3350*300" | material: layers "Wall: Insitu CONCRETE/B45" ("CONCRETE/B45" 300.) | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "2955*220" | object type "2955*220" | names: "BETONGVEGG" | descriptions: "2955*220" | material: layers "Wall: Insitu CONCRETE/B45" ("CONCRETE/B45" 220.); layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 220.) | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          2 x IFCSLAB | type IFCSLABTYPE "250*2180" | object type "250*2180" | FLOOR | names: "BALKONG" | descriptions: "250*2180" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 250.) | property sets: Tekla Common, Tekla Quantity, Pset_SlabCommon, BaseQuantities
          1 x IFCWALL | type IFCWALLTYPE "2955*220" | object type "2955*220" | names: "BETONGVEGG" | descriptions: "2955*220" | material: "CONCRETE/B30" | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          8 x IFCCOLUMN | type IFCCOLUMNTYPE "RHS200*100*16" | object type "RHS200*100*16" | names: "STÅLSØYLE" | descriptions: "RHS200*100*16" | material: "STEEL/S355J0" | property sets: Pset_ColumnCommon, Tekla Common, Tekla Quantity, BaseQuantities
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3350*220" | object type "3350*220" | names: "BETONGVEGG" | descriptions: "3350*220" | material: layers "Wall: Insitu CONCRETE/B45" ("CONCRETE/B45" 220.); layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 220.) | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          1 x IFCWALL | type IFCWALLTYPE "3350*220" | object type "3350*220" | names: "BETONGVEGG" | descriptions: "3350*220" | material: "CONCRETE/B30" | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          4 x IFCCOLUMN | type IFCCOLUMNTYPE "RHS200*100*12.5" | object type "RHS200*100*12.5" | names: "STÅLSØYLE" | descriptions: "RHS200*100*12.5" | material: "STEEL/S355J0" | property sets: Pset_ColumnCommon, Tekla Common, Tekla Quantity, BaseQuantities
          3 x IFCBEAM | type IFCBEAMTYPE "UPE270" | object type "UPE270" | names: "STÅLBJELKE" | descriptions: "UPE270" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          18 x IFCCOLUMN | type IFCCOLUMNTYPE "HEA140" | object type "HEA140" | names: "STÅLSØYLE" | descriptions: "HEA140" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity, Pset_ColumnCommon, BaseQuantities
          4 x IFCMEMBER | type IFCMEMBERTYPE "D25" | object type "D25" | names: "Kamstål" | descriptions: "D25" | material: "REBAR/B500NC" | property sets: Tekla Quantity, Pset_MemberCommon, Tekla Common, BaseQuantities
          9 x IFCBEAM | type IFCBEAMTYPE "D12" | object type "D12" | names: "Kamstål" | descriptions: "D12" | material: "REBAR/B500NC" | property sets: Tekla Quantity, Pset_BeamCommon, Tekla Common, BaseQuantities
          4 x IFCWALL | type IFCWALLTYPE "1300*100" | object type "1300*100" | names: "Støyskjerm" | descriptions: "1300*100" | material: "CONCRETE/B30" | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          1 x IFCWALL | type IFCWALLTYPE "1400*100" | object type "1400*100" | names: "Støyskjerm" | descriptions: "1400*100" | material: "CONCRETE/B30" | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "1660*100" | object type "1660*100" | names: "Støyskjerm" | descriptions: "1660*100" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 100.) | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "1300*100" | object type "1300*100" | names: "Støyskjerm" | descriptions: "1300*100" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 100.) | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          1 x IFCWALL | type IFCWALLTYPE "1600*100" | object type "1600*100" | names: "Støyskjerm" | descriptions: "1600*100" | material: "CONCRETE/B30" | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          18 x IFCBEAM | type IFCBEAMTYPE "PL15*300" | object type "PL15*300" | names: "Unnamed" | descriptions: "PL15*300" | material: "STEEL/S355J2G3" | property sets: Tekla Quantity, Pset_BeamCommon, Tekla Common, BaseQuantities
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "2950*500" | object type "2950*500" | names: "Pilaster" | descriptions: "2950*500" | material: layers "Wall: Insitu CONCRETE/B45" ("CONCRETE/B45" 500.) | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3150*500" | object type "3150*500" | names: "Pilaster" | descriptions: "3150*500" | material: layers "Wall: Insitu CONCRETE/B45" ("CONCRETE/B45" 500.) | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "1080*1333" | object type "1080*1333" | FLOOR | names: "TRAPP" | descriptions: "1080*1333" | material: layers "Floor: Insitu CONCRETE/B30-SKB" ("CONCRETE/B30-SKB" 1080.) | property sets: Tekla Common, Tekla Quantity, Pset_SlabCommon, BaseQuantities
          1 x IFCCOVERING | object type "arm-tegn, verv v. BT3" | names: "arm-tegn, verv v. BT3" | material: "Undefined/Undefined"
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "250*250" | object type "250*250" | names: "Mangler 6ø16 ift arm-" | descriptions: "250*250" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 250.) | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          1 x IFCWALL | type IFCWALLTYPE "6200*220" | object type "6200*220" | names: "Betong 220mm" | descriptions: "6200*220" | material: "CONCRETE/B45" | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "250*12400" | object type "250*12400" | FLOOR | names: "Betongdekke" | descriptions: "250*12400" | material: layers "Floor: Insitu CONCRETE/B30" ("CONCRETE/B30" 250.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          4 x IFCCOLUMN | type IFCCOLUMNTYPE "RHS88.9X7.1" | object type "RHS88.9X7.1" | names: "STÅLSØYLE-Galv" | descriptions: "RHS88.9X7.1" | material: "STEEL/S355J0" | property sets: Pset_ColumnCommon, Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCSLAB | type IFCSLABTYPE "120*2234" | object type "120*2234" | FLOOR | names: "Bad" | descriptions: "120*2234" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 120.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCSLAB | type IFCSLABTYPE "120*1817" | object type "120*1817" | FLOOR | names: "Bad" | descriptions: "120*1817" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 120.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCSLAB | type IFCSLABTYPE "120*2136" | object type "120*2136" | FLOOR | names: "Bad" | descriptions: "120*2136" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 120.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCPLATE | type IFCPLATETYPE "PL25*250" | object type "PL25*250" | names: "PLATE" | descriptions: "PL25*250" | material: "STEEL/S355J2H" | property sets: Tekla Common, Tekla Quantity, Pset_PlateCommon, BaseQuantities
          2 x IFCPLATE | type IFCPLATETYPE "PL15*250" | object type "PL15*250" | names: "PLATE" | descriptions: "PL15*250" | material: "STEEL/S355J2H" | property sets: Tekla Common, Tekla Quantity, Pset_PlateCommon, BaseQuantities
          8 x IFCBEAM | type IFCBEAMTYPE "D32" | object type "D32" | names: "Kamstål" | descriptions: "D32" | material: "REBAR/B500NC" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          2 x IFCPLATE | type IFCPLATETYPE "PL25*150" | object type "PL25*150" | names: "PLATE" | descriptions: "PL25*150" | material: "STEEL/S355J2H" | property sets: Tekla Common, Tekla Quantity, Pset_PlateCommon, BaseQuantities
          28 x IFCBEAM | type IFCBEAMTYPE "D16" | object type "D16" | names: "Kamstål" | descriptions: "D16" | material: "REBAR/B500NC" | property sets: Tekla Quantity, Pset_BeamCommon, Tekla Common, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "6450*300" | object type "6450*300" | names: "BETONGVEGG" | descriptions: "6450*300" | material: layers "Wall: Insitu CONCRETE/B45" ("CONCRETE/B45" 300.) | property sets: Tekla Common, Pset_WallCommon, Tekla Quantity, BaseQuantities
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "400*600" | object type "400*600" | names: "BETONGSØYLE" | descriptions: "400*600" | material: "CONCRETE/B45" | property sets: Pset_ColumnCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "D750" | object type "D750" | names: "BETONGSØYLE" | descriptions: "D750" | material: "CONCRETE/B55" | property sets: Pset_ColumnCommon, Tekla Common, Tekla Quantity, BaseQuantities
          6 x IFCCOLUMN | type IFCCOLUMNTYPE "CFRHS200X100X12.5" | object type "CFRHS200X100X12.5" | names: "STÅLSØYLE" | descriptions: "CFRHS200X100X12.5" | material: "STEEL/S355J0" | property sets: Pset_ColumnCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "220*2550" | object type "220*2550" | FLOOR | names: "Forsenket dekke" | descriptions: "220*2550" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 220.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "220*2440" | object type "220*2440" | FLOOR | names: "Forsenket dekke" | descriptions: "220*2440" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 220.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "600*600" | object type "600*600" | names: "BETONGSØYLE" | descriptions: "600*600" | material: "CONCRETE/B45" | property sets: Tekla Common, Pset_ColumnCommon, Tekla Quantity, BaseQuantities
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "300*500" | object type "300*500" | names: "BETONGSØYLE" | descriptions: "300*500" | material: "CONCRETE/B45" | property sets: Pset_ColumnCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "200*600" | object type "200*600" | names: "BETONGSØYLE" | descriptions: "200*600" | material: "CONCRETE/B45" | property sets: Pset_ColumnCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCMEMBER | type IFCMEMBERTYPE "CFRHS250X150X12.5" | object type "CFRHS250X150X12.5" | names: "STÅLBJELKE" | descriptions: "CFRHS250X150X12.5" | material: "STEEL/S355J0" | property sets: Tekla Quantity, Pset_MemberCommon, Tekla Common, BaseQuantities
          4 x IFCCOLUMN | type IFCCOLUMNTYPE "CFRHS80X8" | object type "CFRHS80X8" | names: "STÅLSØYLE" | descriptions: "CFRHS80X8" | material: "STEEL/S355J0" | property sets: Pset_ColumnCommon, Tekla Common, Tekla Quantity, BaseQuantities
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3350*250" | object type "3350*250" | names: "BETONGVEGG" | descriptions: "3350*250" | material: layers "Wall: Insitu CONCRETE/B45" ("CONCRETE/B45" 250.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCWALL | type IFCWALLTYPE "3350*250" | object type "3350*250" | names: "BETONGVEGG" | descriptions: "3350*250" | material: "CONCRETE/B45" | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCWALL | type IFCWALLTYPE "3350*200" | object type "3350*200" | names: "BETONGVEGG" | descriptions: "3350*200" | material: "CONCRETE/B45" | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3350*200" | object type "3350*200" | names: "BETONGVEGG" | descriptions: "3350*200" | material: layers "Wall: Insitu CONCRETE/B45" ("CONCRETE/B45" 200.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCWALL | type IFCWALLTYPE "3550*300" | object type "3550*300" | names: "BETONGVEGG" | descriptions: "3550*300" | material: "CONCRETE/B45" | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "270*15080" | object type "270*15080" | FLOOR | names: "BETONGDEKKE" | descriptions: "270*15080" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
      IFCBUILDINGSTOREY "06" | elevation 29420.
        contains 101 elements
          7 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*200" | object type "3000*200" | names: "BETONGVEGG" | descriptions: "3000*200" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 200.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          6 x IFCWALL | type IFCWALLTYPE "3000*220" | object type "3000*220" | names: "BETONGVEGG" | descriptions: "3000*220" | material: "CONCRETE/B30" | property sets: Pset_WallCommon, Tekla Quantity, Tekla Common, BaseQuantities
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*220" | object type "3000*220" | names: "BETONGVEGG" | descriptions: "3000*220" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 220.) | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          4 x IFCWALL | type IFCWALLTYPE "3000*200" | object type "3000*200" | names: "BETONGVEGG" | descriptions: "3000*200" | material: "CONCRETE/B30" | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          4 x IFCBEAM | type IFCBEAMTYPE "D20-400" | object type "D20-400" | names: "Deltabjelke" | descriptions: "D20-400" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Quantity, Tekla Common, BaseQuantities
          4 x IFCSLAB | type IFCSLABTYPE "250*2160" | object type "250*2160" | FLOOR | names: "BALKONG" | descriptions: "250*2160" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 250.) | property sets: Pset_SlabCommon, Tekla Quantity, Tekla Common, BaseQuantities
          8 x IFCCOLUMN | type IFCCOLUMNTYPE "CFRHS200X100X8" | object type "CFRHS200X100X8" | names: "STÅLSØYLE" | descriptions: "CFRHS200X100X8" | material: "STEEL/S355J0" | property sets: Pset_ColumnCommon, Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCSLAB | type IFCSLABTYPE "270*1987" | object type "270*1987" | FLOOR | names: "BALKONG" | descriptions: "270*1987" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Tekla Quantity, Pset_SlabCommon, Tekla Common, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "250*12400" | object type "250*12400" | FLOOR | names: "Betongdekke" | descriptions: "250*12400" | material: layers "Floor: Insitu CONCRETE/B30" ("CONCRETE/B30" 250.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCSLAB | type IFCSLABTYPE "120*1817" | object type "120*1817" | FLOOR | names: "Bad" | descriptions: "120*1817" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 120.) | property sets: Pset_SlabCommon, Tekla Quantity, Tekla Common, BaseQuantities
          2 x IFCSLAB | type IFCSLABTYPE "120*1780" | object type "120*1780" | FLOOR | names: "Bad" | descriptions: "120*1780" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 120.) | property sets: Pset_SlabCommon, Tekla Quantity, Tekla Common, BaseQuantities
          4 x IFCBEAM | type IFCBEAMTYPE "370*150" | object type "370*150" | names: "Teglkon(eks.Ytong)" | descriptions: "370*150" | material: "CONCRETE/B35" | property sets: Pset_BeamCommon, Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "L200*14" | object type "L200*14" | names: "TEGLKONSOLL-HALFEN" | descriptions: "L200*14" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Common, Tekla Quantity, BaseQuantities
          11 x IFCCOLUMN | type IFCCOLUMNTYPE "RHS200*100*16" | object type "RHS200*100*16" | names: "STÅLSØYLE" | descriptions: "RHS200*100*16" | material: "STEEL/S355J0" | property sets: Pset_ColumnCommon, Tekla Quantity, Tekla Common, BaseQuantities
          23 x IFCCOLUMN | type IFCCOLUMNTYPE "CFRHS200X100X12.5" | object type "CFRHS200X100X12.5" | names: "STÅLSØYLE" | descriptions: "CFRHS200X100X12.5" | material: "STEEL/S355J0" | property sets: Pset_ColumnCommon, Tekla Quantity, Tekla Common, BaseQuantities
          2 x IFCMEMBER | type IFCMEMBERTYPE "CFRHS80X6" | object type "CFRHS80X6" | names: "STÅLBJELKE" | descriptions: "CFRHS80X6" | material: "STEEL/S355J0" | property sets: Pset_MemberCommon, Tekla Quantity, Tekla Common, BaseQuantities
          3 x IFCBEAM | type IFCBEAMTYPE "IPE240" | object type "IPE240" | names: "STÅLBJELKE" | descriptions: "IPE240" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Quantity, Tekla Common, BaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "IPE300" | object type "IPE300" | names: "STÅLBJELKE" | descriptions: "IPE300" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Quantity, BaseQuantities, Tekla Common
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*250" | object type "3000*250" | names: "BETONGVEGG" | descriptions: "3000*250" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 250.); layers "Wall: Insitu CONCRETE/B45" ("CONCRETE/B45" 250.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCWALL | type IFCWALLTYPE "3000*250" | object type "3000*250" | names: "BETONGVEGG" | descriptions: "3000*250" | material: "CONCRETE/B30" | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "2730*250" | object type "2730*250" | names: "BETONGVEGG" | descriptions: "2730*250" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 250.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "270*2170" | object type "270*2170" | FLOOR | names: "BALKONG" | descriptions: "270*2170" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "UPE270" | object type "UPE270" | names: "STÅLBJELKE" | descriptions: "UPE270" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "270*20150" | object type "270*20150" | FLOOR | names: "BETONGDEKKE" | descriptions: "270*20150" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "270*2100" | object type "270*2100" | FLOOR | names: "BALKONG" | descriptions: "270*2100" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
      IFCBUILDINGSTOREY "07" | elevation 32420.
        contains 99 elements
          5 x IFCBEAM | type IFCBEAMTYPE "D20-400" | object type "D20-400" | names: "Deltabjelke" | descriptions: "D20-400" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Common, Tekla Quantity, BaseQuantities
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3650*220" | object type "3650*220" | names: "BETONGVEGG" | descriptions: "3650*220" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 220.) | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3650*200" | object type "3650*200" | names: "BETONGVEGG" | descriptions: "3650*200" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 200.) | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          4 x IFCWALL | type IFCWALLTYPE "3000*220" | object type "3000*220" | names: "BETONGVEGG" | descriptions: "3000*220" | material: "CONCRETE/B30" | property sets: Tekla Common, Pset_WallCommon, Tekla Quantity, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "250*12400" | object type "250*12400" | FLOOR | names: "Betongdekke" | descriptions: "250*12400" | material: layers "Floor: Insitu CONCRETE/B30" ("CONCRETE/B30" 250.) | property sets: Pset_SlabCommon, Tekla Quantity, Tekla Common, BaseQuantities
          5 x IFCBEAM | type IFCBEAMTYPE "UPE270" | object type "UPE270" | names: "STÅLBJELKE" | descriptions: "UPE270" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCSLAB | type IFCSLABTYPE "270*1987" | object type "270*1987" | FLOOR | names: "BALKONG" | descriptions: "270*1987" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Tekla Common, Tekla Quantity, Pset_SlabCommon, BaseQuantities
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*200" | object type "3000*200" | names: "BETONGVEGG" | descriptions: "3000*200" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 200.) | property sets: Tekla Common, Pset_WallCommon, Tekla Quantity, BaseQuantities
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*220" | object type "3000*220" | names: "BETONGVEGG" | descriptions: "3000*220" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 220.) | property sets: Tekla Common, Pset_WallCommon, Tekla Quantity, BaseQuantities
          4 x IFCSLAB | type IFCSLABTYPE "250*2160" | object type "250*2160" | FLOOR | names: "BALKONG" | descriptions: "250*2160" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 250.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCWALL | type IFCWALLTYPE "3000*200" | object type "3000*200" | names: "BETONGVEGG" | descriptions: "3000*200" | material: "CONCRETE/B30" | property sets: Tekla Common, Pset_WallCommon, Tekla Quantity, BaseQuantities
          11 x IFCCOLUMN | type IFCCOLUMNTYPE "CFRHS100X8" | object type "CFRHS100X8" | names: "STÅLSØYLE" | descriptions: "CFRHS100X8" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity, Pset_ColumnCommon, BaseQuantities
          2 x IFCSLAB | type IFCSLABTYPE "120*1817" | object type "120*1817" | FLOOR | names: "Bad" | descriptions: "120*1817" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 120.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCSLAB | type IFCSLABTYPE "120*1780" | object type "120*1780" | FLOOR | names: "Bad" | descriptions: "120*1780" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 120.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "L200*14" | object type "L200*14" | names: "TEGLKONSOLL-HALFEN" | descriptions: "L200*14" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Common, Tekla Quantity, BaseQuantities
          8 x IFCCOLUMN | type IFCCOLUMNTYPE "RHS200*100*16" | object type "RHS200*100*16" | names: "STÅLSØYLE" | descriptions: "RHS200*100*16" | material: "STEEL/S355J0" | property sets: Pset_ColumnCommon, Tekla Common, Tekla Quantity, BaseQuantities
          22 x IFCCOLUMN | type IFCCOLUMNTYPE "CFRHS200X100X12.5" | object type "CFRHS200X100X12.5" | names: "STÅLSØYLE" | descriptions: "CFRHS200X100X12.5" | material: "STEEL/S355J0" | property sets: Pset_ColumnCommon, Tekla Quantity, Tekla Common, BaseQuantities
          3 x IFCMEMBER | type IFCMEMBERTYPE "CFRHS80X6" | object type "CFRHS80X6" | names: "STÅLBJELKE" | descriptions: "CFRHS80X6" | material: "STEEL/S355J0" | property sets: Pset_MemberCommon, Tekla Quantity, Tekla Common, BaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "IPE300" | object type "IPE300" | names: "STÅLBJELKE" | descriptions: "IPE300" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Quantity, BaseQuantities, Tekla Common
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*250" | object type "3000*250" | names: "BETONGVEGG" | descriptions: "3000*250" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 250.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          4 x IFCWALL | type IFCWALLTYPE "3000*250" | object type "3000*250" | names: "BETONGVEGG" | descriptions: "3000*250" | material: "CONCRETE/B30" | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "2730*200" | object type "2730*200" | names: "BETONGVEGG" | descriptions: "2730*200" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 200.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "270*2170" | object type "270*2170" | FLOOR | names: "BALKONG" | descriptions: "270*2170" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "IPE240" | object type "IPE240" | names: "STÅLBJELKE" | descriptions: "IPE240" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Quantity, BaseQuantities, Tekla Common
          1 x IFCSLAB | type IFCSLABTYPE "270*20150" | object type "270*20150" | FLOOR | names: "BETONGDEKKE" | descriptions: "270*20150" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Quantity, Tekla Common, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "270*2100" | object type "270*2100" | FLOOR | names: "BALKONG" | descriptions: "270*2100" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
      IFCBUILDINGSTOREY "08" | elevation 35420.
        contains 93 elements
          2 x IFCWALL | type IFCWALLTYPE "3650*200" | object type "3650*200" | names: "BETONGVEGG" | descriptions: "3650*200" | material: "CONCRETE/B30" | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          2 x IFCSLAB | type IFCSLABTYPE "250*2120" | object type "250*2120" | FLOOR | names: "Heislokk" | descriptions: "250*2120" | material: layers "Floor: Insitu CONCRETE/B30" ("CONCRETE/B30" 250.) | property sets: Tekla Common, Tekla Quantity, Pset_SlabCommon, BaseQuantities
          1 x IFCPLATE | type IFCPLATETYPE "200*12401" | object type "200*12401" | names: "STÅLPLATETAK" | descriptions: "200*12401" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Pset_PlateCommon, Tekla Common, Tekla Quantity, BaseQuantities
          4 x IFCBEAM | type IFCBEAMTYPE "HSQ250*8-30*150-10*450" | object type "HSQ250*8-30*150-10*450" | names: "STÅLBJELKE" | descriptions: "HSQ250*8-30*150-10*450" | material: "STEEL/S355J0" | property sets: Tekla Common, Pset_BeamCommon, Tekla Quantity, BaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "CFRHS250X150X12.5" | object type "CFRHS250X150X12.5" | names: "STÅLBJELKE" | descriptions: "CFRHS250X150X12.5" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Common, Tekla Quantity, BaseQuantities
          4 x IFCBEAM | type IFCBEAMTYPE "IPE240" | object type "IPE240" | names: "STÅLBJELKE" | descriptions: "IPE240" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          26 x IFCBEAM | type IFCBEAMTYPE "L100*10" | object type "L100*10" | names: "Stålvinnkel" | descriptions: "L100*10" | material: "STEEL/S355J0" | property sets: Tekla Common, Pset_BeamCommon, Tekla Quantity, BaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "L200*14" | object type "L200*14" | names: "TEGLKONSOLL-HALFEN" | descriptions: "L200*14" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Common, Tekla Quantity, BaseQuantities
          5 x IFCCOLUMN | type IFCCOLUMNTYPE "RHS200*100*16" | object type "RHS200*100*16" | names: "STÅLSØYLE" | descriptions: "RHS200*100*16" | material: "STEEL/S355J0" | property sets: Pset_ColumnCommon, Tekla Common, Tekla Quantity, BaseQuantities
          24 x IFCCOLUMN | type IFCCOLUMNTYPE "CFRHS200X100X12.5" | object type "CFRHS200X100X12.5" | names: "STÅLSØYLE" | descriptions: "CFRHS200X100X12.5" | material: "STEEL/S355J0" | property sets: Pset_ColumnCommon, Tekla Quantity, Tekla Common, BaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "D20-400" | object type "D20-400" | names: "Deltabjelke" | descriptions: "D20-400" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Quantity, Tekla Common, BaseQuantities
          3 x IFCMEMBER | type IFCMEMBERTYPE "CFRHS80X6" | object type "CFRHS80X6" | names: "STÅLBJELKE" | descriptions: "CFRHS80X6" | material: "STEEL/S355J0" | property sets: Pset_MemberCommon, Tekla Quantity, Tekla Common, BaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "IPE300" | object type "IPE300" | names: "STÅLBJELKE" | descriptions: "IPE300" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Quantity, BaseQuantities, Tekla Common
          3 x IFCWALL | type IFCWALLTYPE "3000*250" | object type "3000*250" | names: "BETONGVEGG" | descriptions: "3000*250" | material: "CONCRETE/B30" | property sets: Pset_WallCommon, Tekla Quantity, Tekla Common, BaseQuantities
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*250" | object type "3000*250" | names: "BETONGVEGG" | descriptions: "3000*250" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 250.) | property sets: Pset_WallCommon, Tekla Quantity, Tekla Common, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*220" | object type "3000*220" | names: "BETONGVEGG" | descriptions: "3000*220" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 220.) | property sets: Pset_WallCommon, Tekla Quantity, Tekla Common, BaseQuantities
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*200" | object type "3000*200" | names: "BETONGVEGG" | descriptions: "3000*200" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 200.) | property sets: Pset_WallCommon, Tekla Quantity, Tekla Common, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "270*2170" | object type "270*2170" | FLOOR | names: "BALKONG" | descriptions: "270*2170" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          3 x IFCBEAM | type IFCBEAMTYPE "UPE270" | object type "UPE270" | names: "STÅLBJELKE" | descriptions: "UPE270" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "270*20150" | object type "270*20150" | FLOOR | names: "BETONGDEKKE" | descriptions: "270*20150" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Quantity, Tekla Common, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "270*2100" | object type "270*2100" | FLOOR | names: "BALKONG" | descriptions: "270*2100" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
      IFCBUILDINGSTOREY "09" | elevation 38420.
        contains 52 elements
          28 x IFCCOLUMN | type IFCCOLUMNTYPE "CFRHS200X100X12.5" | object type "CFRHS200X100X12.5" | names: "STÅLSØYLE" | descriptions: "CFRHS200X100X12.5" | material: "STEEL/S355J0" | property sets: Pset_ColumnCommon, Tekla Quantity, Tekla Common, BaseQuantities
          3 x IFCMEMBER | type IFCMEMBERTYPE "CFRHS80X6" | object type "CFRHS80X6" | names: "STÅLBJELKE" | descriptions: "CFRHS80X6" | material: "STEEL/S355J0" | property sets: Pset_MemberCommon, Tekla Quantity, Tekla Common, BaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "IPE300" | object type "IPE300" | names: "STÅLBJELKE" | descriptions: "IPE300" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Quantity, BaseQuantities, Tekla Common
          1 x IFCBEAM | type IFCBEAMTYPE "D20-400" | object type "D20-400" | names: "Deltabjelke" | descriptions: "D20-400" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Quantity, BaseQuantities, Tekla Common
          3 x IFCWALL | type IFCWALLTYPE "3000*250" | object type "3000*250" | names: "BETONGVEGG" | descriptions: "3000*250" | material: "CONCRETE/B30" | property sets: Pset_WallCommon, Tekla Quantity, BaseQuantities, Tekla Common
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*250" | object type "3000*250" | names: "BETONGVEGG" | descriptions: "3000*250" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 250.) | property sets: Pset_WallCommon, Tekla Quantity, BaseQuantities, Tekla Common
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*220" | object type "3000*220" | names: "BETONGVEGG" | descriptions: "3000*220" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 220.) | property sets: Pset_WallCommon, Tekla Quantity, BaseQuantities, Tekla Common
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*200" | object type "3000*200" | names: "BETONGVEGG" | descriptions: "3000*200" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 200.) | property sets: Pset_WallCommon, Tekla Quantity, BaseQuantities, Tekla Common
          1 x IFCSLAB | type IFCSLABTYPE "270*2170" | object type "270*2170" | FLOOR | names: "BALKONG" | descriptions: "270*2170" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          3 x IFCBEAM | type IFCBEAMTYPE "UPE270" | object type "UPE270" | names: "STÅLBJELKE" | descriptions: "UPE270" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "IPE240" | object type "IPE240" | names: "STÅLBJELKE" | descriptions: "IPE240" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Quantity, BaseQuantities, Tekla Common
          1 x IFCSLAB | type IFCSLABTYPE "270*20150" | object type "270*20150" | FLOOR | names: "BETONGDEKKE" | descriptions: "270*20150" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Quantity, BaseQuantities, Tekla Common
          1 x IFCSLAB | type IFCSLABTYPE "270*2100" | object type "270*2100" | FLOOR | names: "BALKONG" | descriptions: "270*2100" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
      IFCBUILDINGSTOREY "10" | elevation 41420.
        contains 52 elements
          28 x IFCCOLUMN | type IFCCOLUMNTYPE "CFRHS200X100X12.5" | object type "CFRHS200X100X12.5" | names: "STÅLSØYLE" | descriptions: "CFRHS200X100X12.5" | material: "STEEL/S355J0" | property sets: Pset_ColumnCommon, Tekla Quantity, Tekla Common, BaseQuantities
          3 x IFCMEMBER | type IFCMEMBERTYPE "CFRHS80X6" | object type "CFRHS80X6" | names: "STÅLBJELKE" | descriptions: "CFRHS80X6" | material: "STEEL/S355J0" | property sets: Pset_MemberCommon, Tekla Quantity, Tekla Common, BaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "IPE300" | object type "IPE300" | names: "STÅLBJELKE" | descriptions: "IPE300" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Quantity, Tekla Common, BaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "D20-400" | object type "D20-400" | names: "Deltabjelke" | descriptions: "D20-400" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Quantity, BaseQuantities, Tekla Common
          3 x IFCWALL | type IFCWALLTYPE "3000*250" | object type "3000*250" | names: "BETONGVEGG" | descriptions: "3000*250" | material: "CONCRETE/B30" | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*250" | object type "3000*250" | names: "BETONGVEGG" | descriptions: "3000*250" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 250.) | property sets: Pset_WallCommon, Tekla Quantity, BaseQuantities, Tekla Common
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*220" | object type "3000*220" | names: "BETONGVEGG" | descriptions: "3000*220" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 220.) | property sets: Pset_WallCommon, Tekla Quantity, Tekla Common, BaseQuantities
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*200" | object type "3000*200" | names: "BETONGVEGG" | descriptions: "3000*200" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 200.) | property sets: Pset_WallCommon, Tekla Quantity, BaseQuantities, Tekla Common
          1 x IFCSLAB | type IFCSLABTYPE "270*2170" | object type "270*2170" | FLOOR | names: "BALKONG" | descriptions: "270*2170" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          3 x IFCBEAM | type IFCBEAMTYPE "UPE270" | object type "UPE270" | names: "STÅLBJELKE" | descriptions: "UPE270" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "IPE240" | object type "IPE240" | names: "STÅLBJELKE" | descriptions: "IPE240" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Quantity, Tekla Common, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "270*20150" | object type "270*20150" | FLOOR | names: "BETONGDEKKE" | descriptions: "270*20150" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Quantity, Tekla Common, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "270*2100" | object type "270*2100" | FLOOR | names: "BALKONG" | descriptions: "270*2100" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
      IFCBUILDINGSTOREY "03" | elevation 20420.
        contains 117 elements
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*200" | object type "3000*200" | names: "BETONGVEGG" | descriptions: "3000*200" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 200.); layers "Wall: Insitu CONCRETE/B45" ("CONCRETE/B45" 200.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          5 x IFCWALL | type IFCWALLTYPE "3000*220" | object type "3000*220" | names: "BETONGVEGG" | descriptions: "3000*220" | material: "CONCRETE/B30" | property sets: Pset_WallCommon, Tekla Quantity, Tekla Common, BaseQuantities
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*220" | object type "3000*220" | names: "BETONGVEGG" | descriptions: "3000*220" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 220.); layers "Wall: Insitu CONCRETE/B45" ("CONCRETE/B45" 220.) | property sets: Tekla Common, Pset_WallCommon, Tekla Quantity, BaseQuantities
          5 x IFCWALL | type IFCWALLTYPE "3000*200" | object type "3000*200" | names: "BETONGVEGG" | descriptions: "3000*200" | material: "CONCRETE/B30"; "CONCRETE/B45" | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          2 x IFCSLAB | type IFCSLABTYPE "270*1987" | object type "270*1987" | FLOOR | names: "BALKONG" | descriptions: "270*1987" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Tekla Common, Tekla Quantity, Pset_SlabCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "250*2202" | object type "250*2202" | FLOOR | names: "BALKONG" | descriptions: "250*2202" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 250.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          4 x IFCBEAM | type IFCBEAMTYPE "D20-400" | object type "D20-400" | names: "Deltabjelke" | descriptions: "D20-400" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Quantity, Tekla Common, BaseQuantities
          5 x IFCSLAB | type IFCSLABTYPE "250*2160" | object type "250*2160" | FLOOR | names: "BALKONG" | descriptions: "250*2160" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 250.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          15 x IFCCOLUMN | type IFCCOLUMNTYPE "RHS200*100*12.5" | object type "RHS200*100*12.5" | names: "STÅLSØYLE" | descriptions: "RHS200*100*12.5" | material: "STEEL/S355J0" | property sets: Pset_ColumnCommon, Tekla Quantity, Tekla Common, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "250*12420" | object type "250*12420" | FLOOR | names: "Betongdekke" | descriptions: "250*12420" | material: layers "Floor: Insitu CONCRETE/B30" ("CONCRETE/B30" 250.) | property sets: Pset_SlabCommon, Tekla Quantity, Tekla Common, BaseQuantities
          8 x IFCCOLUMN | type IFCCOLUMNTYPE "CFRHS200X100X10" | object type "CFRHS200X100X10" | names: "STÅLSØYLE" | descriptions: "CFRHS200X100X10" | material: "STEEL/S355J0" | property sets: Pset_ColumnCommon, Tekla Common, Tekla Quantity, BaseQuantities
          5 x IFCBEAM | type IFCBEAMTYPE "UPE270" | object type "UPE270" | names: "STÅLBJELKE" | descriptions: "UPE270" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "D20-300" | object type "D20-300" | names: "STÅLBJELKE" | descriptions: "D20-300" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*250" | object type "3000*250" | names: "BETONGVEGG" | descriptions: "3000*250" | material: layers "Wall: Insitu CONCRETE/B45" ("CONCRETE/B45" 250.) | property sets: Pset_WallCommon, Tekla Quantity, Tekla Common, BaseQuantities
          4 x IFCWALL | type IFCWALLTYPE "3000*250" | object type "3000*250" | names: "BETONGVEGG" | descriptions: "3000*250" | material: "CONCRETE/B45" | property sets: Pset_WallCommon, Tekla Quantity, Tekla Common, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "120*2065" | object type "120*2065" | FLOOR | names: "Bad" | descriptions: "120*2065" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 120.) | property sets: Pset_SlabCommon, Tekla Quantity, Tekla Common, BaseQuantities
          2 x IFCSLAB | type IFCSLABTYPE "120*1817" | object type "120*1817" | FLOOR | names: "Bad" | descriptions: "120*1817" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 120.) | property sets: Pset_SlabCommon, Tekla Quantity, Tekla Common, BaseQuantities
          2 x IFCSLAB | type IFCSLABTYPE "120*1780" | object type "120*1780" | FLOOR | names: "Bad" | descriptions: "120*1780" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 120.) | property sets: Pset_SlabCommon, Tekla Quantity, Tekla Common, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "120*1700" | object type "120*1700" | FLOOR | names: "Bad" | descriptions: "120*1700" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 120.) | property sets: Pset_SlabCommon, Tekla Quantity, Tekla Common, BaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "L200*14" | object type "L200*14" | names: "TEGLKONSOLL-HALFEN" | descriptions: "L200*14" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "CFRHS200*100*12" | object type "CFRHS200*100*12" | names: "STÅLSØYLE" | descriptions: "CFRHS200*100*12" | material: "STEEL/S355J0" | property sets: Pset_ColumnCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "370*150" | object type "370*150" | names: "Teglkon(eks.Ytong)" | descriptions: "370*150" | material: "CONCRETE/B35" | property sets: Pset_BeamCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*400" | object type "3000*400" | names: "BETONGVEGG" | descriptions: "3000*400" | material: layers "Wall: Insitu CONCRETE/B55" ("CONCRETE/B55" 400.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          15 x IFCCOLUMN | type IFCCOLUMNTYPE "RHS200*100*16" | object type "RHS200*100*16" | names: "STÅLSØYLE" | descriptions: "RHS200*100*16" | material: "STEEL/S355J0" | property sets: Pset_ColumnCommon, Tekla Quantity, Tekla Common, BaseQuantities
          13 x IFCCOLUMN | type IFCCOLUMNTYPE "CFRHS200X100X12.5" | object type "CFRHS200X100X12.5" | names: "STÅLSØYLE" | descriptions: "CFRHS200X100X12.5" | material: "STEEL/S355J0" | property sets: Pset_ColumnCommon, Tekla Quantity, Tekla Common, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "220*2350" | object type "220*2350" | FLOOR | names: "Forsenket dekke" | descriptions: "220*2350" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 220.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCMEMBER | type IFCMEMBERTYPE "CFRHS80X6" | object type "CFRHS80X6" | names: "STÅLBJELKE" | descriptions: "CFRHS80X6" | material: "STEEL/S355J0" | property sets: Pset_MemberCommon, Tekla Quantity, Tekla Common, BaseQuantities
          3 x IFCBEAM | type IFCBEAMTYPE "IPE240" | object type "IPE240" | names: "STÅLBJELKE" | descriptions: "IPE240" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Quantity, Tekla Common, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "270*20150" | object type "270*20150" | FLOOR | names: "BETONGDEKKE" | descriptions: "270*20150" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Quantity, Tekla Common, BaseQuantities
          2 x IFCSLAB | type IFCSLABTYPE "270*2170" | object type "270*2170" | FLOOR | names: "BALKONG" | descriptions: "270*2170" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Tekla Quantity, Pset_SlabCommon, Tekla Common, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "270*2280" | object type "270*2280" | FLOOR | names: "BALKONG" | descriptions: "270*2280" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Quantity, BaseQuantities, Tekla Common
      IFCBUILDINGSTOREY "04" | elevation 23420.
        contains 113 elements
          7 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*200" | object type "3000*200" | names: "BETONGVEGG" | descriptions: "3000*200" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 200.); layers "Wall: Insitu CONCRETE/B45" ("CONCRETE/B45" 200.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          6 x IFCWALL | type IFCWALLTYPE "3000*220" | object type "3000*220" | names: "BETONGVEGG" | descriptions: "3000*220" | material: "CONCRETE/B30" | property sets: Pset_WallCommon, Tekla Quantity, Tekla Common, BaseQuantities
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*220" | object type "3000*220" | names: "BETONGVEGG" | descriptions: "3000*220" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 220.); layers "Wall: Insitu CONCRETE/B45" ("CONCRETE/B45" 220.) | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          4 x IFCWALL | type IFCWALLTYPE "3000*200" | object type "3000*200" | names: "BETONGVEGG" | descriptions: "3000*200" | material: "CONCRETE/B30" | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "250*2202" | object type "250*2202" | FLOOR | names: "BALKONG" | descriptions: "250*2202" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 250.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          4 x IFCBEAM | type IFCBEAMTYPE "D20-400" | object type "D20-400" | names: "Deltabjelke" | descriptions: "D20-400" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Quantity, Tekla Common, BaseQuantities
          5 x IFCSLAB | type IFCSLABTYPE "250*2160" | object type "250*2160" | FLOOR | names: "BALKONG" | descriptions: "250*2160" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 250.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          21 x IFCCOLUMN | type IFCCOLUMNTYPE "CFRHS200X100X12.5" | object type "CFRHS200X100X12.5" | names: "STÅLSØYLE" | descriptions: "CFRHS200X100X12.5" | material: "STEEL/S355J0" | property sets: Pset_ColumnCommon, Tekla Quantity, Tekla Common, BaseQuantities
          8 x IFCCOLUMN | type IFCCOLUMNTYPE "CFRHS200X100X8" | object type "CFRHS200X100X8" | names: "STÅLSØYLE" | descriptions: "CFRHS200X100X8" | material: "STEEL/S355J0" | property sets: Pset_ColumnCommon, Tekla Quantity, Tekla Common, BaseQuantities
          5 x IFCBEAM | type IFCBEAMTYPE "UPE270" | object type "UPE270" | names: "STÅLBJELKE" | descriptions: "UPE270" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "D20-300" | object type "D20-300" | names: "STÅLBJELKE" | descriptions: "D20-300" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          2 x IFCSLAB | type IFCSLABTYPE "270*1987" | object type "270*1987" | FLOOR | names: "BALKONG" | descriptions: "270*1987" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Tekla Common, Tekla Quantity, Pset_SlabCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "250*12420" | object type "250*12420" | FLOOR | names: "Betongdekke" | descriptions: "250*12420" | material: layers "Floor: Insitu CONCRETE/B30" ("CONCRETE/B30" 250.) | property sets: Pset_SlabCommon, Tekla Quantity, BaseQuantities, Tekla Common
          1 x IFCSLAB | type IFCSLABTYPE "120*2065" | object type "120*2065" | FLOOR | names: "Bad" | descriptions: "120*2065" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 120.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCSLAB | type IFCSLABTYPE "120*1817" | object type "120*1817" | FLOOR | names: "Bad" | descriptions: "120*1817" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 120.) | property sets: Pset_SlabCommon, Tekla Quantity, Tekla Common, BaseQuantities
          2 x IFCSLAB | type IFCSLABTYPE "120*1780" | object type "120*1780" | FLOOR | names: "Bad" | descriptions: "120*1780" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 120.) | property sets: Pset_SlabCommon, Tekla Quantity, Tekla Common, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "120*1700" | object type "120*1700" | FLOOR | names: "Bad" | descriptions: "120*1700" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 120.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCMEMBER | type IFCMEMBERTYPE "CFRHS80X6" | object type "CFRHS80X6" | names: "STÅLBJELKE" | descriptions: "CFRHS80X6" | material: "STEEL/S355J0" | property sets: Pset_MemberCommon, Tekla Quantity, Tekla Common, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "270*2101" | object type "270*2101" | FLOOR | names: "BALKONG" | descriptions: "270*2101" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "IPE300" | object type "IPE300" | names: "STÅLBJELKE" | descriptions: "IPE300" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Quantity, Tekla Common, BaseQuantities
          3 x IFCBEAM | type IFCBEAMTYPE "IPE240" | object type "IPE240" | names: "STÅLBJELKE" | descriptions: "IPE240" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Quantity, Tekla Common, BaseQuantities
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*250" | object type "3000*250" | names: "BETONGVEGG" | descriptions: "3000*250" | material: layers "Wall: Insitu CONCRETE/B45" ("CONCRETE/B45" 250.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          4 x IFCWALL | type IFCWALLTYPE "3000*250" | object type "3000*250" | names: "BETONGVEGG" | descriptions: "3000*250" | material: "CONCRETE/B45" | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*300" | object type "3000*300" | names: "BETONGVEGG" | descriptions: "3000*300" | material: layers "Wall: Insitu CONCRETE/B55" ("CONCRETE/B55" 300.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "270*2170" | object type "270*2170" | FLOOR | names: "BALKONG" | descriptions: "270*2170" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          6 x IFCCOLUMN | type IFCCOLUMNTYPE "RHS200*100*12.5" | object type "RHS200*100*12.5" | names: "STÅLSØYLE" | descriptions: "RHS200*100*12.5" | material: "STEEL/S355J0" | property sets: Pset_ColumnCommon, Tekla Common, Tekla Quantity, BaseQuantities
          14 x IFCCOLUMN | type IFCCOLUMNTYPE "RHS200*100*16" | object type "RHS200*100*16" | names: "STÅLSØYLE" | descriptions: "RHS200*100*16" | material: "STEEL/S355J0" | property sets: Pset_ColumnCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "270*20150" | object type "270*20150" | FLOOR | names: "BETONGDEKKE" | descriptions: "270*20150" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Quantity, Tekla Common, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "270*2280" | object type "270*2280" | FLOOR | names: "BALKONG" | descriptions: "270*2280" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
      IFCBUILDINGSTOREY "05" | elevation 26420.
        contains 98 elements
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3400*200" | object type "3400*200" | names: "BETONGVEGG" | descriptions: "3400*200" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 200.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          6 x IFCWALL | type IFCWALLTYPE "3400*220" | object type "3400*220" | names: "BETONGVEGG" | descriptions: "3400*220" | material: "CONCRETE/B30" | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3400*220" | object type "3400*220" | names: "BETONGVEGG" | descriptions: "3400*220" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 220.) | property sets: Tekla Common, Pset_WallCommon, Tekla Quantity, BaseQuantities
          4 x IFCWALL | type IFCWALLTYPE "3400*200" | object type "3400*200" | names: "BETONGVEGG" | descriptions: "3400*200" | material: "CONCRETE/B30" | property sets: Tekla Common, Pset_WallCommon, Tekla Quantity, BaseQuantities
          30 x IFCCOLUMN | type IFCCOLUMNTYPE "CFRHS200X100X12.5" | object type "CFRHS200X100X12.5" | names: "STÅLSØYLE" | descriptions: "CFRHS200X100X12.5" | material: "STEEL/S355J0" | property sets: Pset_ColumnCommon, Tekla Common, Tekla Quantity, BaseQuantities
          8 x IFCCOLUMN | type IFCCOLUMNTYPE "CFRHS200X100X6" | object type "CFRHS200X100X6" | names: "STÅLSØYLE" | descriptions: "CFRHS200X100X6" | material: "STEEL/S355J0" | property sets: Pset_ColumnCommon, Tekla Common, Tekla Quantity, BaseQuantities
          4 x IFCBEAM | type IFCBEAMTYPE "UPE270" | object type "UPE270" | names: "STÅLBJELKE" | descriptions: "UPE270" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "250*5490" | object type "250*5490" | FLOOR | names: "Betongdekke" | descriptions: "250*5490" | material: layers "Floor: Insitu CONCRETE/B30" ("CONCRETE/B30" 250.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "250*5600" | object type "250*5600" | FLOOR | names: "Betongdekke" | descriptions: "250*5600" | material: layers "Floor: Insitu CONCRETE/B30" ("CONCRETE/B30" 250.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "L200*14" | object type "L200*14" | names: "TEGLKONSOLL-HALFEN" | descriptions: "L200*14" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCPLATE | type IFCPLATETYPE "198*1500" | object type "198*1500" | names: "TØMMERTAK" | descriptions: "198*1500" | material: "TIMBER/C24" | property sets: Pset_PlateCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "250*1400" | object type "250*1400" | FLOOR | names: "BALKONG" | descriptions: "250*1400" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 250.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          11 x IFCCOLUMN | type IFCCOLUMNTYPE "RHS200*100*16" | object type "RHS200*100*16" | names: "STÅLSØYLE" | descriptions: "RHS200*100*16" | material: "STEEL/S355J0" | property sets: Pset_ColumnCommon, Tekla Quantity, Tekla Common, BaseQuantities
          2 x IFCMEMBER | type IFCMEMBERTYPE "CFRHS80X6" | object type "CFRHS80X6" | names: "STÅLBJELKE" | descriptions: "CFRHS80X6" | material: "STEEL/S355J0" | property sets: Pset_MemberCommon, Tekla Quantity, Tekla Common, BaseQuantities
          3 x IFCBEAM | type IFCBEAMTYPE "IPE240" | object type "IPE240" | names: "STÅLBJELKE" | descriptions: "IPE240" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Quantity, Tekla Common, BaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "IPE300" | object type "IPE300" | names: "STÅLBJELKE" | descriptions: "IPE300" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Quantity, BaseQuantities, Tekla Common
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*250" | object type "3000*250" | names: "BETONGVEGG" | descriptions: "3000*250" | material: layers "Wall: Insitu CONCRETE/B45" ("CONCRETE/B45" 250.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          4 x IFCWALL | type IFCWALLTYPE "3000*250" | object type "3000*250" | names: "BETONGVEGG" | descriptions: "3000*250" | material: "CONCRETE/B45" | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*200" | object type "3000*200" | names: "BETONGVEGG" | descriptions: "3000*200" | material: layers "Wall: Insitu CONCRETE/B45" ("CONCRETE/B45" 200.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*220" | object type "3000*220" | names: "BETONGVEGG" | descriptions: "3000*220" | material: layers "Wall: Insitu CONCRETE/B45" ("CONCRETE/B45" 220.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "270*2170" | object type "270*2170" | FLOOR | names: "BALKONG" | descriptions: "270*2170" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "270*20150" | object type "270*20150" | FLOOR | names: "BETONGDEKKE" | descriptions: "270*20150" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Quantity, Tekla Common, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "270*2100" | object type "270*2100" | FLOOR | names: "BALKONG" | descriptions: "270*2100" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "270*2280" | object type "270*2280" | FLOOR | names: "BALKONG" | descriptions: "270*2280" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
      IFCBUILDINGSTOREY "14" | elevation 53820.
        contains 120 elements
          41 x IFCCOLUMN | type IFCCOLUMNTYPE "CFRHS200X100X12.5" | object type "CFRHS200X100X12.5" | names: "STÅLSØYLE" | descriptions: "CFRHS200X100X12.5" | material: "STEEL/S355J0" | property sets: Pset_ColumnCommon, Tekla Quantity, Tekla Common, BaseQuantities
          9 x IFCMEMBER | type IFCMEMBERTYPE "CFRHS80X6" | object type "CFRHS80X6" | names: "STÅLBJELKE" | descriptions: "CFRHS80X6" | material: "STEEL/S355J0" | property sets: Pset_MemberCommon, Tekla Quantity, Tekla Common, BaseQuantities
          3 x IFCBEAM | type IFCBEAMTYPE "IPE300" | object type "IPE300" | names: "STÅLBJELKE" | descriptions: "IPE300" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Quantity, BaseQuantities, Tekla Common
          1 x IFCPLATE | type IFCPLATETYPE "200*13020" | object type "200*13020" | names: "STÅLPLATETAK" | descriptions: "200*13020" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Tekla Common, Tekla Quantity, Pset_PlateCommon, BaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "CFRHS80X6" | object type "CFRHS80X6" | names: "STÅLBJELKE" | descriptions: "CFRHS80X6" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "D20-400" | object type "D20-400" | names: "Deltabjelke" | descriptions: "D20-400" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Quantity, BaseQuantities, Tekla Common
          1 x IFCBEAM | type IFCBEAMTYPE "DR26-260" | object type "DR26-260" | names: "Deltabjelke" | descriptions: "DR26-260" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Common, Tekla Quantity, BaseQuantities
          8 x IFCWALL | type IFCWALLTYPE "3000*250" | object type "3000*250" | names: "BETONGVEGG" | descriptions: "3000*250" | material: "CONCRETE/B30" | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          11 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*250" | object type "3000*250" | names: "BETONGVEGG" | descriptions: "3000*250" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 250.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          9 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*200" | object type "3000*200" | names: "BETONGVEGG" | descriptions: "3000*200" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 200.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*220" | object type "3000*220" | names: "BETONGVEGG" | descriptions: "3000*220" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 220.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3200*250" | object type "3200*250" | names: "BETONGVEGG" | descriptions: "3200*250" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 250.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3200*220" | object type "3200*220" | names: "BETONGVEGG" | descriptions: "3200*220" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 220.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "4450*200" | object type "4450*200" | names: "BETONGVEGG" | descriptions: "4450*200" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 200.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "4450*250" | object type "4450*250" | names: "BETONGVEGG" | descriptions: "4450*250" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 250.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          3 x IFCSLAB | type IFCSLABTYPE "270*2170" | object type "270*2170" | FLOOR | names: "BALKONG" | descriptions: "270*2170" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          8 x IFCBEAM | type IFCBEAMTYPE "UPE270" | object type "UPE270" | names: "STÅLBJELKE" | descriptions: "UPE270" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Common, Tekla Quantity, BaseQuantities
          6 x IFCBEAM | type IFCBEAMTYPE "IPE240" | object type "IPE240" | names: "STÅLBJELKE" | descriptions: "IPE240" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Quantity, BaseQuantities, Tekla Common
          2 x IFCSLAB | type IFCSLABTYPE "270*20150" | object type "270*20150" | FLOOR | names: "BETONGDEKKE" | descriptions: "270*20150" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Quantity, Tekla Common, BaseQuantities
          3 x IFCSLAB | type IFCSLABTYPE "270*2100" | object type "270*2100" | FLOOR | names: "BALKONG" | descriptions: "270*2100" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "270*17750" | object type "270*17750" | FLOOR | names: "BETONGDEKKE" | descriptions: "270*17750" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
      IFCBUILDINGSTOREY "13" | elevation 50420.
        contains 42 elements
          18 x IFCCOLUMN | type IFCCOLUMNTYPE "CFRHS200X100X12.5" | object type "CFRHS200X100X12.5" | names: "STÅLSØYLE" | descriptions: "CFRHS200X100X12.5" | material: "STEEL/S355J0" | property sets: Pset_ColumnCommon, Tekla Quantity, Tekla Common, BaseQuantities
          3 x IFCMEMBER | type IFCMEMBERTYPE "CFRHS80X6" | object type "CFRHS80X6" | names: "STÅLBJELKE" | descriptions: "CFRHS80X6" | material: "STEEL/S355J0" | property sets: Pset_MemberCommon, Tekla Quantity, BaseQuantities, Tekla Common
          1 x IFCBEAM | type IFCBEAMTYPE "IPE300" | object type "IPE300" | names: "STÅLBJELKE" | descriptions: "IPE300" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Quantity, BaseQuantities, Tekla Common
          1 x IFCBEAM | type IFCBEAMTYPE "D20-400" | object type "D20-400" | names: "Deltabjelke" | descriptions: "D20-400" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Quantity, BaseQuantities, Tekla Common
          3 x IFCWALL | type IFCWALLTYPE "3000*250" | object type "3000*250" | names: "BETONGVEGG" | descriptions: "3000*250" | material: "CONCRETE/B30" | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*250" | object type "3000*250" | names: "BETONGVEGG" | descriptions: "3000*250" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 250.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*200" | object type "3000*200" | names: "BETONGVEGG" | descriptions: "3000*200" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 200.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "270*2170" | object type "270*2170" | FLOOR | names: "BALKONG" | descriptions: "270*2170" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          3 x IFCBEAM | type IFCBEAMTYPE "UPE270" | object type "UPE270" | names: "STÅLBJELKE" | descriptions: "UPE270" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "IPE240" | object type "IPE240" | names: "STÅLBJELKE" | descriptions: "IPE240" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Quantity, BaseQuantities, Tekla Common
          1 x IFCSLAB | type IFCSLABTYPE "270*20150" | object type "270*20150" | FLOOR | names: "BETONGDEKKE" | descriptions: "270*20150" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Quantity, BaseQuantities, Tekla Common
          1 x IFCSLAB | type IFCSLABTYPE "270*2100" | object type "270*2100" | FLOOR | names: "BALKONG" | descriptions: "270*2100" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*220" | object type "3000*220" | names: "BETONGVEGG" | descriptions: "3000*220" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 220.) | property sets: Pset_WallCommon, Tekla Quantity, Tekla Common, BaseQuantities
      IFCBUILDINGSTOREY "12" | elevation 47420.
        contains 47 elements
          23 x IFCCOLUMN | type IFCCOLUMNTYPE "CFRHS200X100X12.5" | object type "CFRHS200X100X12.5" | names: "STÅLSØYLE" | descriptions: "CFRHS200X100X12.5" | material: "STEEL/S355J0" | property sets: Pset_ColumnCommon, Tekla Common, Tekla Quantity, BaseQuantities
          3 x IFCMEMBER | type IFCMEMBERTYPE "CFRHS80X6" | object type "CFRHS80X6" | names: "STÅLBJELKE" | descriptions: "CFRHS80X6" | material: "STEEL/S355J0" | property sets: Pset_MemberCommon, Tekla Quantity, Tekla Common, BaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "IPE300" | object type "IPE300" | names: "STÅLBJELKE" | descriptions: "IPE300" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Quantity, BaseQuantities, Tekla Common
          1 x IFCBEAM | type IFCBEAMTYPE "D20-400" | object type "D20-400" | names: "Deltabjelke" | descriptions: "D20-400" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Quantity, BaseQuantities, Tekla Common
          3 x IFCWALL | type IFCWALLTYPE "3000*250" | object type "3000*250" | names: "BETONGVEGG" | descriptions: "3000*250" | material: "CONCRETE/B30" | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*250" | object type "3000*250" | names: "BETONGVEGG" | descriptions: "3000*250" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 250.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*200" | object type "3000*200" | names: "BETONGVEGG" | descriptions: "3000*200" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 200.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "270*2170" | object type "270*2170" | FLOOR | names: "BALKONG" | descriptions: "270*2170" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          3 x IFCBEAM | type IFCBEAMTYPE "UPE270" | object type "UPE270" | names: "STÅLBJELKE" | descriptions: "UPE270" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "IPE240" | object type "IPE240" | names: "STÅLBJELKE" | descriptions: "IPE240" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Quantity, BaseQuantities, Tekla Common
          1 x IFCSLAB | type IFCSLABTYPE "270*20150" | object type "270*20150" | FLOOR | names: "BETONGDEKKE" | descriptions: "270*20150" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Quantity, BaseQuantities, Tekla Common
          1 x IFCSLAB | type IFCSLABTYPE "270*2100" | object type "270*2100" | FLOOR | names: "BALKONG" | descriptions: "270*2100" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*220" | object type "3000*220" | names: "BETONGVEGG" | descriptions: "3000*220" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 220.) | property sets: Pset_WallCommon, Tekla Quantity, Tekla Common, BaseQuantities
      IFCBUILDINGSTOREY "11" | elevation 44420.
        contains 50 elements
          26 x IFCCOLUMN | type IFCCOLUMNTYPE "CFRHS200X100X12.5" | object type "CFRHS200X100X12.5" | names: "STÅLSØYLE" | descriptions: "CFRHS200X100X12.5" | material: "STEEL/S355J0" | property sets: Pset_ColumnCommon, Tekla Quantity, Tekla Common, BaseQuantities
          3 x IFCMEMBER | type IFCMEMBERTYPE "CFRHS80X6" | object type "CFRHS80X6" | names: "STÅLBJELKE" | descriptions: "CFRHS80X6" | material: "STEEL/S355J0" | property sets: Pset_MemberCommon, Tekla Quantity, BaseQuantities, Tekla Common
          1 x IFCBEAM | type IFCBEAMTYPE "IPE300" | object type "IPE300" | names: "STÅLBJELKE" | descriptions: "IPE300" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Quantity, BaseQuantities, Tekla Common
          1 x IFCBEAM | type IFCBEAMTYPE "D20-400" | object type "D20-400" | names: "Deltabjelke" | descriptions: "D20-400" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Quantity, BaseQuantities, Tekla Common
          3 x IFCWALL | type IFCWALLTYPE "3000*250" | object type "3000*250" | names: "BETONGVEGG" | descriptions: "3000*250" | material: "CONCRETE/B30" | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*250" | object type "3000*250" | names: "BETONGVEGG" | descriptions: "3000*250" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 250.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*200" | object type "3000*200" | names: "BETONGVEGG" | descriptions: "3000*200" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 200.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "270*2170" | object type "270*2170" | FLOOR | names: "BALKONG" | descriptions: "270*2170" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          3 x IFCBEAM | type IFCBEAMTYPE "UPE270" | object type "UPE270" | names: "STÅLBJELKE" | descriptions: "UPE270" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "IPE240" | object type "IPE240" | names: "STÅLBJELKE" | descriptions: "IPE240" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Quantity, BaseQuantities, Tekla Common
          1 x IFCSLAB | type IFCSLABTYPE "270*20150" | object type "270*20150" | FLOOR | names: "BETONGDEKKE" | descriptions: "270*20150" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Quantity, BaseQuantities, Tekla Common
          1 x IFCSLAB | type IFCSLABTYPE "270*2100" | object type "270*2100" | FLOOR | names: "BALKONG" | descriptions: "270*2100" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*220" | object type "3000*220" | names: "BETONGVEGG" | descriptions: "3000*220" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 220.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
      IFCBUILDINGSTOREY "U2" | elevation 8100.
        contains 629 elements
          2 x IFCCOVERING | object type "V1-1" | names: "V1-1" | material: "Undefined/Undefined"
          1 x IFCWALL | type IFCWALLTYPE "3070*250" | object type "3070*250" | names: "BETONGVEGG" | descriptions: "3070*250" | material: "CONCRETE/B30" | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          5 x IFCCOVERING | object type "V12" | names: "V12" | material: "Undefined/Undefined"
          2 x IFCWALL | type IFCWALLTYPE "3000*220" | object type "3000*220" | names: "BETONGVEGG" | descriptions: "3000*220" | material: "CONCRETE/B30" | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          2 x IFCWALL | type IFCWALLTYPE "3120*220" | object type "3120*220" | names: "BETONGVEGG" | descriptions: "3120*220" | material: "CONCRETE/B30" | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "LB500*520-650*200" | object type "LB500*520-650*200" | names: "BETONGBJELKE" | descriptions: "LB500*520-650*200" | material: "CONCRETE/B45-SKB" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          1 x IFCCOVERING | object type "V3-1" | names: "V3-1" | material: "Undefined/Undefined"
          1 x IFCWALL | type IFCWALLTYPE "2820*250" | object type "2820*250" | names: "INNERVEGG" | descriptions: "2820*250" | material: "CONCRETE/B30" | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          146 x IFCBEAM | type IFCBEAMTYPE "HD320" | object type "HD320" | names: "HULLDEKKE" | descriptions: "HD320" | material: "CONCRETE/B45" | property sets: Tekla Common, Pset_BeamCommon, Tekla Quantity, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*200" | object type "3000*200" | names: "BETONGVEGG" | descriptions: "3000*200" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 200.) | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          11 x IFCCOLUMN | type IFCCOLUMNTYPE "900*400" | object type "900*400" | names: "BETONGSØYLE" | descriptions: "900*400" | material: "CONCRETE/B55-SKB"; "CONCRETE/B55" | property sets: Tekla Common, Tekla Quantity, Pset_ColumnCommon, BaseQuantities
          5 x IFCCOLUMN | type IFCCOLUMNTYPE "D5" | object type "D5" | names: "Koordpunkt" | descriptions: "D5" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity, Pset_ColumnCommon, BaseQuantities
          5 x IFCCOLUMN | type IFCCOLUMNTYPE "600*350" | object type "600*350" | names: "BETONGSØYLE" | descriptions: "600*350" | material: "CONCRETE/B55-SKB"; "CONCRETE/B45-SKB" | property sets: Tekla Common, Tekla Quantity, Pset_ColumnCommon, BaseQuantities
          4 x IFCCOVERING | object type "P1" | names: "P1" | material: "Undefined/Undefined"
          6 x IFCCOLUMN | type IFCCOLUMNTYPE "400*400" | object type "400*400" | names: "Pilaster" | descriptions: "400*400" | material: "CONCRETE/B45" | property sets: Pset_ColumnCommon, Tekla Quantity, Tekla Common, BaseQuantities
          1 x IFCWALL | type IFCWALLTYPE "3000*200" | object type "3000*200" | names: "BETONGVEGG" | descriptions: "3000*200" | material: "CONCRETE/B30" | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          1 x IFCCOVERING | object type "P2" | names: "P2" | material: "Undefined/Undefined"
          3 x IFCCOLUMN | type IFCCOLUMNTYPE "600*600" | object type "600*600" | names: "Pilaster", "BETONGSØYLE" | descriptions: "600*600" | material: "CONCRETE/B45"; "CONCRETE/B55-SKB"; "CONCRETE/B35" | property sets: Pset_ColumnCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "265*2159" | object type "265*2159" | FLOOR | names: "Repos" | descriptions: "265*2159" | material: layers "Floor: Insitu CONCRETE/B30-SKB" ("CONCRETE/B30-SKB" 265.) | property sets: Tekla Common, Tekla Quantity, Pset_SlabCommon, BaseQuantities
          5 x IFCBEAM | type IFCBEAMTYPE "DLB600*520-900*200" | object type "DLB600*520-900*200" | names: "BETONGBJELKE" | descriptions: "DLB600*520-900*200" | material: "CONCRETE/B45-SKB" | property sets: Tekla Common, Pset_BeamCommon, Tekla Quantity, BaseQuantities
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3070*250" | object type "3070*250" | names: "BETONGVEGG" | descriptions: "3070*250" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 250.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "5500*50" | object type "5500*50" | names: "X-Fjellskjæring" | descriptions: "5500*50" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 50.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "600*400" | object type "600*400" | names: "BETONGSØYLE" | descriptions: "600*400" | material: "CONCRETE/B55-SKB" | property sets: Tekla Common, Tekla Quantity, Pset_ColumnCommon, BaseQuantities
          7 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "250*200" | object type "250*200" | names: "Konsoll" | descriptions: "250*200" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 200.) | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          57 x IFCBEAM | type IFCBEAMTYPE "50*10" | object type "50*10" | names: "TPA-FZ_2,5TONN", "TPA-FZ_7,5TONN", "TPA-FZ_5,0TONN" (+25 more) | descriptions: "50*10" | material: "STEEL/S355J0" | property sets: Tekla Quantity, Pset_BeamCommon, Tekla Common, BaseQuantities
          41 x IFCBEAM | type IFCBEAMTYPE "D50" | object type "D50" | names: "KORR.RØR_Ø50" | descriptions: "D50" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "5000*300" | object type "5000*300" | names: "BETONGVEGG" | descriptions: "5000*300" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 300.) | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3070*300" | object type "3070*300" | names: "BETONGVEGG" | descriptions: "3070*300" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 300.) | property sets: Tekla Common, Pset_WallCommon, Tekla Quantity, BaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "15*170" | object type "15*170" | names: "STP7" | descriptions: "15*170" | material: "STEEL/S355J2G3" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          27 x IFCCOLUMN | type IFCCOLUMNTYPE "D20" | object type "D20" | names: "Kamstål ø20", "Flattstål", "STÅLBJELKE" | descriptions: "D20" | material: "REBAR/B500C"; "STEEL/S355J0" | property sets: Tekla Quantity, Pset_ColumnCommon, Tekla Common, BaseQuantities
          5 x IFCBEAM | type IFCBEAMTYPE "D75" | object type "D75" | names: "KORR.RØR_Ø75" | descriptions: "D75" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Tekla Quantity, Tekla Common, Pset_BeamCommon, BaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "25*380" | object type "25*380" | names: "STP13" | descriptions: "25*380" | material: "STEEL/S355J2G3" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          60 x IFCBEAM | type IFCBEAMTYPE "D20" | object type "D20" | names: "Kamstål ø20", "Flattstål", "Bunnfyllingslist" | descriptions: "D20" | material: "REBAR/B500C"; "STEEL/S355J0"; "MISCELLANEOUS/NEOPREN" | property sets: Tekla Quantity, Tekla Common, Pset_BeamCommon, BaseQuantities
          3 x IFCBEAM | type IFCBEAMTYPE "25*330" | object type "25*330" | names: "STP14" | descriptions: "25*330" | material: "STEEL/S355J2G3" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "25*580" | object type "25*580" | names: "STP15" | descriptions: "25*580" | material: "STEEL/S355J2G3" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          12 x IFCBEAM | type IFCBEAMTYPE "L150*12" | object type "L150*12" | names: "Stålvinkel" | descriptions: "L150*12" | material: "STEEL/S355J2H" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "1100*1323" | object type "1100*1323" | FLOOR | names: "TRAPP" | descriptions: "1100*1323" | material: layers "Floor: Insitu CONCRETE/B30-SKB" ("CONCRETE/B30-SKB" 1100.) | property sets: Tekla Common, Tekla Quantity, Pset_SlabCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "1110*375" | object type "1110*375" | FLOOR | names: "TRAPP" | descriptions: "1110*375" | material: layers "Floor: Insitu CONCRETE/B30-SKB" ("CONCRETE/B30-SKB" 1110.) | property sets: Tekla Common, Tekla Quantity, Pset_SlabCommon, BaseQuantities
          3 x IFCBEAM | type IFCBEAMTYPE "D100" | object type "D100" | names: "KORR.RØR Ø100" | descriptions: "D100" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Tekla Quantity, Pset_BeamCommon, BaseQuantities, Tekla Common
          2 x IFCBEAM | type IFCBEAMTYPE "8*100" | object type "8*100" | names: "Flattstål" | descriptions: "8*100" | material: "STEEL/S355J0" | property sets: Tekla Quantity, Pset_BeamCommon, Tekla Common, BaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "D16" | object type "D16" | names: "Flattstål" | descriptions: "D16" | material: "STEEL/S355J0" | property sets: Tekla Quantity, Pset_BeamCommon, Tekla Common, BaseQuantities
          15 x IFCCOLUMN | type IFCCOLUMNTYPE "D24" | object type "D24" | names: "Gjengestag M24" | descriptions: "D24" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity, Pset_ColumnCommon, BaseQuantities
          13 x IFCCOLUMN | type IFCCOLUMNTYPE "80*80" | object type "80*80" | names: "Skive 80x80x12" | descriptions: "80*80" | material: "STEEL/S355J0" | property sets: Tekla Quantity, Pset_ColumnCommon, Tekla Common, BaseQuantities
          15 x IFCCOLUMN | type IFCCOLUMNTYPE "HALFEN_NUT-M24" | object type "HALFEN_NUT-M24" | names: "Mutter M24" | descriptions: "HALFEN_NUT-M24" | material: "STEEL/S355J0" | property sets: Tekla Quantity, Pset_ColumnCommon, Tekla Common, BaseQuantities
          6 x IFCCOLUMN | type IFCCOLUMNTYPE "860*360" | object type "860*360" | names: "360x860x10 m/hull" | descriptions: "860*360" | material: "STEEL/S355J0" | property sets: Tekla Quantity, Pset_ColumnCommon, Tekla Common, BaseQuantities
          2 x IFCCOLUMN | type IFCCOLUMNTYPE "80*70" | object type "80*70" | names: "Skive 70x80x12" | descriptions: "80*70" | material: "STEEL/S355J0" | property sets: Tekla Quantity, Pset_ColumnCommon, Tekla Common, BaseQuantities
          1 x IFCPLATE | type IFCPLATETYPE "PL20*235" | object type "PL20*235" | names: "PLATE" | descriptions: "PL20*235" | material: "STEEL/S235JR" | property sets: Tekla Quantity, Pset_PlateCommon, BaseQuantities, Tekla Common
          1 x IFCCOVERING | object type "V1-3" | names: "V1-3" | material: "Undefined/Undefined"
          1 x IFCSLAB | type IFCSLABTYPE "1100*1219" | object type "1100*1219" | FLOOR | names: "TRAPP" | descriptions: "1100*1219" | material: layers "Floor: Insitu CONCRETE/B30-SKB" ("CONCRETE/B30-SKB" 1100.) | property sets: Tekla Common, Tekla Quantity, Pset_SlabCommon, BaseQuantities
          12 x IFCBEAM | type IFCBEAMTYPE "RHS120*80*5" | object type "RHS120*80*5" | names: "TSS102" | descriptions: "RHS120*80*5" | material: "Undefined/Steel_Undefined" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          12 x IFCBEAM | type IFCBEAMTYPE "RHS100*50*6" | object type "RHS100*50*6" | names: "BEAM" | descriptions: "RHS100*50*6" | material: "Undefined/Steel_Undefined" | property sets: Tekla Quantity, Tekla Common, Pset_BeamCommon, BaseQuantities
          24 x IFCBEAM | type IFCBEAMTYPE "D30" | object type "D30" | names: "BEAM" | descriptions: "D30" | material: "Undefined/Steel_Undefined" | property sets: Tekla Quantity, Tekla Common, Pset_BeamCommon, BaseQuantities
          12 x IFCPLATE | type IFCPLATETYPE "4*80" | object type "4*80" | names: "BEAM" | descriptions: "4*80" | material: "Undefined/Steel_Undefined" | property sets: Tekla Quantity, Tekla Common, Pset_PlateCommon, BaseQuantities
          12 x IFCBEAM | type IFCBEAMTYPE "PRMDAS120*200-110*160-5*0" | object type "PRMDAS120*200-110*160-5*0" | names: "BEAM" | descriptions: "PRMDAS120*200-110*160-5*0" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Tekla Quantity, Tekla Common, Pset_BeamCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "265*1310" | object type "265*1310" | FLOOR | names: "Repos" | descriptions: "265*1310" | material: layers "Floor: Insitu CONCRETE/B30-SKB" ("CONCRETE/B30-SKB" 265.) | property sets: Tekla Quantity, Tekla Common, Pset_SlabCommon, BaseQuantities
          3 x IFCCOLUMN | type IFCCOLUMNTYPE "D30" | object type "D30" | names: "Kamstål ø25" | descriptions: "D30" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity, Pset_ColumnCommon, BaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "20*215" | object type "20*215" | names: "STÅLSHIMS" | descriptions: "20*215" | material: "STEEL/S355J2G3" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "20*210" | object type "20*210" | names: "STÅLSHIMS" | descriptions: "20*210" | material: "STEEL/S355J2G3" | property sets: Tekla Quantity, Pset_BeamCommon, Tekla Common, BaseQuantities
          5 x IFCBEAM | type IFCBEAMTYPE "D10" | object type "D10" | names: "T.P." | descriptions: "D10" | material: "CONCRETE/B30-SKB" | property sets: Tekla Quantity, Tekla Common, Pset_BeamCommon, BaseQuantities
          18 x IFCBEAM | type IFCBEAMTYPE "10*80" | object type "10*80" | names: "Gummiplate 80x10x120" | descriptions: "10*80" | material: "STEEL/S355J2G3" | property sets: Tekla Quantity, Tekla Common, Pset_BeamCommon, BaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "10*160" | object type "10*160" | names: "Laskeplate 160x10x350" | descriptions: "10*160" | material: "STEEL/S355J2G3" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          3 x IFCCOLUMN | type IFCCOLUMNTYPE "950*500" | object type "950*500" | names: "BETONGSØYLE" | descriptions: "950*500" | material: "CONCRETE/B55" | property sets: Pset_ColumnCommon, Tekla Common, Tekla Quantity, BaseQuantities
          11 x IFCFOOTING | object type "2500*5000" | names: "PUNKTFUNDAMENT" | descriptions: "2500*5000" | material: "CONCRETE/B30" | property sets: Tekla Common, Tekla Quantity, BaseQuantities
          3 x IFCBEAM | type IFCBEAMTYPE "DLB500*520-800*200" | object type "DLB500*520-800*200" | names: "BETONGBJELKE" | descriptions: "DLB500*520-800*200" | material: "CONCRETE/B45-SKB" | property sets: Tekla Common, Pset_BeamCommon, Tekla Quantity, BaseQuantities
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "1700*400" | object type "1700*400" | names: "BETONGSØYLE" | descriptions: "1700*400" | material: "CONCRETE/B55" | property sets: Pset_ColumnCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "1100*600" | object type "1100*600" | names: "BETONGSØYLE" | descriptions: "1100*600" | material: "CONCRETE/B55" | property sets: Pset_ColumnCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "300*300" | object type "300*300" | names: "BETONGSØYLE" | descriptions: "300*300" | material: "CONCRETE/B55" | property sets: Pset_ColumnCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "400*600" | object type "400*600" | names: "BETONGSØYLE" | descriptions: "400*600" | material: "CONCRETE/B45" | property sets: Pset_ColumnCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "300*550" | object type "300*550" | names: "COLUMN" | descriptions: "300*550" | material: "CONCRETE/B45" | property sets: Pset_ColumnCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "600*550" | object type "600*550" | names: "BETONGSØYLE" | descriptions: "600*550" | material: "CONCRETE/B45" | property sets: Pset_ColumnCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "300*500" | object type "300*500" | names: "BETONGSØYLE" | descriptions: "300*500" | material: "CONCRETE/B45" | property sets: Pset_ColumnCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "4150*250" | object type "4150*250" | names: "BETONGVEGG" | descriptions: "4150*250" | material: layers "Wall: Insitu CONCRETE/B45" ("CONCRETE/B45" 250.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3100*250" | object type "3100*250" | names: "BETONGVEGG" | descriptions: "3100*250" | material: layers "Wall: Insitu CONCRETE/B55" ("CONCRETE/B55" 250.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCWALL | type IFCWALLTYPE "3100*300" | object type "3100*300" | names: "BETONGVEGG" | descriptions: "3100*300" | material: "CONCRETE/B55" | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3100*300" | object type "3100*300" | names: "BETONGVEGG" | descriptions: "3100*300" | material: layers "Wall: Insitu CONCRETE/B55" ("CONCRETE/B55" 300.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3100*200" | object type "3100*200" | names: "BETONGVEGG" | descriptions: "3100*200" | material: layers "Wall: Insitu CONCRETE/B45" ("CONCRETE/B45" 200.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3120*300" | object type "3120*300" | names: "BETONGVEGG" | descriptions: "3120*300" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 300.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3100*220" | object type "3100*220" | names: "BETONGVEGG" | descriptions: "3100*220" | material: layers "Wall: Insitu CONCRETE/B45" ("CONCRETE/B45" 220.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "200*600" | object type "200*600" | names: "BETONGSØYLE" | descriptions: "200*600" | material: "CONCRETE/B45" | property sets: Pset_ColumnCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCWALL | type IFCWALLTYPE "3070*300" | object type "3070*300" | names: "BETONGVEGG" | descriptions: "3070*300" | material: "CONCRETE/B45" | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "2950*250" | object type "2950*250" | names: "BETONGVEGG" | descriptions: "2950*250" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 250.) | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
      IFCBUILDINGSTOREY "U1" | elevation 10920.
        contains 1069 elements
          2 x IFCCOVERING | object type "V1-1" | names: "V1-1" | material: "Undefined/Undefined"
          4 x IFCWALL | type IFCWALLTYPE "2950*250" | object type "2950*250" | names: "BETONGVEGG" | descriptions: "2950*250" | material: "CONCRETE/B30" | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          4 x IFCBEAM | type IFCBEAMTYPE "DLB600*900-1000*250-350" | object type "DLB600*900-1000*250-350" | names: "BETONGBJELKE" | descriptions: "DLB600*900-1000*250-350" | material: "CONCRETE/B55-SKB" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          6 x IFCCOVERING | object type "V12" | names: "V12" | material: "Undefined/Undefined"
          4 x IFCWALL | type IFCWALLTYPE "3495*220" | object type "3495*220" | names: "BETONGVEGG" | descriptions: "3495*220" | material: "CONCRETE/B30" | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "LB500*750-700*250" | object type "LB500*750-700*250" | names: "BETONGBJELKE" | descriptions: "LB500*750-700*250" | material: "CONCRETE/B55-SKB" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          1 x IFCCOVERING | object type "V3-1" | names: "V3-1" | material: "Undefined/Undefined"
          1 x IFCWALL | type IFCWALLTYPE "2850*250" | object type "2850*250" | names: "INNERVEGG" | descriptions: "2850*250" | material: "CONCRETE/B30" | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          1 x IFCCOVERING | object type "P2" | names: "P2" | material: "Undefined/Undefined"
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "600*600" | object type "600*600" | names: "Pilaster" | descriptions: "600*600" | material: "CONCRETE/B45" | property sets: Pset_ColumnCommon, Tekla Common, Tekla Quantity, BaseQuantities
          103 x IFCBEAM | type IFCBEAMTYPE "HD500" | object type "HD500" | names: "HULLDEKKE" | descriptions: "HD500" | material: "CONCRETE/B45" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3495*200" | object type "3495*200" | names: "BETONGVEGG" | descriptions: "3495*200" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 200.) | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          10 x IFCCOLUMN | type IFCCOLUMNTYPE "900*400" | object type "900*400" | names: "BETONGSØYLE" | descriptions: "900*400" | material: "CONCRETE/B55-SKB"; "CONCRETE/B55" | property sets: Tekla Common, Tekla Quantity, Pset_ColumnCommon, BaseQuantities
          4 x IFCCOVERING | object type "P1" | names: "P1" | material: "Undefined/Undefined"
          6 x IFCCOLUMN | type IFCCOLUMNTYPE "400*400" | object type "400*400" | names: "Pilaster" | descriptions: "400*400" | material: "CONCRETE/B45" | property sets: Pset_ColumnCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCWALL | type IFCWALLTYPE "3495*200" | object type "3495*200" | names: "BETONGVEGG" | descriptions: "3495*200" | material: "CONCRETE/B30" | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          32 x IFCBEAM | type IFCBEAMTYPE "HD400" | object type "HD400" | names: "HULLDEKKE" | descriptions: "HD400" | material: "CONCRETE/B45" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "100*12420" | object type "100*12420" | FLOOR | names: "PÅSTØP" | descriptions: "100*12420" | material: layers "Floor: Insitu CONCRETE/B30" ("CONCRETE/B30" 100.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "DLB600*850-1000*250" | object type "DLB600*850-1000*250" | names: "BETONGBJELKE" | descriptions: "DLB600*850-1000*250" | material: "CONCRETE/B45-SKB" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "DLB600*1000-900*350-450" | object type "DLB600*1000-900*350-450" | names: "BETONGBJELKE" | descriptions: "DLB600*1000-900*350-450" | material: "CONCRETE/B55" | property sets: Tekla Common, Pset_BeamCommon, Tekla Quantity, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "2950*250" | object type "2950*250" | names: "BETONGVEGG" | descriptions: "2950*250" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 250.) | property sets: Tekla Common, Pset_WallCommon, Tekla Quantity, BaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "400*1200" | object type "400*1200" | names: "BETONGBJELKE" | descriptions: "400*1200" | material: "CONCRETE/B45-SKB" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "400*700" | object type "400*700" | names: "BETONGBJELKE" | descriptions: "400*700" | material: "CONCRETE/B45"; "CONCRETE/B55" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          2 x IFCCOVERING | object type "V7" | names: "V7" | material: "Undefined/Undefined"
          1 x IFCWALL | type IFCWALLTYPE "5000*200" | object type "5000*200" | names: "Kulvert" | descriptions: "5000*200" | material: "CONCRETE/B30" | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "250*200" | object type "250*200" | names: "Konsoll" | descriptions: "250*200" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 200.) | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "250*2000" | object type "250*2000" | FLOOR | names: "Avlastningsplate" | descriptions: "250*2000" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity, Pset_SlabCommon, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "650*250" | object type "650*250" | names: "INNERVEGG" | descriptions: "650*250" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 250.) | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "850*250" | object type "850*250" | names: "INNERVEGG" | descriptions: "850*250" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 250.) | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          4 x IFCFOOTING | object type "250*1200" | names: "BANKETT" | descriptions: "250*1200" | material: "CONCRETE/B30" | property sets: Tekla Common, Tekla Quantity, BaseQuantities
          6 x IFCCOLUMN | type IFCCOLUMNTYPE "D50" | object type "D50" | names: "Kotehøyde" | descriptions: "D50" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Pset_ColumnCommon, Tekla Common, Tekla Quantity, BaseQuantities
          4 x IFCWALL | type IFCWALLTYPE "950*250" | object type "950*250" | names: "INNERVEGG" | descriptions: "950*250" | material: "CONCRETE/B30" | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          5 x IFCBEAM | type IFCBEAMTYPE "PL10*80" | object type "PL10*80" | names: "STP" | descriptions: "PL10*80" | material: "STEEL/S355J2G3" | property sets: Tekla Quantity, Pset_BeamCommon, Tekla Common, BaseQuantities
          4 x IFCBEAM | type IFCBEAMTYPE "50*80" | object type "50*80" | names: "PLASTRØR 50x80" | descriptions: "50*80" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "1100*897" | object type "1100*897" | FLOOR | names: "TRAPP" | descriptions: "1100*897" | material: layers "Floor: Insitu CONCRETE/B30-SKB" ("CONCRETE/B30-SKB" 1100.) | property sets: Tekla Common, Tekla Quantity, Pset_SlabCommon, BaseQuantities
          13 x IFCBEAM | type IFCBEAMTYPE "D60" | object type "D60" | names: "KORR.RØR Ø60" | descriptions: "D60" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          65 x IFCBEAM | type IFCBEAMTYPE "50*10" | object type "50*10" | names: "TPA-FZ_2,5TONN", "TPA-FS_10,0TONN", "TPA-FZ_7,5TONN" (+39 more) | descriptions: "50*10" | material: "STEEL/S355J0" | property sets: Tekla Quantity, Tekla Common, Pset_BeamCommon, BaseQuantities
          73 x IFCBEAM | type IFCBEAMTYPE "D24" | object type "D24" | names: "Gjengestag" | descriptions: "D24" | material: "STEEL/S355J2H"; "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Quantity, Tekla Common, BaseQuantities
          288 x IFCBEAM | type IFCBEAMTYPE "NUT_M24" | object type "NUT_M24" | names: "Mutter" | descriptions: "NUT_M24" | material: "STEEL/S355J2H" | property sets: Tekla Quantity, Pset_BeamCommon, Tekla Common, BaseQuantities
          15 x IFCCOLUMN | type IFCCOLUMNTYPE "D5" | object type "D5" | names: "Koordpunkt", "Målepunkt" | descriptions: "D5" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity, Pset_ColumnCommon, BaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "15*450" | object type "15*450" | names: "STP8" | descriptions: "15*450" | material: "STEEL/S355J2G3" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          6 x IFCCOLUMN | type IFCCOLUMNTYPE "D25" | object type "D25" | names: "Kamstål ø25" | descriptions: "D25" | material: "REBAR/B500C" | property sets: Tekla Common, Tekla Quantity, Pset_ColumnCommon, BaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "D100" | object type "D100" | names: "KORR.RØR Ø100" | descriptions: "D100" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Tekla Quantity, Pset_BeamCommon, Tekla Common, BaseQuantities
          18 x IFCBEAM | type IFCBEAMTYPE "D50" | object type "D50" | names: "KORR.RØR_Ø50" | descriptions: "D50" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          6 x IFCBEAM | type IFCBEAMTYPE "L150*14" | object type "L150*14" | names: "Stålvinkel" | descriptions: "L150*14" | material: "STEEL/S355J2H" | property sets: Tekla Quantity, Pset_BeamCommon, Tekla Common, BaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "15*250" | object type "15*250" | names: "STP17" | descriptions: "15*250" | material: "STEEL/S355J2G3" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          51 x IFCCOLUMN | type IFCCOLUMNTYPE "D20" | object type "D20" | names: "Kamstål ø20", "Flattstål", "BEAM" (+6 more) | descriptions: "D20" | material: "REBAR/B500C"; "STEEL/S355J0" | property sets: Tekla Quantity, Tekla Common, Pset_ColumnCommon, BaseQuantities
          5 x IFCCOLUMN | type IFCCOLUMNTYPE "D24" | object type "D24" | names: "Gjengestag M24" | descriptions: "D24" | material: "STEEL/S355J0" | property sets: Tekla Quantity, Pset_ColumnCommon, Tekla Common, BaseQuantities
          4 x IFCCOLUMN | type IFCCOLUMNTYPE "80*70" | object type "80*70" | names: "Skive 70x80x12" | descriptions: "80*70" | material: "STEEL/S355J0" | property sets: Tekla Quantity, Pset_ColumnCommon, Tekla Common, BaseQuantities
          5 x IFCCOLUMN | type IFCCOLUMNTYPE "HALFEN_NUT-M24" | object type "HALFEN_NUT-M24" | names: "Mutter M24" | descriptions: "HALFEN_NUT-M24" | material: "STEEL/S355J0" | property sets: Tekla Quantity, Pset_ColumnCommon, Tekla Common, BaseQuantities
          2 x IFCCOVERING | object type "V1-3" | names: "V1-3" | material: "Undefined/Undefined"
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "680*200" | object type "680*200" | names: "Kulvert" | descriptions: "680*200" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 200.) | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "400*645" | object type "400*645" | names: "BETONGBJELKE" | descriptions: "400*645" | material: "CONCRETE/B45-SKB" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "PL20*150" | object type "PL20*150" | names: "STP16" | descriptions: "PL20*150" | material: "STEEL/S355J2G3" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          30 x IFCBEAM | type IFCBEAMTYPE "D16" | object type "D16" | names: "BEAM", "Kamstål", "Flattstål" | descriptions: "D16" | material: "REBAR/B500C"; "REBAR/B500NC"; "STEEL/S355J0" | property sets: Tekla Quantity, Pset_BeamCommon, Tekla Common, BaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "PL25*200" | object type "PL25*200" | names: "STP6" | descriptions: "PL25*200" | material: "STEEL/S355J2G3" | property sets: Tekla Quantity, Pset_BeamCommon, Tekla Common, BaseQuantities
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "600*300" | object type "600*300" | names: "BETONGSØYLE" | descriptions: "600*300" | material: "CONCRETE/B45-SKB" | property sets: Tekla Common, Tekla Quantity, Pset_ColumnCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "1100*1490" | object type "1100*1490" | FLOOR | names: "TRAPP" | descriptions: "1100*1490" | material: layers "Floor: Insitu CONCRETE/B30-SKB" ("CONCRETE/B30-SKB" 1100.) | property sets: Tekla Common, Tekla Quantity, Pset_SlabCommon, BaseQuantities
          12 x IFCBEAM | type IFCBEAMTYPE "PRMDAS120*200-110*160-5*0" | object type "PRMDAS120*200-110*160-5*0" | names: "BEAM" | descriptions: "PRMDAS120*200-110*160-5*0" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Tekla Quantity, Tekla Common, Pset_BeamCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "265*2291" | object type "265*2291" | FLOOR | names: "Repos" | descriptions: "265*2291" | material: layers "Floor: Insitu CONCRETE/B30-SKB" ("CONCRETE/B30-SKB" 265.) | property sets: Tekla Common, Tekla Quantity, Pset_SlabCommon, BaseQuantities
          1 x IFCPLATE | type IFCPLATETYPE "PL20*235" | object type "PL20*235" | names: "PLATE" | descriptions: "PL20*235" | material: "STEEL/S235JR" | property sets: Tekla Common, Tekla Quantity, Pset_PlateCommon, BaseQuantities
          1 x IFCPLATE | type IFCPLATETYPE "PL20*424" | object type "PL20*424" | names: "PLATE" | descriptions: "PL20*424" | material: "STEEL/S235JR" | property sets: Tekla Common, Tekla Quantity, Pset_PlateCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "1110*375" | object type "1110*375" | FLOOR | names: "TRAPP" | descriptions: "1110*375" | material: layers "Floor: Insitu CONCRETE/B30-SKB" ("CONCRETE/B30-SKB" 1110.) | property sets: Tekla Common, Tekla Quantity, Pset_SlabCommon, BaseQuantities
          12 x IFCBEAM | type IFCBEAMTYPE "RHS120*80*5" | object type "RHS120*80*5" | names: "TSS102" | descriptions: "RHS120*80*5" | material: "Undefined/Steel_Undefined" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          12 x IFCBEAM | type IFCBEAMTYPE "RHS100*50*6" | object type "RHS100*50*6" | names: "BEAM" | descriptions: "RHS100*50*6" | material: "Undefined/Steel_Undefined" | property sets: Tekla Quantity, Tekla Common, Pset_BeamCommon, BaseQuantities
          24 x IFCBEAM | type IFCBEAMTYPE "D30" | object type "D30" | names: "BEAM" | descriptions: "D30" | material: "Undefined/Steel_Undefined" | property sets: Tekla Quantity, Tekla Common, Pset_BeamCommon, BaseQuantities
          12 x IFCPLATE | type IFCPLATETYPE "4*80" | object type "4*80" | names: "BEAM" | descriptions: "4*80" | material: "Undefined/Steel_Undefined" | property sets: Tekla Quantity, Tekla Common, Pset_PlateCommon, BaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "20*215" | object type "20*215" | names: "STÅLSHIMS" | descriptions: "20*215" | material: "STEEL/S355J2G3" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          6 x IFCCOLUMN | type IFCCOLUMNTYPE "860*360" | object type "860*360" | names: "360x860x10 m/hull" | descriptions: "860*360" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity, Pset_ColumnCommon, BaseQuantities
          8 x IFCCOLUMN | type IFCCOLUMNTYPE "D30" | object type "D30" | names: "Kamstål ø25", "Gjengestag M30" | descriptions: "D30" | material: "STEEL/S355J0" | property sets: Tekla Quantity, Pset_ColumnCommon, BaseQuantities, Tekla Common
          46 x IFCBEAM | type IFCBEAMTYPE "D20" | object type "D20" | names: "Bunnfyllingslist", "BETONGBJELKE", "Flattstål" (+4 more) | descriptions: "D20" | material: "MISCELLANEOUS/NEOPREN"; "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "80*80" | object type "80*80" | names: "Skive 80x80x12" | descriptions: "80*80" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity, Pset_ColumnCommon, BaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "20*210" | object type "20*210" | names: "STÅLSHIMS" | descriptions: "20*210" | material: "STEEL/S355J2G3" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3545*250" | object type "3545*250" | names: "BETONGVEGG" | descriptions: "3545*250" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 250.) | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          5 x IFCBEAM | type IFCBEAMTYPE "D10" | object type "D10" | names: "T.P." | descriptions: "D10" | material: "CONCRETE/B30-SKB" | property sets: Tekla Quantity, Tekla Common, Pset_BeamCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "265*1310" | object type "265*1310" | FLOOR | names: "Repos" | descriptions: "265*1310" | material: layers "Floor: Insitu CONCRETE/B30-SKB" ("CONCRETE/B30-SKB" 265.) | property sets: Tekla Common, Tekla Quantity, Pset_SlabCommon, BaseQuantities
          18 x IFCBEAM | type IFCBEAMTYPE "10*80" | object type "10*80" | names: "Gummiplate 80x10x120" | descriptions: "10*80" | material: "STEEL/S355J2G3" | property sets: Tekla Quantity, Tekla Common, Pset_BeamCommon, BaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "10*160" | object type "10*160" | names: "Laskeplate 160x10x350" | descriptions: "10*160" | material: "STEEL/S355J2G3" | property sets: Tekla Quantity, Tekla Common, Pset_BeamCommon, BaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "PL40*1000" | object type "PL40*1000" | names: "ST" | descriptions: "PL40*1000" | material: "STEEL/S355J2G3" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          6 x IFCCOLUMN | type IFCCOLUMNTYPE "D75" | object type "D75" | names: "KORR.RØR_Ø75" | descriptions: "D75" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Tekla Quantity, Pset_ColumnCommon, Tekla Common, BaseQuantities
          5 x IFCBEAM | type IFCBEAMTYPE "L150*12" | object type "L150*12" | names: "Stålvinkel" | descriptions: "L150*12" | material: "STEEL/S355J2H" | property sets: Tekla Quantity, Pset_BeamCommon, Tekla Common, BaseQuantities
          4 x IFCBEAM | type IFCBEAMTYPE "15*200" | object type "15*200" | names: "Laskeplate 900x200x15" | descriptions: "15*200" | material: "STEEL/S355J2G3" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "20*410" | object type "20*410" | names: "STÅLSHIMS" | descriptions: "20*410" | material: "STEEL/S355J2G3" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          4 x IFCBEAM | type IFCBEAMTYPE "PL40*550" | object type "PL40*550" | names: "ST", "ST20" | descriptions: "PL40*550" | material: "STEEL/S355J2G3" | property sets: Tekla Quantity, Tekla Common, Pset_BeamCommon, BaseQuantities
          8 x IFCBEAM | type IFCBEAMTYPE "D75" | object type "D75" | names: "KORR.RØR_Ø75" | descriptions: "D75" | material: "MISCELLANEOUS/NEOPREN" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          1 x IFCPLATE | type IFCPLATETYPE "PL25*240" | object type "PL25*240" | names: "PLATE" | descriptions: "PL25*240" | material: "STEEL/S355J2H" | property sets: Tekla Common, Tekla Quantity, Pset_PlateCommon, BaseQuantities
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "CFRHS200*100*12.5" | object type "CFRHS200*100*12.5" | names: "STÅLSØYLE" | descriptions: "CFRHS200*100*12.5" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity, Pset_ColumnCommon, BaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "PL20*130" | object type "PL20*130" | names: "PLATE" | descriptions: "PL20*130" | material: "STEEL/S355J2H" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "8*100" | object type "8*100" | names: "Flattstål" | descriptions: "8*100" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "1700*400" | object type "1700*400" | names: "BETONGSØYLE" | descriptions: "1700*400" | material: "CONCRETE/B55" | property sets: Pset_ColumnCommon, Tekla Common, Tekla Quantity, BaseQuantities
          3 x IFCBEAM | type IFCBEAMTYPE "DLB500*700-800*200" | object type "DLB500*700-800*200" | names: "BETONGBJELKE" | descriptions: "DLB500*700-800*200" | material: "CONCRETE/B45-SKB" | property sets: Pset_BeamCommon, Tekla Common, Tekla Quantity, BaseQuantities
          9 x IFCBEAM | type IFCBEAMTYPE "HD320" | object type "HD320" | names: "HULLDEKKE" | descriptions: "HD320" | material: "CONCRETE/B45" | property sets: Tekla Common, Pset_BeamCommon, Tekla Quantity, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "2250*300" | object type "2250*300" | names: "BETONGVEGG" | descriptions: "2250*300" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 300.) | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          12 x IFCBEAM | type IFCBEAMTYPE "610*150" | object type "610*150" | names: "Teglkon(eks.Ytong)" | descriptions: "610*150" | material: "CONCRETE/B35" | property sets: Tekla Common, Pset_BeamCommon, Tekla Quantity, BaseQuantities
          13 x IFCBEAM | type IFCBEAMTYPE "L200*16" | object type "L200*16" | names: "TEGLKONSOLL" | descriptions: "L200*16" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "950*500" | object type "950*500" | names: "BETONGSØYLE" | descriptions: "950*500" | material: "CONCRETE/B55" | property sets: Pset_ColumnCommon, Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCCOLUMN | type IFCCOLUMNTYPE "800*400" | object type "800*400" | names: "BETONGSØYLE" | descriptions: "800*400" | material: "CONCRETE/B55" | property sets: Pset_ColumnCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "20*200" | object type "20*200" | names: "Flattstål" | descriptions: "20*200" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3100*250" | object type "3100*250" | names: "BETONGVEGG" | descriptions: "3100*250" | material: layers "Wall: Insitu CONCRETE/B45" ("CONCRETE/B45" 250.); layers "Wall: Insitu CONCRETE/B55" ("CONCRETE/B55" 250.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCWALL | type IFCWALLTYPE "3100*300" | object type "3100*300" | names: "BETONGVEGG" | descriptions: "3100*300" | material: "CONCRETE/B55" | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3100*300" | object type "3100*300" | names: "BETONGVEGG" | descriptions: "3100*300" | material: layers "Wall: Insitu CONCRETE/B55" ("CONCRETE/B55" 300.); layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 300.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3100*200" | object type "3100*200" | names: "BETONGVEGG" | descriptions: "3100*200" | material: layers "Wall: Insitu CONCRETE/B45" ("CONCRETE/B45" 200.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3100*220" | object type "3100*220" | names: "BETONGVEGG" | descriptions: "3100*220" | material: layers "Wall: Insitu CONCRETE/B45" ("CONCRETE/B45" 220.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
    IFCBUILDING "Undefined"
      IFCBUILDINGSTOREY "Undefined" | elevation 0.
        contains 531 elements
          21 x IFCCOLUMN | type IFCCOLUMNTYPE "500*500" | object type "500*500" | names: "NULLPUNKTSØYLE" | descriptions: "500*500" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Tekla Quantity, BaseQuantities, Pset_ColumnCommon, Tekla Common
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "900*400" | object type "900*400" | names: "BETONGSØYLE" | descriptions: "900*400" | material: "CONCRETE/B55" | property sets: Tekla Common, Tekla Quantity, Pset_ColumnCommon, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3100*200" | object type "3100*200" | names: "BETONGVEGG" | descriptions: "3100*200" | material: layers "Wall: Insitu CONCRETE/B45" ("CONCRETE/B45" 200.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3150*200" | object type "3150*200" | names: "BETONGVEGG" | descriptions: "3150*200" | material: layers "Wall: Insitu CONCRETE/B45" ("CONCRETE/B45" 200.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "1220*200" | object type "1220*200" | names: "Heisgrube" | descriptions: "1220*200" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 200.) | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          2 x IFCSLAB | type IFCSLABTYPE "270*5680" | object type "270*5680" | FLOOR | names: "BETONGDEKKE" | descriptions: "270*5680" | material: layers "Floor: Insitu CONCRETE/B30" ("CONCRETE/B30" 270.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          6 x IFCPLATE | type IFCPLATETYPE "120*1592" | object type "120*1592" | names: "BAD" | descriptions: "120*1592" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Pset_PlateCommon, Tekla Quantity, Tekla Common, BaseQuantities
          3 x IFCPLATE | type IFCPLATETYPE "120*2016" | object type "120*2016" | names: "BAD" | descriptions: "120*2016" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Pset_PlateCommon, Tekla Quantity, Tekla Common, BaseQuantities
          3 x IFCPLATE | type IFCPLATETYPE "120*1566" | object type "120*1566" | names: "BAD" | descriptions: "120*1566" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Pset_PlateCommon, Tekla Quantity, Tekla Common, BaseQuantities
          3 x IFCPLATE | type IFCPLATETYPE "120*1924" | object type "120*1924" | names: "BAD" | descriptions: "120*1924" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Pset_PlateCommon, Tekla Quantity, Tekla Common, BaseQuantities
          3 x IFCPLATE | type IFCPLATETYPE "120*1575" | object type "120*1575" | names: "BAD" | descriptions: "120*1575" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Tekla Quantity, Pset_PlateCommon, Tekla Common, BaseQuantities
          1 x IFCPLATE | type IFCPLATETYPE "120*1875" | object type "120*1875" | names: "BAD" | descriptions: "120*1875" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Pset_PlateCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCPLATE | type IFCPLATETYPE "120*1650" | object type "120*1650" | names: "BAD" | descriptions: "120*1650" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Pset_PlateCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCPLATE | type IFCPLATETYPE "120*1999" | object type "120*1999" | names: "BAD" | descriptions: "120*1999" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Pset_PlateCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCPLATE | type IFCPLATETYPE "120*1200" | object type "120*1200" | names: "BAD" | descriptions: "120*1200" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Pset_PlateCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCPLATE | type IFCPLATETYPE "120*1574" | object type "120*1574" | names: "BAD" | descriptions: "120*1574" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Pset_PlateCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCPLATE | type IFCPLATETYPE "120*1595" | object type "120*1595" | names: "BAD" | descriptions: "120*1595" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Pset_PlateCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCPLATE | type IFCPLATETYPE "120*1047" | object type "120*1047" | names: "BAD" | descriptions: "120*1047" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Pset_PlateCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCPLATE | type IFCPLATETYPE "120*2281" | object type "120*2281" | names: "BAD" | descriptions: "120*2281" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Pset_PlateCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCPLATE | type IFCPLATETYPE "120*1612" | object type "120*1612" | names: "BAD" | descriptions: "120*1612" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Pset_PlateCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCPLATE | type IFCPLATETYPE "120*1470" | object type "120*1470" | names: "BAD" | descriptions: "120*1470" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Pset_PlateCommon, Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCSLAB | type IFCSLABTYPE "120*1592" | object type "120*1592" | FLOOR | names: "Bad" | descriptions: "120*1592" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 120.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "120*2179" | object type "120*2179" | FLOOR | names: "Bad" | descriptions: "120*2179" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 120.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "120*2129" | object type "120*2129" | FLOOR | names: "Bad" | descriptions: "120*2129" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 120.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCPLATE | type IFCPLATETYPE "120*1865" | object type "120*1865" | names: "BAD" | descriptions: "120*1865" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Tekla Common, Pset_PlateCommon, Tekla Quantity, BaseQuantities
          1 x IFCPLATE | type IFCPLATETYPE "120*1321" | object type "120*1321" | names: "BAD" | descriptions: "120*1321" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Tekla Common, Pset_PlateCommon, Tekla Quantity, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3400*250" | object type "3400*250" | names: "BETONGVEGG" | descriptions: "3400*250" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 250.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          3 x IFCFOOTING | object type "300*1500" | names: "Bankett", "BANKETT" | descriptions: "300*1500" | material: "CONCRETE/B30" | property sets: Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "250*2000" | object type "250*2000" | FLOOR | names: "Avlastningsplate" | descriptions: "250*2000" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity, Pset_SlabCommon, BaseQuantities
          1 x IFCFOOTING | object type "400*1500" | names: "Bankett" | descriptions: "400*1500" | material: "CONCRETE/B30" | property sets: Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCCOLUMN | type IFCCOLUMNTYPE "RHS200*100*16" | object type "RHS200*100*16" | names: "STÅLSØYLE" | descriptions: "RHS200*100*16" | material: "STEEL/S355J0" | property sets: Pset_ColumnCommon, Tekla Quantity, Tekla Common, BaseQuantities
          14 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "250*200" | object type "250*200" | names: "Konsoll" | descriptions: "250*200" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 200.) | property sets: Tekla Common, Pset_WallCommon, Tekla Quantity, BaseQuantities
          4 x IFCBEAM | type IFCBEAMTYPE "HD320" | object type "HD320" | names: "HULLDEKKE" | descriptions: "HD320" | material: "CONCRETE/B45" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "200*200" | object type "200*200" | names: "Konsoll" | descriptions: "200*200" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 200.) | property sets: Pset_WallCommon, Tekla Quantity, Tekla Common, BaseQuantities
          2 x IFCSLAB | type IFCSLABTYPE "320*790" | object type "320*790" | FLOOR | names: "BETONGDEKKE" | descriptions: "320*790" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 320.) | property sets: Pset_SlabCommon, Tekla Quantity, Tekla Common, BaseQuantities
          3 x IFCBEAM | type IFCBEAMTYPE "HD500" | object type "HD500" | names: "HULLDEKKE" | descriptions: "HD500" | material: "CONCRETE/B45" | property sets: Pset_BeamCommon, Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCWALL | type IFCWALLTYPE "250*200" | object type "250*200" | names: "Konsoll" | descriptions: "250*200" | material: "CONCRETE/B30" | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "300*550" | object type "300*550" | names: "COLUMN" | descriptions: "300*550" | material: "CONCRETE/B45" | property sets: Pset_ColumnCommon, Tekla Common, Tekla Quantity, BaseQuantities
          3 x IFCFOOTING | object type "400*1000" | names: "B2" | descriptions: "400*1000" | material: "CONCRETE/B30" | property sets: Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3050*300" | object type "3050*300" | names: "BETONGVEGG" | descriptions: "3050*300" | material: layers "Wall: Insitu CONCRETE/B45" ("CONCRETE/B45" 300.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          3 x IFCFOOTING | object type "1400*1400" | names: "F1" | descriptions: "1400*1400" | material: "CONCRETE/B30" | property sets: Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCPLATE | type IFCPLATETYPE "50*24400" | object type "50*24400" | names: "ASFALT" | descriptions: "50*24400" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Pset_PlateCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "100*5342" | object type "100*5342" | FLOOR | names: "GULV PÅ GRUNN" | descriptions: "100*5342" | material: layers "Floor: Insitu CONCRETE/B30" ("CONCRETE/B30" 100.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "100*3250" | object type "100*3250" | FLOOR | names: "GULV PÅ GRUNN" | descriptions: "100*3250" | material: layers "Floor: Insitu CONCRETE/B30" ("CONCRETE/B30" 100.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "100*8100" | object type "100*8100" | FLOOR | names: "GULV PÅ GRUNN" | descriptions: "100*8100" | material: layers "Floor: Insitu CONCRETE/B30" ("CONCRETE/B30" 100.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "100*10970" | object type "100*10970" | FLOOR | names: "GULV PÅ GRUNN" | descriptions: "100*10970" | material: layers "Floor: Insitu CONCRETE/B30" ("CONCRETE/B30" 100.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "100*5180" | object type "100*5180" | FLOOR | names: "GULV PÅ GRUNN" | descriptions: "100*5180" | material: layers "Floor: Insitu CONCRETE/B30" ("CONCRETE/B30" 100.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "100*9590" | object type "100*9590" | FLOOR | names: "GULV PÅ GRUNN" | descriptions: "100*9590" | material: layers "Floor: Insitu CONCRETE/B30" ("CONCRETE/B30" 100.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "50*9022" | object type "50*9022" | FLOOR | names: "Påstøp" | descriptions: "50*9022" | material: layers "Floor: Insitu CONCRETE/B30" ("CONCRETE/B30" 50.) | property sets: Tekla Common, Pset_SlabCommon, Tekla Quantity, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "50*9590" | object type "50*9590" | FLOOR | names: "Påstøp" | descriptions: "50*9590" | material: layers "Floor: Insitu CONCRETE/B30" ("CONCRETE/B30" 50.) | property sets: Tekla Common, Pset_SlabCommon, Tekla Quantity, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "50*5342" | object type "50*5342" | FLOOR | names: "Påstøp" | descriptions: "50*5342" | material: layers "Floor: Insitu CONCRETE/B30" ("CONCRETE/B30" 50.) | property sets: Tekla Common, Tekla Quantity, Pset_SlabCommon, BaseQuantities
          1 x IFCWALL | type IFCWALLTYPE "3500*400" | object type "3500*400" | names: "BETONGVEGG" | descriptions: "3500*400" | material: "CONCRETE/B45" | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          6 x IFCPLATE | type IFCPLATETYPE "PL25*150" | object type "PL25*150" | names: "PLATE" | descriptions: "PL25*150" | material: "STEEL/S235JR" | property sets: Pset_PlateCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCPLATE | type IFCPLATETYPE "PL25*200" | object type "PL25*200" | names: "PLATE" | descriptions: "PL25*200" | material: "STEEL/S235JR" | property sets: Pset_PlateCommon, Tekla Common, Tekla Quantity, BaseQuantities
          4 x IFCBEAM | type IFCBEAMTYPE "L150*14" | object type "L150*14" | names: "Stålvinkel" | descriptions: "L150*14" | material: "STEEL/S355J2H" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "950*500" | object type "950*500" | names: "COLUMN" | descriptions: "950*500" | material: "CONCRETE/B55" | property sets: Tekla Common, Tekla Quantity, Pset_ColumnCommon, BaseQuantities
          1 x IFCPLATE | type IFCPLATETYPE "120*1192" | object type "120*1192" | names: "BAD" | descriptions: "120*1192" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Pset_PlateCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCPLATE | type IFCPLATETYPE "120*2314" | object type "120*2314" | names: "BAD" | descriptions: "120*2314" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Tekla Common, Tekla Quantity, Pset_PlateCommon, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*250" | object type "3000*250" | names: "BETONGVEGG" | descriptions: "3000*250" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 250.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCWALL | type IFCWALLTYPE "3000*250" | object type "3000*250" | names: "BETONGVEGG" | descriptions: "3000*250" | material: "CONCRETE/B30" | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "4450*250" | object type "4450*250" | names: "BETONGVEGG" | descriptions: "4450*250" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 250.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          14 x IFCSLAB | type IFCSLABTYPE "270*2170" | object type "270*2170" | FLOOR | names: "BALKONG" | descriptions: "270*2170" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 270.) | property sets: Tekla Quantity, Pset_SlabCommon, BaseQuantities, Tekla Common
          3 x IFCCOLUMN | type IFCCOLUMNTYPE "CFRHS200X100X12.5" | object type "CFRHS200X100X12.5" | names: "STÅLSØYLE" | descriptions: "CFRHS200X100X12.5" | material: "STEEL/S355J0" | property sets: Pset_ColumnCommon, Tekla Quantity, BaseQuantities, Tekla Common
          3 x IFCCOLUMN | type IFCCOLUMNTYPE "CFRHS100X10" | object type "CFRHS100X10" | names: "STÅLSØYLE" | descriptions: "CFRHS100X10" | material: "STEEL/S355J0" | property sets: Pset_ColumnCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "250*5680" | object type "250*5680" | FLOOR | names: "BETONGDEKKE" | descriptions: "250*5680" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 250.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "1000*250" | object type "1000*250" | names: "BETONGVEGG" | descriptions: "1000*250" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 250.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "250*3100" | object type "250*3100" | FLOOR | names: "BETONGDEKKE" | descriptions: "250*3100" | material: layers "Floor: Insitu CONCRETE/B35" ("CONCRETE/B35" 250.) | property sets: Tekla Common, Tekla Quantity, Pset_SlabCommon, BaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "IPE240" | object type "IPE240" | names: "STÅLBJELKE" | descriptions: "IPE240" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Common, Tekla Quantity, BaseQuantities
          14 x IFCCOLUMN | type IFCCOLUMNTYPE "CFRHS80X8" | object type "CFRHS80X8" | names: "STÅLSØYLE" | descriptions: "CFRHS80X8" | material: "STEEL/S355J0" | property sets: Pset_ColumnCommon, Tekla Common, Tekla Quantity, BaseQuantities
          5 x IFCBEAM | type IFCBEAMTYPE "HSQ250*8-30*150-10*450" | object type "HSQ250*8-30*150-10*450" | names: "STÅLBJELKE" | descriptions: "HSQ250*8-30*150-10*450" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "UPE270" | object type "UPE270" | names: "STÅLBJELKE" | descriptions: "UPE270" | material: "STEEL/S355J0" | property sets: Pset_BeamCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "80*9590" | object type "80*9590" | FLOOR | names: "PÅSTØP" | descriptions: "80*9590" | material: layers "Floor: Insitu CONCRETE/B30" ("CONCRETE/B30" 80.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "80*6971" | object type "80*6971" | FLOOR | names: "PÅSTØP" | descriptions: "80*6971" | material: layers "Floor: Insitu CONCRETE/B30" ("CONCRETE/B30" 80.) | property sets: Pset_SlabCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "80*2282" | object type "80*2282" | FLOOR | names: "PÅSTØP" | descriptions: "80*2282" | material: layers "Floor: Insitu CONCRETE/B30" ("CONCRETE/B30" 80.) | property sets: Tekla Common, Tekla Quantity, Pset_SlabCommon, BaseQuantities
          1 x IFCFOOTING | object type "250*1200" | names: "BANKETT" | descriptions: "250*1200" | material: "CONCRETE/B30" | property sets: Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "950*250" | object type "950*250" | names: "INNERVEGG" | descriptions: "950*250" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 250.) | property sets: Tekla Common, Pset_WallCommon, Tekla Quantity, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "6450*300" | object type "6450*300" | names: "BETONGVEGG" | descriptions: "6450*300" | material: layers "Wall: Insitu CONCRETE/B45" ("CONCRETE/B45" 300.) | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          9 x IFCBEAM | type IFCBEAMTYPE "750*150" | object type "750*150" | names: "Ringmur" | descriptions: "750*150" | material: "CONCRETE/B45" | property sets: Pset_BeamCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3150*250" | object type "3150*250" | names: "BETONGVEGG" | descriptions: "3150*250" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 250.) | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          12 x IFCCOVERING | object type "V12" | names: "V12" | material: "Undefined/Undefined"
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3545*250" | object type "3545*250" | names: "BETONGVEGG" | descriptions: "3545*250" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 250.) | property sets: Tekla Common, Pset_WallCommon, Tekla Quantity, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "2950*250" | object type "2950*250" | names: "BETONGVEGG" | descriptions: "2950*250" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 250.) | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          1 x IFCMEMBER | type IFCMEMBERTYPE "CFRHS250X150X12.5" | object type "CFRHS250X150X12.5" | names: "STÅLBJELKE" | descriptions: "CFRHS250X150X12.5" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity, Pset_MemberCommon, BaseQuantities
          4 x IFCBEAM | type IFCBEAMTYPE "400*150" | object type "400*150" | names: "Ringmur" | descriptions: "400*150" | material: "CONCRETE/B45" | property sets: Tekla Common, Pset_BeamCommon, Tekla Quantity, BaseQuantities
          2 x IFCWALL | type IFCWALLTYPE "3000*220" | object type "3000*220" | names: "BETONGVEGG" | descriptions: "3000*220" | material: "CONCRETE/B30" | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          2 x IFCWALL | type IFCWALLTYPE "3120*220" | object type "3120*220" | names: "BETONGVEGG" | descriptions: "3120*220" | material: "CONCRETE/B30" | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          4 x IFCWALL | type IFCWALLTYPE "3495*220" | object type "3495*220" | names: "BETONGVEGG" | descriptions: "3495*220" | material: "CONCRETE/B30" | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3000*200" | object type "3000*200" | names: "BETONGVEGG" | descriptions: "3000*200" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 200.) | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "3495*200" | object type "3495*200" | names: "BETONGVEGG" | descriptions: "3495*200" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 200.) | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          1 x IFCWALL | type IFCWALLTYPE "3000*200" | object type "3000*200" | names: "BETONGVEGG" | descriptions: "3000*200" | material: "CONCRETE/B30" | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          1 x IFCWALL | type IFCWALLTYPE "3495*200" | object type "3495*200" | names: "BETONGVEGG" | descriptions: "3495*200" | material: "CONCRETE/B30" | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "265*2159" | object type "265*2159" | FLOOR | names: "Repos" | descriptions: "265*2159" | material: layers "Floor: Insitu CONCRETE/B30-SKB" ("CONCRETE/B30-SKB" 265.) | property sets: Tekla Common, Tekla Quantity, Pset_SlabCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "1100*1323" | object type "1100*1323" | FLOOR | names: "TRAPP" | descriptions: "1100*1323" | material: layers "Floor: Insitu CONCRETE/B30-SKB" ("CONCRETE/B30-SKB" 1100.) | property sets: Tekla Common, Tekla Quantity, Pset_SlabCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "1100*897" | object type "1100*897" | FLOOR | names: "TRAPP" | descriptions: "1100*897" | material: layers "Floor: Insitu CONCRETE/B30-SKB" ("CONCRETE/B30-SKB" 1100.) | property sets: Tekla Common, Tekla Quantity, Pset_SlabCommon, BaseQuantities
          2 x IFCSLAB | type IFCSLABTYPE "1110*375" | object type "1110*375" | FLOOR | names: "TRAPP" | descriptions: "1110*375" | material: layers "Floor: Insitu CONCRETE/B30-SKB" ("CONCRETE/B30-SKB" 1110.) | property sets: Tekla Common, Tekla Quantity, Pset_SlabCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "1100*1219" | object type "1100*1219" | FLOOR | names: "TRAPP" | descriptions: "1100*1219" | material: layers "Floor: Insitu CONCRETE/B30-SKB" ("CONCRETE/B30-SKB" 1100.) | property sets: Tekla Common, Tekla Quantity, Pset_SlabCommon, BaseQuantities
          24 x IFCBEAM | type IFCBEAMTYPE "PRMDAS120*200-110*160-5*0" | object type "PRMDAS120*200-110*160-5*0" | names: "BEAM" | descriptions: "PRMDAS120*200-110*160-5*0" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Tekla Quantity, Pset_BeamCommon, Tekla Common, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "1100*1490" | object type "1100*1490" | FLOOR | names: "TRAPP" | descriptions: "1100*1490" | material: layers "Floor: Insitu CONCRETE/B30-SKB" ("CONCRETE/B30-SKB" 1100.) | property sets: Tekla Common, Tekla Quantity, Pset_SlabCommon, BaseQuantities
          2 x IFCSLAB | type IFCSLABTYPE "265*1310" | object type "265*1310" | FLOOR | names: "Repos" | descriptions: "265*1310" | material: layers "Floor: Insitu CONCRETE/B30-SKB" ("CONCRETE/B30-SKB" 265.) | property sets: Tekla Quantity, Pset_SlabCommon, Tekla Common, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "265*2291" | object type "265*2291" | FLOOR | names: "Repos" | descriptions: "265*2291" | material: layers "Floor: Insitu CONCRETE/B30-SKB" ("CONCRETE/B30-SKB" 265.) | property sets: Tekla Common, Tekla Quantity, Pset_SlabCommon, BaseQuantities
          36 x IFCBEAM | type IFCBEAMTYPE "10*80" | object type "10*80" | names: "Gummiplate 80x10x120" | descriptions: "10*80" | material: "STEEL/S355J2G3" | property sets: Tekla Quantity, Pset_BeamCommon, Tekla Common, BaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "10*160" | object type "10*160" | names: "Laskeplate 160x10x350" | descriptions: "10*160" | material: "STEEL/S355J2G3" | property sets: Tekla Quantity, Pset_BeamCommon, Tekla Common, BaseQuantities
          9 x IFCCOLUMN | type IFCCOLUMNTYPE "D20" | object type "D20" | names: "Kamstål ø20", "Flattstål" | descriptions: "D20" | material: "STEEL/S355J0" | property sets: Tekla Quantity, Pset_ColumnCommon, Tekla Common, BaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "8*100" | object type "8*100" | names: "Flattstål" | descriptions: "8*100" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          6 x IFCBEAM | type IFCBEAMTYPE "D20" | object type "D20" | names: "Gjengestag M20", "Flattstål" | descriptions: "D20" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          1 x IFCCOVERING | object type "arm-tegn, verv v. BT3" | names: "arm-tegn, verv v. BT3" | material: "Undefined/Undefined"
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "250*250" | object type "250*250" | names: "Mangler 6ø16 ift arm-" | descriptions: "250*250" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 250.) | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          10 x IFCBEAM | type IFCBEAMTYPE "D10" | object type "D10" | names: "T.P." | descriptions: "D10" | material: "CONCRETE/B30-SKB" | property sets: Tekla Quantity, Pset_BeamCommon, Tekla Common, BaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "D16" | object type "D16" | names: "Flattstål" | descriptions: "D16" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          4 x IFCBEAM | type IFCBEAMTYPE "D50" | object type "D50" | names: "KORR.RØR_Ø50" | descriptions: "D50" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          24 x IFCBEAM | type IFCBEAMTYPE "RHS120*80*5" | object type "RHS120*80*5" | names: "TSS102" | descriptions: "RHS120*80*5" | material: "Undefined/Steel_Undefined" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          50 x IFCBEAM | type IFCBEAMTYPE "50*10" | object type "50*10" | names: "TPA-FS_2,5TONN", "TPA-FA_2,5TONN", "TPA-FS_5,0TONN" (+4 more) | descriptions: "50*10" | material: "STEEL/S355J0" | property sets: Tekla Quantity, Pset_BeamCommon, Tekla Common, BaseQuantities
          24 x IFCBEAM | type IFCBEAMTYPE "RHS100*50*6" | object type "RHS100*50*6" | names: "BEAM" | descriptions: "RHS100*50*6" | material: "Undefined/Steel_Undefined" | property sets: Tekla Quantity, Pset_BeamCommon, Tekla Common, BaseQuantities
          48 x IFCBEAM | type IFCBEAMTYPE "D30" | object type "D30" | names: "BEAM" | descriptions: "D30" | material: "Undefined/Steel_Undefined" | property sets: Tekla Quantity, Pset_BeamCommon, Tekla Common, BaseQuantities
          24 x IFCPLATE | type IFCPLATETYPE "4*80" | object type "4*80" | names: "BEAM" | descriptions: "4*80" | material: "Undefined/Steel_Undefined" | property sets: Tekla Quantity, Pset_PlateCommon, Tekla Common, BaseQuantities
          1 x IFCFOOTING | object type "2300*3000" | names: "Heisgrube" | descriptions: "2300*3000" | material: "CONCRETE/B35" | property sets: Tekla Common, Tekla Quantity, BaseQuantities
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "1220*300" | object type "1220*300" | names: "Heisgrube" | descriptions: "1220*300" | material: layers "Wall: Insitu CONCRETE/B35" ("CONCRETE/B35" 300.) | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          1 x IFCWALL | type IFCWALLTYPE "4000*300" | object type "4000*300" | names: "INNERVEGG" | descriptions: "4000*300" | material: "CONCRETE/B30" | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCWALL | type IFCWALLTYPE "2500*300" | object type "2500*300" | names: "INNERVEGG" | descriptions: "2500*300" | material: "CONCRETE/B30" | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCWALL | type IFCWALLTYPE "10000*20" | object type "10000*20" | names: "Ant-berg" | descriptions: "10000*20" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCWALL | type IFCWALLTYPE "2200*50" | object type "2200*50" | names: "X-Fjellskjæring" | descriptions: "2200*50" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          3 x IFCWALL | type IFCWALLTYPE "6200*50" | object type "6200*50" | names: "X-Fjellskjæring" | descriptions: "6200*50" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Pset_WallCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCPLATE | type IFCPLATETYPE "20*5364" | object type "20*5364" | names: "BETONGDEKKE" | descriptions: "20*5364" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Pset_PlateCommon, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "DLB600*1000-900*350-450" | object type "DLB600*1000-900*350-450" | names: "BETONGBJELKE" | descriptions: "DLB600*1000-900*350-450" | material: "CONCRETE/B45" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "DLB600*520-900*200" | object type "DLB600*520-900*200" | names: "BETONGBJELKE" | descriptions: "DLB600*520-900*200" | material: "CONCRETE/B45-SKB" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          1 x IFCWALL | type IFCWALLTYPE "5500*50" | object type "5500*50" | names: "X-Fjellskjæring" | descriptions: "5500*50" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          1 x IFCWALL | type IFCWALLTYPE "7500*50" | object type "7500*50" | names: "X-Fjellskjæring" | descriptions: "7500*50" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "4070*250" | object type "4070*250" | names: "BETONGVEGG" | descriptions: "4070*250" | material: layers "Wall: Insitu CONCRETE/B30" ("CONCRETE/B30" 250.) | property sets: Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          1 x IFCPLATE | type IFCPLATETYPE "50*10401" | object type "50*10401" | names: "BETONGDEKKE" | descriptions: "50*10401" | material: "MISCELLANEOUS/NULLVEKT" | property sets: Tekla Common, Tekla Quantity, Pset_PlateCommon, BaseQuantities
          2 x IFCCOLUMN | type IFCCOLUMNTYPE "CFRHS100X8" | object type "CFRHS100X8" | names: "STÅLSØYLE" | descriptions: "CFRHS100X8" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity, Pset_ColumnCommon, BaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "L100*10" | object type "L100*10" | names: "Stålvinnkel" | descriptions: "L100*10" | material: "STEEL/S355J0" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities

Types
  IFCWALLTYPE "3000*200" | 85 occurrences
  IFCWALLTYPE "3000*220" | 57 occurrences
  IFCSLABTYPE "250*2202" | 3 occurrences
  IFCSLABTYPE "250*2160" | 23 occurrences
  IFCCOLUMNTYPE "RHS200*100*16" | 81 occurrences
  IFCCOLUMNTYPE "CFRHS200X100X12.5" | 316 occurrences
  IFCBEAMTYPE "UPE270" | 53 occurrences
  IFCBEAMTYPE "HD320" | 169 occurrences
  IFCSLABTYPE "220*2100" | 2 occurrences
  IFCSLABTYPE "250*12420" | 3 occurrences
  IFCBEAMTYPE "D20-400" | 27 occurrences
  IFCSLABTYPE "120*2065" | 3 occurrences
  IFCSLABTYPE "120*1817" | 12 occurrences
  IFCSLABTYPE "120*1780" | 10 occurrences
  IFCSLABTYPE "120*1700" | 3 occurrences
  IFCWALLTYPE "250*200" | 26 occurrences
  IFCSLABTYPE "270*21040" | 1 occurrence
  IFCCOLUMNTYPE "RHS200*100*12.5" | 35 occurrences
  IFCSLABTYPE "270*2170" | 30 occurrences
  IFCSLABTYPE "270*2280" | 4 occurrences
  IFCBEAMTYPE "IPE240" | 39 occurrences
  IFCWALLTYPE "3000*250" | 108 occurrences
  IFCWALLTYPE "3000*300" | 2 occurrences
  IFCWALLTYPE "1220*300" | 11 occurrences
  IFCPLATETYPE "10*62145" | 1 occurrence
  IFCPLATETYPE "10*2000" | 2 occurrences
  IFCPLATETYPE "10*11327" | 1 occurrence
  IFCPLATETYPE "10*1999" | 1 occurrence
  IFCBEAMTYPE "D75" | 61 occurrences
  IFCCOLUMNTYPE "D5" | 21 occurrences
  IFCWALLTYPE "1220*250" | 1 occurrence
  IFCWALLTYPE "3050*220" | 2 occurrences
  IFCWALLTYPE "3050*200" | 4 occurrences
  IFCWALLTYPE "3350*300" | 4 occurrences
  IFCWALLTYPE "2955*220" | 3 occurrences
  IFCSLABTYPE "250*2180" | 2 occurrences
  IFCWALLTYPE "3350*220" | 4 occurrences
  IFCCOLUMNTYPE "HEA140" | 18 occurrences
  IFCMEMBERTYPE "D25" | 4 occurrences
  IFCBEAMTYPE "D12" | 9 occurrences
  IFCWALLTYPE "1300*100" | 5 occurrences
  IFCWALLTYPE "1400*100" | 1 occurrence
  IFCWALLTYPE "1660*100" | 1 occurrence
  IFCWALLTYPE "1600*100" | 1 occurrence
  IFCBEAMTYPE "PL15*300" | 18 occurrences
  IFCWALLTYPE "2950*500" | 3 occurrences
  IFCWALLTYPE "3150*500" | 3 occurrences
  IFCSLABTYPE "1080*1333" | 1 occurrence
  IFCWALLTYPE "250*250" | 2 occurrences
  IFCWALLTYPE "6200*220" | 1 occurrence
  IFCSLABTYPE "250*12400" | 3 occurrences
  IFCCOLUMNTYPE "RHS88.9X7.1" | 4 occurrences
  IFCSLABTYPE "120*2234" | 2 occurrences
  IFCSLABTYPE "120*2136" | 2 occurrences
  IFCPLATETYPE "PL25*250" | 2 occurrences
  IFCPLATETYPE "PL15*250" | 2 occurrences
  IFCBEAMTYPE "D32" | 8 occurrences
  IFCPLATETYPE "PL25*150" | 8 occurrences
  IFCBEAMTYPE "D16" | 62 occurrences
  IFCWALLTYPE "6450*300" | 2 occurrences
  IFCCOLUMNTYPE "400*600" | 2 occurrences
  IFCCOLUMNTYPE "D750" | 1 occurrence
  IFCSLABTYPE "220*2550" | 1 occurrence
  IFCSLABTYPE "220*2440" | 1 occurrence
  IFCCOLUMNTYPE "600*600" | 5 occurrences
  IFCCOLUMNTYPE "300*500" | 2 occurrences
  IFCCOLUMNTYPE "200*600" | 2 occurrences
  IFCMEMBERTYPE "CFRHS250X150X12.5" | 2 occurrences
  IFCCOLUMNTYPE "CFRHS80X8" | 18 occurrences
  IFCWALLTYPE "3350*250" | 6 occurrences
  IFCWALLTYPE "3350*200" | 2 occurrences
  IFCWALLTYPE "3550*300" | 1 occurrence
  IFCSLABTYPE "270*15080" | 1 occurrence
  IFCCOLUMNTYPE "CFRHS200X100X8" | 16 occurrences
  IFCSLABTYPE "270*1987" | 8 occurrences
  IFCBEAMTYPE "370*150" | 5 occurrences
  IFCBEAMTYPE "L200*14" | 7 occurrences
  IFCMEMBERTYPE "CFRHS80X6" | 37 occurrences
  IFCBEAMTYPE "IPE300" | 13 occurrences
  IFCWALLTYPE "2730*250" | 1 occurrence
  IFCSLABTYPE "270*20150" | 13 occurrences
  IFCSLABTYPE "270*2100" | 12 occurrences
  IFCWALLTYPE "3650*220" | 4 occurrences
  IFCWALLTYPE "3650*200" | 4 occurrences
  IFCCOLUMNTYPE "CFRHS100X8" | 13 occurrences
  IFCWALLTYPE "2730*200" | 1 occurrence
  IFCSLABTYPE "250*2120" | 2 occurrences
  IFCPLATETYPE "200*12401" | 1 occurrence
  IFCBEAMTYPE "HSQ250*8-30*150-10*450" | 9 occurrences
  IFCBEAMTYPE "CFRHS250X150X12.5" | 2 occurrences
  IFCBEAMTYPE "L100*10" | 28 occurrences
  IFCCOLUMNTYPE "CFRHS200X100X10" | 8 occurrences
  IFCBEAMTYPE "D20-300" | 2 occurrences
  IFCCOLUMNTYPE "CFRHS200*100*12" | 1 occurrence
  IFCWALLTYPE "3000*400" | 1 occurrence
  IFCSLABTYPE "220*2350" | 1 occurrence
  IFCSLABTYPE "270*2101" | 1 occurrence
  IFCWALLTYPE "3400*200" | 9 occurrences
  IFCWALLTYPE "3400*220" | 8 occurrences
  IFCCOLUMNTYPE "CFRHS200X100X6" | 8 occurrences
  IFCSLABTYPE "250*5490" | 1 occurrence
  IFCSLABTYPE "250*5600" | 1 occurrence
  IFCPLATETYPE "198*1500" | 1 occurrence
  IFCSLABTYPE "250*1400" | 1 occurrence
  IFCPLATETYPE "200*13020" | 1 occurrence
  IFCBEAMTYPE "CFRHS80X6" | 1 occurrence
  IFCBEAMTYPE "DR26-260" | 1 occurrence
  IFCWALLTYPE "3200*250" | 4 occurrences
  IFCWALLTYPE "3200*220" | 1 occurrence
  IFCWALLTYPE "4450*200" | 2 occurrences
  IFCWALLTYPE "4450*250" | 2 occurrences
  IFCSLABTYPE "270*17750" | 1 occurrence
  IFCWALLTYPE "3070*250" | 5 occurrences
  IFCWALLTYPE "3120*220" | 4 occurrences
  IFCBEAMTYPE "LB500*520-650*200" | 1 occurrence
  IFCWALLTYPE "2820*250" | 1 occurrence
  IFCCOLUMNTYPE "900*400" | 22 occurrences
  IFCCOLUMNTYPE "600*350" | 5 occurrences
  IFCCOLUMNTYPE "400*400" | 12 occurrences
  IFCSLABTYPE "265*2159" | 2 occurrences
  IFCBEAMTYPE "DLB600*520-900*200" | 6 occurrences
  IFCWALLTYPE "5500*50" | 2 occurrences
  IFCCOLUMNTYPE "600*400" | 1 occurrence
  IFCBEAMTYPE "50*10" | 172 occurrences
  IFCBEAMTYPE "D50" | 63 occurrences
  IFCWALLTYPE "5000*300" | 1 occurrence
  IFCWALLTYPE "3070*300" | 2 occurrences
  IFCBEAMTYPE "15*170" | 1 occurrence
  IFCCOLUMNTYPE "D20" | 87 occurrences
  IFCBEAMTYPE "25*380" | 1 occurrence
  IFCBEAMTYPE "D20" | 112 occurrences
  IFCBEAMTYPE "25*330" | 3 occurrences
  IFCBEAMTYPE "25*580" | 1 occurrence
  IFCBEAMTYPE "L150*12" | 17 occurrences
  IFCSLABTYPE "1100*1323" | 2 occurrences
  IFCSLABTYPE "1110*375" | 4 occurrences
  IFCBEAMTYPE "D100" | 5 occurrences
  IFCBEAMTYPE "8*100" | 6 occurrences
  IFCCOLUMNTYPE "D24" | 20 occurrences
  IFCCOLUMNTYPE "80*80" | 14 occurrences
  IFCCOLUMNTYPE "HALFEN_NUT-M24" | 20 occurrences
  IFCCOLUMNTYPE "860*360" | 12 occurrences
  IFCCOLUMNTYPE "80*70" | 6 occurrences
  IFCPLATETYPE "PL20*235" | 2 occurrences
  IFCSLABTYPE "1100*1219" | 2 occurrences
  IFCBEAMTYPE "RHS120*80*5" | 48 occurrences
  IFCBEAMTYPE "RHS100*50*6" | 48 occurrences
  IFCBEAMTYPE "D30" | 96 occurrences
  IFCPLATETYPE "4*80" | 48 occurrences
  IFCBEAMTYPE "PRMDAS120*200-110*160-5*0" | 48 occurrences
  IFCSLABTYPE "265*1310" | 4 occurrences
  IFCCOLUMNTYPE "D30" | 11 occurrences
  IFCBEAMTYPE "20*215" | 2 occurrences
  IFCBEAMTYPE "20*210" | 2 occurrences
  IFCBEAMTYPE "D10" | 20 occurrences
  IFCBEAMTYPE "10*80" | 72 occurrences
  IFCBEAMTYPE "10*160" | 4 occurrences
  IFCCOLUMNTYPE "950*500" | 5 occurrences
  IFCBEAMTYPE "DLB500*520-800*200" | 3 occurrences
  IFCCOLUMNTYPE "1700*400" | 2 occurrences
  IFCCOLUMNTYPE "1100*600" | 1 occurrence
  IFCCOLUMNTYPE "300*300" | 1 occurrence
  IFCCOLUMNTYPE "300*550" | 2 occurrences
  IFCCOLUMNTYPE "600*550" | 1 occurrence
  IFCWALLTYPE "4150*250" | 1 occurrence
  IFCWALLTYPE "3100*250" | 5 occurrences
  IFCWALLTYPE "3100*300" | 7 occurrences
  IFCWALLTYPE "3100*200" | 5 occurrences
  IFCWALLTYPE "3120*300" | 1 occurrence
  IFCWALLTYPE "3100*220" | 2 occurrences
  IFCWALLTYPE "2950*250" | 7 occurrences
  IFCBEAMTYPE "DLB600*900-1000*250-350" | 4 occurrences
  IFCWALLTYPE "3495*220" | 8 occurrences
  IFCBEAMTYPE "LB500*750-700*250" | 1 occurrence
  IFCWALLTYPE "2850*250" | 1 occurrence
  IFCBEAMTYPE "HD500" | 106 occurrences
  IFCWALLTYPE "3495*200" | 4 occurrences
  IFCBEAMTYPE "HD400" | 32 occurrences
  IFCSLABTYPE "100*12420" | 1 occurrence
  IFCBEAMTYPE "DLB600*850-1000*250" | 1 occurrence
  IFCBEAMTYPE "DLB600*1000-900*350-450" | 2 occurrences
  IFCBEAMTYPE "400*1200" | 2 occurrences
  IFCBEAMTYPE "400*700" | 2 occurrences
  IFCWALLTYPE "5000*200" | 1 occurrence
  IFCSLABTYPE "250*2000" | 2 occurrences
  IFCWALLTYPE "650*250" | 1 occurrence
  IFCWALLTYPE "850*250" | 1 occurrence
  IFCCOLUMNTYPE "D50" | 6 occurrences
  IFCWALLTYPE "950*250" | 6 occurrences
  IFCBEAMTYPE "PL10*80" | 5 occurrences
  IFCBEAMTYPE "50*80" | 4 occurrences
  IFCSLABTYPE "1100*897" | 2 occurrences
  IFCBEAMTYPE "D60" | 13 occurrences
  IFCBEAMTYPE "D24" | 73 occurrences
  IFCBEAMTYPE "NUT_M24" | 288 occurrences
  IFCBEAMTYPE "15*450" | 1 occurrence
  IFCCOLUMNTYPE "D25" | 6 occurrences
  IFCBEAMTYPE "L150*14" | 10 occurrences
  IFCBEAMTYPE "15*250" | 1 occurrence
  IFCWALLTYPE "680*200" | 1 occurrence
  IFCBEAMTYPE "400*645" | 2 occurrences
  IFCBEAMTYPE "PL20*150" | 2 occurrences
  IFCBEAMTYPE "PL25*200" | 2 occurrences
  IFCCOLUMNTYPE "600*300" | 1 occurrence
  IFCSLABTYPE "1100*1490" | 2 occurrences
  IFCSLABTYPE "265*2291" | 2 occurrences
  IFCPLATETYPE "PL20*424" | 1 occurrence
  IFCWALLTYPE "3545*250" | 3 occurrences
  IFCBEAMTYPE "PL40*1000" | 2 occurrences
  IFCCOLUMNTYPE "D75" | 6 occurrences
  IFCBEAMTYPE "15*200" | 4 occurrences
  IFCBEAMTYPE "20*410" | 1 occurrence
  IFCBEAMTYPE "PL40*550" | 4 occurrences
  IFCPLATETYPE "PL25*240" | 1 occurrence
  IFCCOLUMNTYPE "CFRHS200*100*12.5" | 1 occurrence
  IFCBEAMTYPE "PL20*130" | 1 occurrence
  IFCBEAMTYPE "DLB500*700-800*200" | 3 occurrences
  IFCWALLTYPE "2250*300" | 1 occurrence
  IFCBEAMTYPE "610*150" | 12 occurrences
  IFCBEAMTYPE "L200*16" | 13 occurrences
  IFCCOLUMNTYPE "800*400" | 2 occurrences
  IFCBEAMTYPE "20*200" | 1 occurrence
  IFCCOLUMNTYPE "500*500" | 21 occurrences
  IFCWALLTYPE "3150*200" | 1 occurrence
  IFCWALLTYPE "1220*200" | 1 occurrence
  IFCSLABTYPE "270*5680" | 2 occurrences
  IFCPLATETYPE "120*1592" | 6 occurrences
  IFCPLATETYPE "120*2016" | 3 occurrences
  IFCPLATETYPE "120*1566" | 3 occurrences
  IFCPLATETYPE "120*1924" | 3 occurrences
  IFCPLATETYPE "120*1575" | 3 occurrences
  IFCPLATETYPE "120*1875" | 1 occurrence
  IFCPLATETYPE "120*1650" | 1 occurrence
  IFCPLATETYPE "120*1999" | 1 occurrence
  IFCPLATETYPE "120*1200" | 1 occurrence
  IFCPLATETYPE "120*1574" | 1 occurrence
  IFCPLATETYPE "120*1595" | 1 occurrence
  IFCPLATETYPE "120*1047" | 1 occurrence
  IFCPLATETYPE "120*2281" | 1 occurrence
  IFCPLATETYPE "120*1612" | 1 occurrence
  IFCPLATETYPE "120*1470" | 1 occurrence
  IFCSLABTYPE "120*1592" | 2 occurrences
  IFCSLABTYPE "120*2179" | 1 occurrence
  IFCSLABTYPE "120*2129" | 1 occurrence
  IFCPLATETYPE "120*1865" | 2 occurrences
  IFCPLATETYPE "120*1321" | 1 occurrence
  IFCWALLTYPE "3400*250" | 1 occurrence
  IFCWALLTYPE "200*200" | 2 occurrences
  IFCSLABTYPE "320*790" | 2 occurrences
  IFCWALLTYPE "3050*300" | 1 occurrence
  IFCPLATETYPE "50*24400" | 2 occurrences
  IFCSLABTYPE "100*5342" | 1 occurrence
  IFCSLABTYPE "100*3250" | 1 occurrence
  IFCSLABTYPE "100*8100" | 1 occurrence
  IFCSLABTYPE "100*10970" | 1 occurrence
  IFCSLABTYPE "100*5180" | 1 occurrence
  IFCSLABTYPE "100*9590" | 1 occurrence
  IFCSLABTYPE "50*9022" | 1 occurrence
  IFCSLABTYPE "50*9590" | 1 occurrence
  IFCSLABTYPE "50*5342" | 1 occurrence
  IFCWALLTYPE "3500*400" | 1 occurrence
  IFCPLATETYPE "PL25*200" | 1 occurrence
  IFCPLATETYPE "120*1192" | 1 occurrence
  IFCPLATETYPE "120*2314" | 1 occurrence
  IFCCOLUMNTYPE "CFRHS100X10" | 3 occurrences
  IFCSLABTYPE "250*5680" | 1 occurrence
  IFCWALLTYPE "1000*250" | 1 occurrence
  IFCSLABTYPE "250*3100" | 1 occurrence
  IFCSLABTYPE "80*9590" | 1 occurrence
  IFCSLABTYPE "80*6971" | 1 occurrence
  IFCSLABTYPE "80*2282" | 1 occurrence
  IFCBEAMTYPE "750*150" | 9 occurrences
  IFCWALLTYPE "3150*250" | 1 occurrence
  IFCBEAMTYPE "400*150" | 4 occurrences
  IFCWALLTYPE "4000*300" | 1 occurrence
  IFCWALLTYPE "2500*300" | 2 occurrences
  IFCWALLTYPE "10000*20" | 1 occurrence
  IFCWALLTYPE "2200*50" | 1 occurrence
  IFCWALLTYPE "6200*50" | 3 occurrences
  IFCPLATETYPE "20*5364" | 1 occurrence
  IFCWALLTYPE "7500*50" | 1 occurrence
  IFCWALLTYPE "4070*250" | 1 occurrence
  IFCPLATETYPE "50*10401" | 1 occurrence

Property sets
  Tekla Common | properties | on 148 objects (148 IFCBEAM)
    Bottom elevation = "+10.550" (IFCLABEL)
    Class = "272" (IFCLABEL)
    Finish = "" (IFCLABEL)
    Initial GUID (no value)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+10.870" (IFCLABEL)
  Tekla Common | properties | on 60 objects (60 IFCBEAM)
    Bottom elevation = "+13.772" (IFCLABEL)
    Class = "146" (IFCLABEL)
    Finish = "" (IFCLABEL)
    Initial GUID (no value)
    Phase = 12 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+13.793" (IFCLABEL)
  Tekla Common | properties | on 60 objects (60 IFCBEAM)
    Bottom elevation = "+13.672" (IFCLABEL)
    Class = "146" (IFCLABEL)
    Finish = "" (IFCLABEL)
    Initial GUID (no value)
    Phase = 12 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+13.693" (IFCLABEL)
  Tekla Common | properties | on 60 objects (60 IFCBEAM)
    Bottom elevation = "+13.572" (IFCLABEL)
    Class = "146" (IFCLABEL)
    Finish = "" (IFCLABEL)
    Initial GUID (no value)
    Phase = 12 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+13.593" (IFCLABEL)
  Tekla Common | properties | on 60 objects (60 IFCBEAM)
    Bottom elevation = "+14.515" (IFCLABEL)
    Class = "146" (IFCLABEL)
    Finish = "" (IFCLABEL)
    Initial GUID (no value)
    Phase = 12 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+14.537" (IFCLABEL)
  Tekla Common | properties | on 60 objects (60 IFCBEAM)
    Bottom elevation = "+13.550" (IFCLABEL)
    Class = "146" (IFCLABEL)
    Finish = "" (IFCLABEL)
    Initial GUID (no value)
    Phase = 12 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+14.550" (IFCLABEL)
  Tekla Common | properties | on 54 objects (54 IFCBEAM)
    Bottom elevation = "+13.745" (IFCLABEL)
    Class = "101" (IFCLABEL)
    Finish = "" (IFCLABEL)
    Initial GUID (no value)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+13.995" (IFCLABEL)
  Tekla Common | properties | on 48 objects (48 IFCBEAM)
    Bottom elevation = "+7.400" (IFCLABEL)
    Class = "100" (IFCLABEL)
    Finish = "" (IFCLABEL)
    Initial GUID (no value)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+7.800" (IFCLABEL)
  Tekla Common: 709 more contents on 3000 objects not shown
  Tekla Quantity | properties | on 304 objects (304 IFCCOLUMN)
    Area per tons = 10.8 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 3000. (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 1.8 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 161.9 (IFCMASSMEASURE) [KILO GRAM]
    Width = 100. (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 288 objects (288 IFCBEAM)
    Area per tons = 25.9 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 36. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 21.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 0.2 (IFCMASSMEASURE) [KILO GRAM]
    Width = 41.6 (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 172 objects (172 IFCBEAM)
    Area per tons = 31.8 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 0.8 (IFCMASSMEASURE) [KILO GRAM]
    Width = 10. (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 96 objects (96 IFCBEAM)
    Area per tons = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 30. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 90. (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 0. (IFCMASSMEASURE) [KILO GRAM]
    Width = 30. (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 76 objects (56 IFCBEAM, 20 IFCCOLUMN)
    Area per tons = 28.6 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 20. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 0.6 (IFCMASSMEASURE) [KILO GRAM]
    Width = 20. (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 73 objects (73 IFCCOLUMN)
    Area per tons = 8.4 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 3000. (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 1.8 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 199. (IFCMASSMEASURE) [KILO GRAM]
    Width = 100. (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 72 objects (72 IFCBEAM)
    Area per tons = 30.8 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 10. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 120. (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 0.8 (IFCMASSMEASURE) [KILO GRAM]
    Width = 80. (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 70 objects (70 IFCBEAM)
    Area per tons = 22.3 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 24. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 0.1 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 3.4 (IFCMASSMEASURE) [KILO GRAM]
    Width = 24. (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity: 731 more contents on 2399 objects not shown
  Pset_WallCommon | properties | on 217 objects (158 IFCWALLSTANDARDCASE, 59 IFCWALL)
    AcousticRating (no value)
    Compartmentation = FALSE (IFCBOOLEAN)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "P0(?)" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 17 objects (9 IFCWALLSTANDARDCASE, 8 IFCWALL)
    AcousticRating (no value)
    Compartmentation = FALSE (IFCBOOLEAN)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "CP_BV-1138(?)" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 15 objects (13 IFCWALLSTANDARDCASE, 2 IFCWALL)
    AcousticRating (no value)
    Compartmentation = FALSE (IFCBOOLEAN)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "CP_BV-1182(?)" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 12 objects (12 IFCWALLSTANDARDCASE)
    AcousticRating (no value)
    Compartmentation = FALSE (IFCBOOLEAN)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "CP_BV-1137(?)" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 12 objects (11 IFCWALL, 1 IFCWALLSTANDARDCASE)
    AcousticRating (no value)
    Compartmentation = FALSE (IFCBOOLEAN)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "CP_BV-1145(?)" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 10 objects (10 IFCWALL)
    AcousticRating (no value)
    Compartmentation = FALSE (IFCBOOLEAN)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "CP_BV-1152(?)" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 9 objects (9 IFCWALL)
    AcousticRating (no value)
    Compartmentation = FALSE (IFCBOOLEAN)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "CP_BV-10(?)" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 8 objects (7 IFCWALL, 1 IFCWALLSTANDARDCASE)
    AcousticRating (no value)
    Compartmentation = FALSE (IFCBOOLEAN)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "CP_BV-1141(?)" (IFCIDENTIFIER)
  Pset_WallCommon: 105 more contents on 161 objects not shown
  BaseQuantities | quantities | on 38 objects (38 IFCBEAM)
    Length = 21.50000000008 [MILLI METRE]
    NetVolume = 2.41309318505445E-05 [CUBIC_METRE]
    NetWeight = 0.189427815026775 [KILO GRAM]
    OuterSurfaceArea = 0.00492595249664748 [SQUARE_METRE]
  BaseQuantities | quantities | on 28 objects (28 IFCBEAM)
    Length = 21.50000000008 [MILLI METRE]
    NetVolume = 2.41309318505543E-05 [CUBIC_METRE]
    NetWeight = 0.189427815026851 [KILO GRAM]
    OuterSurfaceArea = 0.00492595249664893 [SQUARE_METRE]
  BaseQuantities | quantities | on 22 objects (22 IFCBEAM)
    Length = 21.50000000008 [MILLI METRE]
    NetVolume = 2.41309318505389E-05 [CUBIC_METRE]
    NetWeight = 0.18942781502673 [KILO GRAM]
    OuterSurfaceArea = 0.00492595249664664 [SQUARE_METRE]
  BaseQuantities | quantities | on 21 objects (21 IFCCOLUMN)
    Length = 2000. [MILLI METRE]
    NetVolume = 0.5 [CUBIC_METRE]
    NetWeight = 0. [KILO GRAM]
    OuterSurfaceArea = 4.5 [SQUARE_METRE]
  BaseQuantities | quantities | on 19 objects (19 IFCBEAM)
    Length = 21.50000000008 [MILLI METRE]
    NetVolume = 2.41309318505551E-05 [CUBIC_METRE]
    NetWeight = 0.189427815026857 [KILO GRAM]
    OuterSurfaceArea = 0.00492595249664904 [SQUARE_METRE]
  BaseQuantities | quantities | on 19 objects (19 IFCBEAM)
    Length = 21.50000000008 [MILLI METRE]
    NetVolume = 2.41309318505487E-05 [CUBIC_METRE]
    NetWeight = 0.189427815026807 [KILO GRAM]
    OuterSurfaceArea = 0.00492595249664809 [SQUARE_METRE]
  BaseQuantities | quantities | on 18 objects (18 IFCBEAM)
    Length = 21.50000000008 [MILLI METRE]
    NetVolume = 2.41309318505502E-05 [CUBIC_METRE]
    NetWeight = 0.189427815026819 [KILO GRAM]
    OuterSurfaceArea = 0.00492595249664832 [SQUARE_METRE]
  BaseQuantities | quantities | on 17 objects (17 IFCBEAM)
    Length = 21.50000000008 [MILLI METRE]
    NetVolume = 2.41309318505494E-05 [CUBIC_METRE]
    NetWeight = 0.189427815026813 [KILO GRAM]
    OuterSurfaceArea = 0.00492595249664821 [SQUARE_METRE]
  BaseQuantities: 2729 more contents on 3368 objects not shown
  Pset_BeamCommon | properties | on 360 objects (360 IFCBEAM)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "EXL0(?)" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 141 objects (141 IFCBEAM)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "sb0(?)" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 101 objects (101 IFCBEAM)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "CP_PB-1125(?)" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 56 objects (56 IFCBEAM)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "b1" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 48 objects (48 IFCBEAM)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "P20(?)" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 48 objects (48 IFCBEAM)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "P20" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 48 objects (48 IFCBEAM)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "b7" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 38 objects (38 IFCBEAM)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Concrete_B-11" (IFCIDENTIFIER)
  Pset_BeamCommon: 200 more contents on 1010 objects not shown
  Pset_ColumnCommon | properties | on 509 objects (509 IFCCOLUMN)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "ss0(?)" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 35 objects (35 IFCCOLUMN)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "CP_C-10(?)" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 31 objects (31 IFCCOLUMN)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "P0(?)" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 20 objects (20 IFCCOLUMN)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "sb30" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 20 objects (20 IFCCOLUMN)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "b1" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 16 objects (16 IFCCOLUMN)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "b12" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 15 objects (15 IFCCOLUMN)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "DJB102" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 14 objects (14 IFCCOLUMN)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "dsb2" (IFCIDENTIFIER)
  Pset_ColumnCommon: 34 more contents on 159 objects not shown
  Pset_PlateCommon | properties | on 24 objects (24 IFCPLATE)
    AcousticRating (no value)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "P21(?)" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 24 objects (24 IFCPLATE)
    AcousticRating (no value)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "P21" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 18 objects (18 IFCPLATE)
    AcousticRating (no value)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "CP_BD-137(?)" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 15 objects (15 IFCPLATE)
    AcousticRating (no value)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "CP_BD-136(?)" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 7 objects (7 IFCPLATE)
    AcousticRating (no value)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "DSP0(?)" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 4 objects (4 IFCPLATE)
    AcousticRating (no value)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "CP_BD-10(?)" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 3 objects (3 IFCPLATE)
    AcousticRating (no value)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "CP_PS-10(?)" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 2 objects (2 IFCPLATE)
    AcousticRating (no value)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "STL203(?)" (IFCIDENTIFIER)
  Pset_PlateCommon: 10 more contents on 13 objects not shown
  Pset_SlabCommon | properties | on 77 objects (77 IFCSLAB)
    AcousticRating (no value)
    Compartmentation = FALSE (IFCBOOLEAN)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "CP_BD-171(?)" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 58 objects (58 IFCSLAB)
    AcousticRating (no value)
    Compartmentation = FALSE (IFCBOOLEAN)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "CP_BD-10(?)" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 12 objects (12 IFCSLAB)
    AcousticRating (no value)
    Compartmentation = FALSE (IFCBOOLEAN)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "CP_PS-10(?)" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 10 objects (10 IFCSLAB)
    AcousticRating (no value)
    Compartmentation = FALSE (IFCBOOLEAN)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "CP_BD-169(?)" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 9 objects (9 IFCSLAB)
    AcousticRating (no value)
    Compartmentation = FALSE (IFCBOOLEAN)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "CP_GPG-10(?)" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    AcousticRating (no value)
    Compartmentation = FALSE (IFCBOOLEAN)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "CP_ -42012(?)" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    AcousticRating (no value)
    Compartmentation = FALSE (IFCBOOLEAN)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "CP_BD-172(?)" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    AcousticRating (no value)
    Compartmentation = FALSE (IFCBOOLEAN)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "CP_ -42012" (IFCIDENTIFIER)
  Pset_SlabCommon: 20 more contents on 21 objects not shown
  Pset_MemberCommon | properties | on 39 objects (39 IFCMEMBER)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "sb0(?)" (IFCIDENTIFIER)
  Pset_MemberCommon | properties | on 4 objects (4 IFCMEMBER)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "ss0(?)" (IFCIDENTIFIER)