IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0, QuantityTakeOffAddOnView, SpaceBoundary2ndLevelAddOnView]"
Description: "Option [Elements to export: Visible elements (on all stories)]"
Description: "Option [Partial Structure Display: Entire Model]"
Description: "Option [IFC Domain: All]"
Description: "Option [Structural Function: All Elements]"
Description: "Option [Convert Grid elements: On]"
Description: "Option [Convert IFC Annotations and Archicad 2D elements: Off]"
Description: "Option [Convert 2D symbols of Doors and Windows: On]"
Description: "Option [Export geometries that Participates in Collision Detection only: Off]"
Description: "Option [Split complex elements: Off]"
Description: "Option [Material Preservation: Explode where necessary]"
Description: "Option [Elements in Solid Element Operations: Extruded/revolved]"
Description: "Option [Elements with junctions: Extruded/revolved without junctions]"
Description: "Option [IFC Model position: Project Origin only]"
Description: "Option [Curtain Wall export mode: Container Element]"
Description: "Option [Railing export mode: Single Element]"
File name: "C:\Users\aamman\Arkama AS\ArkAma - General\01 KUNDER\2023\2326 Bjørnstad entreprenørpark - rehabilitering\03 PRO\02 Dokumentasjon\03 Tegninger\03-01 Digital Tegningsutsendelse\02 IFC\2326 Bjørnstad entreprenørpark ARK.ifc"
Time stamp: "2024-05-07T10:13:56"
Author: "Arkitekten"
Organization: "Ark Ama AS"
Preprocessor: "DDS_IFC v3.0"
Originating system: "IFC file generated by Graphisoft Archicad 27.0.0 NOR FULL Windows version (IFC add-on version: 3001 NOR FULL)."
Authorization: "Arkitekten"
Application: "Archicad" version "27.0.0" identifier "IFC add-on version: 3001 NOR FULL" by Organization "Graphisoft" id "GS" description "Graphisoft"

People and organizations
  Person "Arkitekten" (roles: "Ark:"; postal address "Architect Postal Address": "Ordfører Voldens vei 9", "Mysen", "1850"; telecom address "Architect Telecom Address": telephone "+47 906 02 589"; e-mail "ma@arkama.no"; web page "www.arkama.no") of Organization "Ark Ama AS" id "982 534 860 MVA" (postal address "Architect Postal Address": "Ordfører Voldens vei 9", "Mysen", "1850"; telecom address "Architect Telecom Address": telephone "+47 906 02 589"; e-mail "ma@arkama.no"; web page "www.arkama.no")
  Owner history of Person "Arkitekten" (roles: "Ark:"; postal address "Architect Postal Address": "Ordfører Voldens vei 9", "Mysen", "1850"; telecom address "Architect Telecom Address": telephone "+47 906 02 589"; e-mail "ma@arkama.no"; web page "www.arkama.no") of Organization "Ark Ama AS" id "982 534 860 MVA" (postal address "Architect Postal Address": "Ordfører Voldens vei 9", "Mysen", "1850"; telecom address "Architect Telecom Address": telephone "+47 906 02 589"; e-mail "ma@arkama.no"; web page "www.arkama.no") | application "Archicad" version "27.0.0" identifier "IFC add-on version: 3001 NOR FULL" by Organization "Graphisoft" id "GS" description "Graphisoft" | change NOCHANGE | created 1715069621 (2024-05-07T08:13:41Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  SOLIDANGLEUNIT: SQUAREDEGREE (conversion based)
  CURRENCY: NOK
  TIMEUNIT: Year (conversion based)
  MASSUNIT: KILO GRAM
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN
  ENERGYUNIT: MEGA JOULE
  THERMALCONDUCTANCEUNIT: derived
  SPECIFICHEATCAPACITYUNIT: derived
  MASSDENSITYUNIT: derived

Spatial structure
IFCPROJECT "Bjørnstad entreprenørpark" | phase "Arbeidstegning" | description "Prosjektbeskrivelse"
  IFCSITE "Eiendomsnavn" | latitude 59° 55′ 52.428″ | longitude 10° 42′ 27.972″ | elevation above sea level 0. | postal address: "Gamle Kongevei 101", "#", "Grålum", "1712", "Norge"
    IFCBUILDING "Bygningens navn" | long name "Byggnummer" | postal address: "Gamle Kongevei 101", "#", "Grålum", "1712", "Norge" | description "Bygningstype"
      IFCBUILDINGSTOREY "Kjeller" | elevation 950.
        contains 74 elements
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Betong 400" | names: "YVT-" | material: layers "Betong 400" ("Betong" 400.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          5 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | property sets: Pset_DoorCommon, AC_Pset_RenovationAndPhasing, BaseQuantities, Pset_FireRatingProperties
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu" | object type "WINDOW" | property sets: Pset_FireRatingProperties, Pset_WindowCommon, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet asymmetrisk" | object type "DOOR" | names: "YD-7" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Betong 300" | names: "V-" | material: layers "Betong 300" ("Betong" 300.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          8 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Betong 200" | names: "V-" | material: layers "Betong 200" ("Betong" 200.) | property sets: Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | property sets: Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, Pset_DoorCommon
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Betong 150" | names: "V-" | material: layers "Betong 150" ("Betong" 150.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          3 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, BaseQuantities, AC_Pset_RenovationAndPhasing
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Betong 100" | names: "V-" | material: layers "Betong 100" ("Betong" 100.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | property sets: Pset_FireRatingProperties, Pset_DoorCommon, BaseQuantities, AC_Pset_RenovationAndPhasing
          7 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Betong 250" | names: "YVT-" | material: layers "Betong 250" ("Betong" 250.) | property sets: Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, Pset_WallCommon
          3 x IFCCOVERING | type IFCCOVERINGTYPE "Gulvbelegg 100" | CEILING | names: "H-" | material: "Gulvbelegg" | property sets: Pset_CoveringCommon, AC_Pset_Dimension, AC_Pset_RenovationAndPhasing, BaseQuantities, Pset_FireRatingProperties
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Betong - Strukturell 150" | names: "YVT-" | material: layers "Betong - Strukturell 150" ("Betong - Strukturell" 150.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, BaseQuantities, AC_Pset_RenovationAndPhasing
          2 x IFCSTAIR | names: "Trapp-" | parts: 6 IFCBUILDINGELEMENTPART | property sets: Pset_FireRatingProperties, Pset_StairCommon, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Betong 160" | names: "V-" | material: layers "Betong 160" ("Betong" 160.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Betong 220" | names: "V-" | material: layers "Betong 220" ("Betong" 220.) | property sets: Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, BaseQuantities, AC_Pset_RenovationAndPhasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Trestender 98 mm, isolert, 2x platekl. to sider 148" | names: "V-" | material: layers "Trestender 98 mm, isolert, 2x platekl. to sider" ("Platekledning - Vegg" 12.5, "Platekledning - Vegg" 12.5, "Stenderverk tre - Isolert" 98., "Platekledning - Vegg" 12.5, "Platekledning - Vegg" 12.5) | property sets: Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          7 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Isolasjon - Trykkfast 100" | names: "YVT-" | material: layers "Isolasjon - Trykkfast 100" ("Isolasjon - Trykkfast" 100.) | property sets: Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, Pset_WallCommon
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Isolasjon - Trykkfast 200" | names: "YVT-" | material: layers "Isolasjon - Trykkfast 200" ("Isolasjon - Trykkfast" 200.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet asymmetrisk" | object type "DOOR" | names: "D-" | property sets: Pset_FireRatingProperties, BaseQuantities, AC_Pset_RenovationAndPhasing, Pset_DoorCommon
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCGRID
      IFCBUILDINGSTOREY "1. etasje" | elevation 3650.
        contains 282 elements
          14 x IFCCOLUMN | type IFCCOLUMNTYPE "Betong 400 x 300" | object type "COLUMN" | names: "Søyle-" | material: "Betong" | property sets: Pset_ColumnCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          22 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Trestender 98 mm, isolert, 2x platekl. to sider 148" | names: "V-" | material: layers "Trestender 98 mm, isolert, 2x platekl. to sider" ("Platekledning - Vegg" 12.5, "Platekledning - Vegg" 12.5, "Stenderverk tre - Isolert" 98., "Platekledning - Vegg" 12.5, "Platekledning - Vegg" 12.5) | property sets: AC_Pset_RenovationAndPhasing, Pset_FireRatingProperties, Pset_WallCommon, BaseQuantities
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Innervegg 100" | names: "V-" | material: layers "Innervegg 100" ("Innervegg" 100.) | property sets: Pset_WallCommon, BaseQuantities, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "Skyvedør utenpåliggende" | object type "DOOR" | names: "D-3" | property sets: Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, Pset_DoorCommon, BaseQuantities
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Innervegg 200" | names: "V-" | material: layers "Innervegg 200" ("Innervegg" 200.) | property sets: Pset_WallCommon, AC_Pset_RenovationAndPhasing, BaseQuantities, Pset_FireRatingProperties
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          2 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "D-4" | property sets: Pset_DoorCommon, AC_Pset_RenovationAndPhasing, BaseQuantities, Pset_FireRatingProperties
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Innervegg 80" | names: "V-" | material: layers "Innervegg 80" ("Innervegg" 80.) | property sets: AC_Pset_RenovationAndPhasing, BaseQuantities, Pset_WallCommon, Pset_FireRatingProperties
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Trestender 98 mm stender 188" | names: "YVT-" | material: layers "Trestender 98 mm stender" ("Platekledning - Vegg" 18., "Lufting - Horisontalt" 23., "Lufting - Horisontalt" 36., "Vindsperre" 12.5, "Bindingsverk - Isolert" 98., "Dampsperre" 0.) | property sets: Pset_WallCommon, AC_Pset_RenovationAndPhasing, Pset_FireRatingProperties, BaseQuantities
          17 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu" | object type "WINDOW" | names: "V-", "V-2" | property sets: Pset_WindowCommon, Pset_FireRatingProperties, BaseQuantities, AC_Pset_RenovationAndPhasing
          40 x IFCWINDOW | type IFCWINDOWSTYLE "Pilaster" | object type "WINDOW" | names: "V-" | material: "Aluminium" | property sets: Pset_WindowCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          12 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu" | object type "WINDOW" | names: "V-2" | property sets: Pset_WindowCommon, AC_Pset_RenovationAndPhasing, Pset_FireRatingProperties, BaseQuantities
          1 x IFCWALL | type IFCWALLTYPE "Trestender 98 mm stender 188" | names: "YVT-" | parts: 5 IFCBUILDINGELEMENTPART | property sets: Pset_WallCommon, AC_Pset_RenovationAndPhasing, BaseQuantities, Pset_FireRatingProperties
          10 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu" | object type "WINDOW" | names: "V-2" | property sets: Pset_WindowCommon, Pset_FireRatingProperties, BaseQuantities, AC_Pset_RenovationAndPhasing
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Gulvbelegg 220" | CEILING | names: "H-" | material: "Gulvbelegg" | property sets: AC_Pset_Dimension, Pset_CoveringCommon, Pset_FireRatingProperties, BaseQuantities, AC_Pset_RenovationAndPhasing
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Betong 150" | names: "V-" | material: layers "Betong 150" ("Betong" 150.) | property sets: Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, Pset_WallCommon
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "NYE YTTERVEGGER_Trestender 198 mm stender, 48 mm Utf, 23 mm lekt 294" | names: "YVT-" | material: layers "NYE YTTERVEGGER_Trestender 198 mm stender, 48 mm Utf, 23 mm lekt" ("Lufting - Vertikalt" 23., "Vindsperre" 12.5, "Bindingsverk - Isolert" 198., "Dampsperre" 0., "Utforing - Isolert" 48., "Platekledning - Vegg" 12.5) | property sets: Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu" | object type "WINDOW" | names: "V-1" | property sets: Pset_WindowCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          3 x IFCCOVERING | type IFCCOVERINGTYPE "Gulvbelegg 200" | CEILING | names: "H-" | material: "Gulvbelegg" | property sets: Pset_CoveringCommon, AC_Pset_Dimension, AC_Pset_RenovationAndPhasing, BaseQuantities, Pset_FireRatingProperties
          1 x IFCDOOR | type IFCDOORSTYLE "Skyvedør utenpåliggende" | object type "DOOR" | names: "D-3" | property sets: AC_Pset_RenovationAndPhasing, Pset_FireRatingProperties, BaseQuantities, Pset_DoorCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Betong 300" | names: "V-" | material: layers "Betong 300" ("Betong" 300.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Glass 30 mm 30" | names: "V-" | material: layers "Glass 30 mm" ("Glass" 15., "Glass" 15.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, BaseQuantities, AC_Pset_RenovationAndPhasing
          2 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "Dg-1" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, BaseQuantities, AC_Pset_RenovationAndPhasing
          4 x IFCWALL | type IFCWALLTYPE "NYE YTTERVEGGER_Trestender 198 mm stender, 48 mm Utf, 23 mm lekt 294" | names: "YVT-" | parts: 20 IFCBUILDINGELEMENTPART | property sets: Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-6" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          2 x IFCWALL | type IFCWALLTYPE "Betong - Strukturell 100" | names: "YVT-" | material: "Betong - Strukturell" | property sets: BaseQuantities, AC_Pset_RenovationAndPhasing, Pset_FireRatingProperties, Pset_WallCommon
          2 x IFCDOOR | type IFCDOORSTYLE "Dør med sidefelt på side 2" | object type "DOOR" | names: "YD-1", "YD-3" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu" | object type "WINDOW" | names: "V-4" | property sets: Pset_WindowCommon, Pset_FireRatingProperties, BaseQuantities, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "Skyvedør med pocketkarm" | object type "DOOR" | names: "D-3" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "Dg-1" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          2 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "Dg-1" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Heis" | names: "Kjøkken-" | parts: 2 IFCBUILDINGELEMENTPART | property sets: AC_Pset_Dimension, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Trestender 148 mm, isolert, 2x platekl. to sider (1) 198" | names: "V-" | material: layers "Trestender 148 mm, isolert, 2x platekl. to sider (1)" ("Platekledning - Vegg" 12.5, "Platekledning - Vegg" 12.5, "Stenderverk tre - Isolert" 148., "Platekledning - Vegg" 12.5, "Platekledning - Vegg" 12.5) | property sets: Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "D-2" | property sets: Pset_DoorCommon, AC_Pset_RenovationAndPhasing, BaseQuantities, Pset_FireRatingProperties
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu to-fags" | object type "WINDOW" | names: "V-22" | property sets: Pset_WindowCommon, AC_Pset_RenovationAndPhasing, BaseQuantities, Pset_FireRatingProperties
          1 x IFCDOOR | type IFCDOORSTYLE "Skyvedør" | object type "DOOR" | names: "YD-5" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          3 x IFCSTAIR | names: "Trapp-" | parts: 7 IFCBUILDINGELEMENTPART | property sets: Pset_StairCommon, AC_Pset_RenovationAndPhasing, BaseQuantities, Pset_FireRatingProperties
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "HEIS_Trestender 98 mm stender, 23 mm lekt 195" | names: "YVT-" | material: layers "HEIS_Trestender 98 mm stender, 23 mm lekt" ("Lufting - Vertikalt" 23., "Vindsperre" 12.5, "Bindingsverk - Isolert" 159., "Dampsperre" 0.) | property sets: Pset_FireRatingProperties, Pset_WallCommon, BaseQuantities, AC_Pset_RenovationAndPhasing
          2 x IFCCOLUMN | type IFCCOLUMNTYPE "Betong 300 x 300" | object type "COLUMN" | names: "Søyle-" | material: "Betong" | property sets: Pset_ColumnCommon, AC_Pset_RenovationAndPhasing, BaseQuantities, Pset_FireRatingProperties
          1 x IFCBEAM | type IFCBEAMTYPE "Betong 200 x 450" | object type "BEAM" | names: "Bjelke-" | material: "Betong" | property sets: Pset_BeamCommon, BaseQuantities, AC_Pset_RenovationAndPhasing, Pset_FireRatingProperties
          37 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Design Profiles" | names: "Kjøkken-" | property sets: AC_Pset_Dimension, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          7 x IFCCOVERING | type IFCCOVERINGTYPE "Betong 30" | CEILING | names: "H-" | material: "Betong" | property sets: Pset_CoveringCommon, AC_Pset_Dimension, Pset_FireRatingProperties, BaseQuantities, AC_Pset_RenovationAndPhasing
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Betong 7254" | CEILING | names: "H-" | material: "Betong" | property sets: Pset_CoveringCommon, AC_Pset_Dimension, Pset_FireRatingProperties, BaseQuantities, AC_Pset_RenovationAndPhasing
          2 x IFCCOVERING | type IFCCOVERINGTYPE "Betong 5730" | CEILING | names: "H-" | material: "Betong" | property sets: Pset_CoveringCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, AC_Pset_Dimension, BaseQuantities
          2 x IFCCOVERING | type IFCCOVERINGTYPE "Betong 5730" | CEILING | names: "H-" | material: "Betong" | property sets: Pset_CoveringCommon, BaseQuantities, AC_Pset_RenovationAndPhasing, Pset_FireRatingProperties, AC_Pset_Dimension
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Betong 3680" | CEILING | names: "H-" | material: "Betong" | property sets: Pset_CoveringCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, AC_Pset_Dimension
          2 x IFCCOLUMN | type IFCCOLUMNTYPE "Limtre 150 x 150" | object type "COLUMN" | names: "Søyle-" | material: "Limtre" | property sets: Pset_ColumnCommon, Pset_FireRatingProperties, BaseQuantities, AC_Pset_RenovationAndPhasing
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Betong 3680" | CEILING | names: "H-" | material: "Betong" | property sets: Pset_CoveringCommon, AC_Pset_RenovationAndPhasing, Pset_FireRatingProperties, AC_Pset_Dimension, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Trestender 198 mm stender, 48 mm Utf 272" | names: "V-" | material: layers "Trestender 198 mm stender, 48 mm Utf" ("Vindsperre" 12.3, "Bindingsverk - Isolert" 198., "Dampsperre" 1., "Utforing - Isolert" 48., "Platekledning - Vegg" 12.5) | property sets: Pset_FireRatingProperties, Pset_WallCommon, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Trestender 98 mm, isolert, 1x platekl. to sider 122" | names: "V-" | material: layers "Trestender 98 mm, isolert, 1x platekl. to sider" ("Platekledning - Vegg" 12., "Stenderverk tre - Isolert" 98., "Platekledning - Vegg" 12.) | property sets: Pset_WallCommon, AC_Pset_RenovationAndPhasing, BaseQuantities, Pset_FireRatingProperties
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Betong 7277" | CEILING | names: "H-" | material: "Betong" | property sets: Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, AC_Pset_Dimension, Pset_CoveringCommon
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Betong 7277" | CEILING | names: "H-" | material: "Betong" | property sets: Pset_CoveringCommon, AC_Pset_Dimension, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "Betong 400 x 400" | object type "BEAM" | names: "Bjelke-" | material: "Betong" | property sets: Pset_BeamCommon, Pset_FireRatingProperties, BaseQuantities, AC_Pset_RenovationAndPhasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Trestender 48 mm, isolert, 1x platekl. en side 61" | names: "V-" | material: layers "Trestender 48 mm, isolert, 1x platekl. en side" ("Platekledning - Vegg" 12.5, "Stenderverk tre - Isolert" 48.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          2 x IFCWALL | type IFCWALLTYPE "Trestender 98 mm + 48 mm, dampsperre 161" | names: "V-" | parts: 6 IFCBUILDINGELEMENTPART | property sets: Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, Pset_WallCommon
          2 x IFCWALL | type IFCWALLTYPE "Trestender 48 mm, isolert, 1x platekl. en side 61" | names: "V-" | parts: 4 IFCBUILDINGELEMENTPART | property sets: Pset_FireRatingProperties, Pset_WallCommon, AC_Pset_RenovationAndPhasing, BaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "Betong 300 x 400" | object type "BEAM" | names: "Bjelke-" | material: "Betong" | property sets: Pset_FireRatingProperties, Pset_BeamCommon, BaseQuantities, AC_Pset_RenovationAndPhasing
          2 x IFCDOOR | type IFCDOORSTYLE "Dør med sidefelt på side 2" | object type "DOOR" | names: "YD-2", "YD-4" | property sets: Pset_FireRatingProperties, Pset_DoorCommon, BaseQuantities, AC_Pset_RenovationAndPhasing
          2 x IFCCOVERING | type IFCCOVERINGTYPE "Betong 7200" | CEILING | names: "H-" | material: "Betong" | property sets: AC_Pset_Dimension, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, Pset_CoveringCommon, BaseQuantities
          2 x IFCCOVERING | type IFCCOVERINGTYPE "Betong 2310" | CEILING | names: "H-" | material: "Betong" | property sets: Pset_FireRatingProperties, BaseQuantities, AC_Pset_RenovationAndPhasing, AC_Pset_Dimension, Pset_CoveringCommon
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Betong 7230" | CEILING | names: "H-" | material: "Betong" | property sets: Pset_CoveringCommon, AC_Pset_Dimension, AC_Pset_RenovationAndPhasing, Pset_FireRatingProperties, BaseQuantities
          15 x IFCCOVERING | type IFCCOVERINGTYPE "Systemhimling - 60x60 30" | CEILING | names: "H-" | material: "Systemhimling - 60x60" | property sets: Pset_CoveringCommon, AC_Pset_Dimension, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "D-4" | property sets: Pset_FireRatingProperties, Pset_DoorCommon, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "D-2" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "D-2" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "D-5" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "D-2" | property sets: Pset_DoorCommon, AC_Pset_RenovationAndPhasing, BaseQuantities, Pset_FireRatingProperties
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Stålstender 120/95 mm forskutte, isolert, 2x2 platekl. EI60, 52 dB (48 C-korr.) 168" | names: "V-" | material: layers "Stålstender 120/95 mm forskutte, isolert, 2x2 platekl. EI60, 52 dB (48 C-korr.)" ("Gipsplate - Vegg" 12., "Gipsplate - Vegg" 12., "Stenderverk stål - Isolert" 120., "Gipsplate - Vegg" 12., "Gipsplate - Vegg" 12.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Trestender 148 mm 161" | names: "V-" | material: layers "Trestender 148 mm" ("Stenderverk tre - Isolert" 148., "Gips" 12.5) | property sets: Pset_WallCommon, BaseQuantities, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
      IFCBUILDINGSTOREY "2. etasje" | long name "1. 2. Etasje" | elevation 7200.
        contains 313 elements
          2 x IFCCOVERING | type IFCCOVERINGTYPE "Gulvbelegg 50" | CEILING | names: "H-" | material: "Gulvbelegg" | property sets: Pset_CoveringCommon, AC_Pset_Dimension, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Trestender 98 mm stender 188" | names: "YVT-" | material: layers "Trestender 98 mm stender" ("Platekledning - Vegg" 18., "Lufting - Horisontalt" 23., "Lufting - Horisontalt" 36., "Vindsperre" 12.5, "Bindingsverk - Isolert" 98., "Dampsperre" 0.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, BaseQuantities, AC_Pset_RenovationAndPhasing
          15 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu" | object type "WINDOW" | names: "V-2" | property sets: Pset_WindowCommon, Pset_FireRatingProperties, BaseQuantities, AC_Pset_RenovationAndPhasing
          23 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu" | object type "WINDOW" | names: "V-2", "V-" | property sets: Pset_FireRatingProperties, BaseQuantities, Pset_WindowCommon, AC_Pset_RenovationAndPhasing
          46 x IFCWINDOW | type IFCWINDOWSTYLE "Pilaster" | object type "WINDOW" | names: "V-" | material: "Aluminium" | property sets: Pset_WindowCommon, Pset_FireRatingProperties, BaseQuantities, AC_Pset_RenovationAndPhasing
          1 x IFCWALL | type IFCWALLTYPE "Trestender 98 mm stender 188" | names: "YVT-" | parts: 5 IFCBUILDINGELEMENTPART | property sets: Pset_FireRatingProperties, Pset_WallCommon, AC_Pset_RenovationAndPhasing, BaseQuantities
          12 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu" | object type "WINDOW" | names: "V-2" | property sets: Pset_WindowCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          21 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Trestender 98 mm, isolert, 2x platekl. to sider 148" | names: "V-" | material: layers "Trestender 98 mm, isolert, 2x platekl. to sider" ("Platekledning - Vegg" 12.5, "Platekledning - Vegg" 12.5, "Stenderverk tre - Isolert" 98., "Platekledning - Vegg" 12.5, "Platekledning - Vegg" 12.5) | property sets: Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          12 x IFCCOLUMN | type IFCCOLUMNTYPE "Betong 400 x 300" | object type "COLUMN" | names: "Søyle-" | material: "Betong" | property sets: Pset_ColumnCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "D-" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Betong 250" | names: "V-" | material: layers "Betong 250" ("Betong" 250.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Betong 200" | names: "V-" | material: layers "Betong 200" ("Betong" 200.) | property sets: Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, Pset_WallCommon
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Innervegg 150" | names: "V-" | material: layers "Innervegg 150" ("Innervegg" 150.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          2 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          7 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Innervegg 100" | names: "V-" | material: layers "Innervegg 100" ("Innervegg" 100.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "D-" | property sets: AC_Pset_RenovationAndPhasing, Pset_FireRatingProperties, Pset_DoorCommon, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "D-" | property sets: Pset_FireRatingProperties, Pset_DoorCommon, BaseQuantities, AC_Pset_RenovationAndPhasing
          2 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Betong 150" | names: "V-" | material: layers "Betong 150" ("Betong" 150.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "Gesims flatt tak ny 268 x 102" | object type "BEAM" | names: "Bjelke-" | parts: 6 IFCBUILDINGELEMENTPART | property sets: Pset_BeamCommon, AC_Pset_RenovationAndPhasing, BaseQuantities, Pset_FireRatingProperties
          4 x IFCWALL | type IFCWALLTYPE "NYE YTTERVEGGER_Trestender 198 mm stender, 48 mm Utf, 23 mm lekt 294" | names: "YVT-" | parts: 20 IFCBUILDINGELEMENTPART | property sets: Pset_WallCommon, AC_Pset_RenovationAndPhasing, Pset_FireRatingProperties, BaseQuantities
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "NYE YTTERVEGGER_Trestender 198 mm stender, 48 mm Utf, 23 mm lekt 294" | names: "YVT-" | material: layers "NYE YTTERVEGGER_Trestender 198 mm stender, 48 mm Utf, 23 mm lekt" ("Lufting - Vertikalt" 23., "Vindsperre" 12.5, "Bindingsverk - Isolert" 198., "Dampsperre" 0., "Utforing - Isolert" 48., "Platekledning - Vegg" 12.5) | property sets: Pset_WallCommon, AC_Pset_RenovationAndPhasing, Pset_FireRatingProperties, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Betong - Strukturell 50" | names: "V-" | material: layers "Betong - Strukturell 50" ("Betong - Strukturell" 50.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "Dg-1" | property sets: Pset_FireRatingProperties, Pset_DoorCommon, BaseQuantities, AC_Pset_RenovationAndPhasing
          9 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Glass 30 mm 30" | names: "V-" | material: layers "Glass 30 mm" ("Glass" 15., "Glass" 15.) | property sets: Pset_WallCommon, AC_Pset_RenovationAndPhasing, BaseQuantities, Pset_FireRatingProperties
          8 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "Dg-1" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, BaseQuantities, AC_Pset_RenovationAndPhasing
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Trestender 148 mm, isolert, 2x platekl. to sider (1) 198" | names: "V-" | material: layers "Trestender 148 mm, isolert, 2x platekl. to sider (1)" ("Platekledning - Vegg" 12.5, "Platekledning - Vegg" 12.5, "Stenderverk tre - Isolert" 148., "Platekledning - Vegg" 12.5, "Platekledning - Vegg" 12.5) | property sets: Pset_FireRatingProperties, Pset_WallCommon, BaseQuantities, AC_Pset_RenovationAndPhasing
          2 x IFCCOVERING | type IFCCOVERINGTYPE "Gulvbelegg 200" | CEILING | names: "H-" | material: "Gulvbelegg" | property sets: Pset_CoveringCommon, Pset_FireRatingProperties, AC_Pset_Dimension, AC_Pset_RenovationAndPhasing, BaseQuantities
          4 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "Dg-1" | property sets: Pset_FireRatingProperties, Pset_DoorCommon, AC_Pset_RenovationAndPhasing, BaseQuantities
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Trestender 98 mm, isolert, 1x platekl. to sider 122" | names: "V-" | material: layers "Trestender 98 mm, isolert, 1x platekl. to sider" ("Platekledning - Vegg" 12., "Stenderverk tre - Isolert" 98., "Platekledning - Vegg" 12.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "Dg-1" | property sets: Pset_DoorCommon, AC_Pset_RenovationAndPhasing, Pset_FireRatingProperties, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "Dg-1" | property sets: AC_Pset_RenovationAndPhasing, BaseQuantities, Pset_DoorCommon, Pset_FireRatingProperties
          1 x IFCDOOR | type IFCDOORSTYLE "Skyvedør utenpåliggende" | object type "DOOR" | names: "Dg-2" | property sets: Pset_FireRatingProperties, Pset_DoorCommon, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Isolasjon - Ekspandert polystyren (EPS) 300" | CEILING | names: "H-" | material: "Isolasjon - Ekspandert polystyren (EPS)" | property sets: Pset_CoveringCommon, Pset_FireRatingProperties, AC_Pset_Dimension, AC_Pset_RenovationAndPhasing, BaseQuantities
          26 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Design Profiles" | names: "Kjøkken-" | property sets: Pset_ManufacturerOccurrence, AC_Pset_Dimension, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          8 x IFCCOVERING | type IFCCOVERINGTYPE "Betong 30" | CEILING | names: "H-" | material: "Betong" | property sets: AC_Pset_Dimension, Pset_FireRatingProperties, BaseQuantities, AC_Pset_RenovationAndPhasing, Pset_CoveringCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Trestender 198 mm stender, 48 mm Utf 272" | names: "V-" | material: layers "Trestender 198 mm stender, 48 mm Utf" ("Vindsperre" 12.3, "Bindingsverk - Isolert" 198., "Dampsperre" 1., "Utforing - Isolert" 48., "Platekledning - Vegg" 12.5) | property sets: Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCWALL | type IFCWALLTYPE "HEIS_Trestender 98 mm stender, 23 mm lekt 195" | names: "YVT-" | parts: 3 IFCBUILDINGELEMENTPART | property sets: BaseQuantities, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, Pset_WallCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu multi-rams horisontalt" | object type "WINDOW" | names: "V-3" | property sets: Pset_WindowCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Trestender 48 mm, isolert, 1x platekl. en side 61" | names: "YVT-" | material: layers "Trestender 48 mm, isolert, 1x platekl. en side" ("Platekledning - Vegg" 12.5, "Stenderverk tre - Isolert" 48.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          2 x IFCWALL | type IFCWALLTYPE "Trestender 98 mm + 48 mm, dampsperre 161" | names: "YVT-" | parts: 6 IFCBUILDINGELEMENTPART | property sets: Pset_WallCommon, AC_Pset_RenovationAndPhasing, BaseQuantities, Pset_FireRatingProperties
          2 x IFCWALL | type IFCWALLTYPE "Trestender 48 mm, isolert, 1x platekl. en side 61" | names: "YVT-" | parts: 4 IFCBUILDINGELEMENTPART | property sets: Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "Betong 400 x 400" | object type "BEAM" | names: "Bjelke-" | material: "Betong" | property sets: Pset_BeamCommon, AC_Pset_RenovationAndPhasing, BaseQuantities, Pset_FireRatingProperties
          44 x IFCBEAM | type IFCBEAMTYPE "DT elementer 1180 x 500" | object type "BEAM" | names: "Bjelke-" | material: "Betong" | property sets: Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, Pset_BeamCommon
          1 x IFCBEAM | type IFCBEAMTYPE "Betong" | names: "Bjelke-" | material: "Betong" | property sets: BaseQuantities, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, Pset_BeamCommon
          2 x IFCCOLUMN | type IFCCOLUMNTYPE "Tre 150 x 150" | object type "COLUMN" | names: "Søyle-" | material: "Tre" | property sets: Pset_ColumnCommon, Pset_FireRatingProperties, BaseQuantities, AC_Pset_RenovationAndPhasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "HEIS_Trestender 98 mm stender, 23 mm lekt 195" | names: "YVT-" | material: layers "HEIS_Trestender 98 mm stender, 23 mm lekt" ("Lufting - Vertikalt" 23., "Vindsperre" 12.5, "Bindingsverk - Isolert" 159., "Dampsperre" 0.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, BaseQuantities, AC_Pset_RenovationAndPhasing
          13 x IFCCOVERING | type IFCCOVERINGTYPE "Systemhimling - 60x60 30" | CEILING | names: "H-" | material: "Systemhimling - 60x60" | property sets: Pset_CoveringCommon, AC_Pset_Dimension, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "D-" | property sets: Pset_DoorCommon, BaseQuantities, AC_Pset_RenovationAndPhasing, Pset_FireRatingProperties
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Trestender 148 mm 161" | names: "V-" | material: layers "Trestender 148 mm" ("Stenderverk tre - Isolert" 148., "Gips" 12.5) | property sets: Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Stålstender 120/95 mm forskutte, isolert, 2x2 platekl. EI60, 52 dB (48 C-korr.) 168" | names: "V-" | material: layers "Stålstender 120/95 mm forskutte, isolert, 2x2 platekl. EI60, 52 dB (48 C-korr.)" ("Gipsplate - Vegg" 12., "Gipsplate - Vegg" 12., "Stenderverk stål - Isolert" 120., "Gipsplate - Vegg" 12., "Gipsplate - Vegg" 12.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-3" | property sets: AC_Pset_RenovationAndPhasing, Pset_FireRatingProperties, BaseQuantities, Pset_DoorCommon
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Gulvbelegg 150" | CEILING | names: "H-" | material: "Gulvbelegg" | property sets: Pset_CoveringCommon, AC_Pset_Dimension, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
      IFCBUILDINGSTOREY "Takplan" | elevation 10400.
        contains 33 elements
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Ny tak 160+30+folie 190" | CEILING | names: "H-" | parts: 2 IFCBUILDINGELEMENTPART | property sets: Pset_CoveringCommon, AC_Pset_Dimension, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCWALL | type IFCWALLTYPE "Trestender 98 mm stender 188" | names: "YVT-" | parts: 5 IFCBUILDINGELEMENTPART | property sets: Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Trestender 98 mm stender 188" | names: "YVT-" | material: layers "Trestender 98 mm stender" ("Platekledning - Vegg" 18., "Lufting - Horisontalt" 23., "Lufting - Horisontalt" 36., "Vindsperre" 12.5, "Bindingsverk - Isolert" 98., "Dampsperre" 0.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          9 x IFCWALL | type IFCWALLTYPE "NYE YTTERVEGGER_Parapet 246" | names: "YVT-" | parts: 36 IFCBUILDINGELEMENTPART | property sets: Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "NYE YTTERVEGGER_Parapet 246" | names: "YVT-" | material: layers "NYE YTTERVEGGER_Parapet" ("Lufting - Vertikalt" 23., "Vindsperre" 12.5, "Bindingsverk - Isolert" 198., "Dampsperre" 0., "Platekledning - Vegg" 12.5) | property sets: Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "Tak 50" | ROOF | names: "Tak-" | material: layers "Tak 49.9844" ("Tak" 49.98442800431426) | property sets: BaseQuantities, AC_Pset_RenovationAndPhasing, Pset_FireRatingProperties, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Tak 153" | ROOF | names: "Tak-" | material: layers "Tak 152.79" ("Tak" 152.7903188174498) | property sets: Pset_FireRatingProperties, BaseQuantities, AC_Pset_RenovationAndPhasing, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "2326 157trp+50+dmp+310+folie 521" | ROOF | names: "Tak-" | material: layers "2326 157trp+50+dmp+310+folie" ("Membran" 2., "Isolasjon - Myk" 310., "Dampsperre" 2., "Isolasjon - Murplate" 50., "Aluminium" 157.) | property sets: Pset_SlabCommon, AC_Pset_RenovationAndPhasing, BaseQuantities, Pset_FireRatingProperties
          5 x IFCBEAM | type IFCBEAMTYPE "Gesims flatt tak ny 268 x 102" | object type "BEAM" | names: "Bjelke-" | parts: 15 IFCBUILDINGELEMENTPART | property sets: Pset_BeamCommon, AC_Pset_RenovationAndPhasing, BaseQuantities, Pset_FireRatingProperties
          2 x IFCBEAM | type IFCBEAMTYPE "Gesims flatt tak ny, påbygg 348 x 102" | object type "BEAM" | names: "Bjelke-" | parts: 6 IFCBUILDINGELEMENTPART | property sets: Pset_BeamCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "Isolasjon - Markplate 310" | ROOF | names: "Tak-" | material: layers "Isolasjon - Markplate 309.903" ("Isolasjon - Markplate" 309.9034536267484) | property sets: Pset_SlabCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCCOVERING | type IFCCOVERINGTYPE "2326 Eks-tak 100eps+papp+100stenull+folie 204" | CEILING | names: "H-" | parts: 4 IFCBUILDINGELEMENTPART | property sets: Pset_CoveringCommon, Pset_FireRatingProperties, AC_Pset_Dimension, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Påstøp 50" | CEILING | names: "H-" | material: "Påstøp" | property sets: Pset_CoveringCommon, AC_Pset_RenovationAndPhasing, AC_Pset_Dimension, Pset_FireRatingProperties, BaseQuantities
          2 x IFCWALL | type IFCWALLTYPE "HEIS_Trestender 98 mm stender, 23 mm lekt 195" | names: "YVT-" | parts: 6 IFCBUILDINGELEMENTPART | property sets: Pset_FireRatingProperties, BaseQuantities, AC_Pset_RenovationAndPhasing, Pset_WallCommon

Types
  IFCWALLTYPE "Betong 400" | 3 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 5 occurrences
  IFCWINDOWSTYLE "Vindu" | SINGLE_PANEL | 1 occurrence
  IFCDOORSTYLE "Dør tofløyet asymmetrisk" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCWALLTYPE "Betong 300" | 5 occurrences
  IFCDOORSTYLE "Dør" | DOUBLE_SWING_RIGHT | 1 occurrence
  IFCWALLTYPE "Betong 200" | 9 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 3 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCWALLTYPE "Betong 150" | 8 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 3 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 1 occurrence
  IFCWALLTYPE "Betong 100" | 3 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 1 occurrence
  IFCWALLTYPE "Betong 250" | 9 occurrences
  IFCCOVERINGTYPE "Gulvbelegg 100" | CEILING | 3 occurrences | property sets: Pset_CoveringCommon
  IFCWALLTYPE "Betong - Strukturell 150" | 3 occurrences
  IFCWALLTYPE "Betong 160" | 1 occurrence
  IFCWALLTYPE "Betong 220" | 3 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 2 occurrences
  IFCWALLTYPE "Trestender 98 mm, isolert, 2x platekl. to sider 148" | 44 occurrences
  IFCWALLTYPE "Isolasjon - Trykkfast 100" | 7 occurrences
  IFCWALLTYPE "Isolasjon - Trykkfast 200" | 6 occurrences
  IFCDOORSTYLE "Dør tofløyet asymmetrisk" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCCOLUMNTYPE "Betong 400 x 300" | COLUMN | 26 occurrences
  IFCWALLTYPE "Innervegg 100" | 11 occurrences
  IFCDOORSTYLE "Skyvedør utenpåliggende" | SLIDING_TO_RIGHT | 1 occurrence
  IFCWALLTYPE "Innervegg 200" | 3 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 1 occurrence
  IFCWALLTYPE "Innervegg 80" | 2 occurrences
  IFCWALLTYPE "Trestender 98 mm stender 188" | 17 occurrences
  IFCWINDOWSTYLE "Vindu" | SINGLE_PANEL | 40 occurrences
  IFCWINDOWSTYLE "Pilaster" | 86 occurrences
  IFCWINDOWSTYLE "Vindu" | SINGLE_PANEL | 24 occurrences
  IFCWINDOWSTYLE "Vindu" | SINGLE_PANEL | 25 occurrences
  IFCCOVERINGTYPE "Gulvbelegg 220" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCWALLTYPE "NYE YTTERVEGGER_Trestender 198 mm stender, 48 mm Utf, 23 mm lekt 294" | 17 occurrences
  IFCWINDOWSTYLE "Vindu" | SINGLE_PANEL | 1 occurrence
  IFCCOVERINGTYPE "Gulvbelegg 200" | CEILING | 5 occurrences | property sets: Pset_CoveringCommon
  IFCDOORSTYLE "Skyvedør utenpåliggende" | SLIDING_TO_LEFT | 2 occurrences
  IFCWALLTYPE "Glass 30 mm 30" | 14 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 3 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCWALLTYPE "Betong - Strukturell 100" | 2 occurrences
  IFCDOORSTYLE "Dør med sidefelt på side 2" | SINGLE_SWING_RIGHT | 2 occurrences
  IFCWINDOWSTYLE "Vindu" | SINGLE_PANEL | 1 occurrence
  IFCDOORSTYLE "Skyvedør med pocketkarm" | USERDEFINED | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 2 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 6 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Heis" | 1 occurrence
  IFCWALLTYPE "Trestender 148 mm, isolert, 2x platekl. to sider (1) 198" | 5 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 1 occurrence
  IFCWINDOWSTYLE "Vindu to-fags" | DOUBLE_PANEL_VERTICAL | 1 occurrence
  IFCDOORSTYLE "Skyvedør" | USERDEFINED | 1 occurrence
  IFCWALLTYPE "HEIS_Trestender 98 mm stender, 23 mm lekt 195" | 6 occurrences
  IFCCOLUMNTYPE "Betong 300 x 300" | COLUMN | 2 occurrences
  IFCBEAMTYPE "Betong 200 x 450" | BEAM | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Design Profiles" | 63 occurrences
  IFCCOVERINGTYPE "Betong 30" | CEILING | 15 occurrences | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Betong 7254" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Betong 5730" | CEILING | 2 occurrences | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Betong 5730" | CEILING | 2 occurrences | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Betong 3680" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOLUMNTYPE "Limtre 150 x 150" | COLUMN | 2 occurrences
  IFCCOVERINGTYPE "Betong 3680" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCWALLTYPE "Trestender 198 mm stender, 48 mm Utf 272" | 2 occurrences
  IFCWALLTYPE "Trestender 98 mm, isolert, 1x platekl. to sider 122" | 6 occurrences
  IFCCOVERINGTYPE "Betong 7277" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Betong 7277" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCBEAMTYPE "Betong 400 x 400" | BEAM | 4 occurrences
  IFCWALLTYPE "Trestender 48 mm, isolert, 1x platekl. en side 61" | 6 occurrences
  IFCWALLTYPE "Trestender 98 mm + 48 mm, dampsperre 161" | 4 occurrences
  IFCBEAMTYPE "Betong 300 x 400" | BEAM | 2 occurrences
  IFCDOORSTYLE "Dør med sidefelt på side 2" | SINGLE_SWING_LEFT | 2 occurrences
  IFCCOVERINGTYPE "Betong 7200" | CEILING | 2 occurrences | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Betong 2310" | CEILING | 2 occurrences | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Betong 7230" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Systemhimling - 60x60 30" | CEILING | 28 occurrences | property sets: Pset_CoveringCommon
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 2 occurrences
  IFCWALLTYPE "Stålstender 120/95 mm forskutte, isolert, 2x2 platekl. EI60, 52 dB (48 C-korr.) 168" | 2 occurrences
  IFCWALLTYPE "Trestender 148 mm 161" | 4 occurrences
  IFCCOVERINGTYPE "Gulvbelegg 50" | CEILING | 2 occurrences | property sets: Pset_CoveringCommon
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCWALLTYPE "Innervegg 150" | 2 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 2 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 2 occurrences
  IFCBEAMTYPE "Gesims flatt tak ny 268 x 102" | BEAM | 7 occurrences
  IFCWALLTYPE "Betong - Strukturell 50" | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 8 occurrences
  IFCCOVERINGTYPE "Isolasjon - Ekspandert polystyren (EPS) 300" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCWINDOWSTYLE "Vindu multi-rams horisontalt" | DOUBLE_PANEL_VERTICAL | 1 occurrence
  IFCBEAMTYPE "DT elementer 1180 x 500" | BEAM | 44 occurrences
  IFCBEAMTYPE "Betong" | 1 occurrence
  IFCCOLUMNTYPE "Tre 150 x 150" | COLUMN | 2 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 1 occurrence
  IFCCOVERINGTYPE "Gulvbelegg 150" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Ny tak 160+30+folie 190" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCWALLTYPE "NYE YTTERVEGGER_Parapet 246" | 12 occurrences
  IFCSLABTYPE "Tak 50" | ROOF | 1 occurrence
  IFCSLABTYPE "Tak 153" | ROOF | 1 occurrence
  IFCSLABTYPE "2326 157trp+50+dmp+310+folie 521" | ROOF | 1 occurrence
  IFCBEAMTYPE "Gesims flatt tak ny, påbygg 348 x 102" | BEAM | 2 occurrences
  IFCSLABTYPE "Isolasjon - Markplate 310" | ROOF | 1 occurrence
  IFCCOVERINGTYPE "2326 Eks-tak 100eps+papp+100stenull+folie 204" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Påstøp 50" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon

Property sets
  BaseQuantities | quantities | on 14 objects (14 IFCOPENINGELEMENT)
    Area = 1.920099999999992 [SQUARE_METRE]
    Depth = 30. [MILLI METRE]
    Height = 2110. [MILLI METRE]
    Volume = 0.01591644933891211 [CUBIC_METRE]
    Width = 909.9999999999966 [MILLI METRE]
  BaseQuantities | quantities | on 14 objects (14 IFCDOOR)
    Area = 1.920099999999992 [SQUARE_METRE]
    Depth = 30. [MILLI METRE]
    Height = 2110. [MILLI METRE]
    NetVolume = 0.01591644933891211 [CUBIC_METRE]
    Perimeter = 6039.999999999992 [MILLI METRE]
    Volume = 0.01591644933891211 [CUBIC_METRE]
    Width = 909.9999999999966 [MILLI METRE]
  BaseQuantities | quantities | on 12 objects (12 IFCCOLUMN)
    CrossSectionArea = 0.12 [SQUARE_METRE]
    Depth = 300. [MILLI METRE]
    GrossSurfaceArea = 5.070000000000021 [SQUARE_METRE]
    GrossVolume = 0.4140000000000019 [CUBIC_METRE]
    Length = 3450. [MILLI METRE]
    NetVolume = 0.4140000000000019 [CUBIC_METRE]
    OuterSurfaceArea = 4.830000000000019 [SQUARE_METRE]
    TotalSurfaceArea = 5.070000000000021 [SQUARE_METRE]
    Width = 400. [MILLI METRE]
  BaseQuantities | quantities | on 10 objects (10 IFCOPENINGELEMENT)
    Area = 0. [SQUARE_METRE]
    Depth = 187.5 [MILLI METRE]
    Height = 0. [MILLI METRE]
    Volume = 0.037949912 [CUBIC_METRE]
    Width = 0. [MILLI METRE]
  BaseQuantities | quantities | on 10 objects (10 IFCWINDOW)
    Area = 0. [SQUARE_METRE]
    Depth = 187.5 [MILLI METRE]
    GrossArea = 0. [SQUARE_METRE]
    Height = 0. [MILLI METRE]
    NetVolume = 0.037949912 [CUBIC_METRE]
    Perimeter = 0. [MILLI METRE]
    Volume = 0.037949912 [CUBIC_METRE]
    Width = 0. [MILLI METRE]
  BaseQuantities | quantities | on 10 objects (10 IFCCOLUMN)
    CrossSectionArea = 0.12 [SQUARE_METRE]
    Depth = 300. [MILLI METRE]
    GrossSurfaceArea = 4.65000000000002 [SQUARE_METRE]
    GrossVolume = 0.3780000000000018 [CUBIC_METRE]
    Length = 3150. [MILLI METRE]
    NetVolume = 0.3780000000000018 [CUBIC_METRE]
    OuterSurfaceArea = 4.410000000000018 [SQUARE_METRE]
    TotalSurfaceArea = 4.65000000000002 [SQUARE_METRE]
    Width = 400. [MILLI METRE]
  BaseQuantities | quantities | on 9 objects (9 IFCOPENINGELEMENT)
    Area = 0. [SQUARE_METRE]
    Depth = 187.5 [MILLI METRE]
    Height = 0. [MILLI METRE]
    Volume = 0.04415112000000002 [CUBIC_METRE]
    Width = 0. [MILLI METRE]
  BaseQuantities | quantities | on 9 objects (9 IFCWINDOW)
    Area = 0. [SQUARE_METRE]
    Depth = 187.5 [MILLI METRE]
    GrossArea = 0. [SQUARE_METRE]
    Height = 0. [MILLI METRE]
    NetVolume = 0.04415112000000002 [CUBIC_METRE]
    Perimeter = 0. [MILLI METRE]
    Volume = 0.04415112000000002 [CUBIC_METRE]
    Width = 0. [MILLI METRE]
  BaseQuantities: 657 more contents on 881 objects not shown
  Pset_WallCommon | properties | on 132 objects (128 IFCWALLSTANDARDCASE, 4 IFCWALL)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WallCommon | properties | on 85 objects (56 IFCWALLSTANDARDCASE, 29 IFCWALL)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_FireRatingProperties | properties | on 803 objects (184 IFCWALLSTANDARDCASE, 180 IFCWINDOW, 166 IFCBUILDINGELEMENTPART, 73 IFCCOVERING)
    FireResistanceRating = "" (IFCLABEL)
  AC_Pset_RenovationAndPhasing | properties | on 433 objects (99 IFCWALLSTANDARDCASE, 80 IFCOPENINGELEMENT, 66 IFCCOVERING, 64 IFCBUILDINGELEMENTPROXY)
    Renovation Status = "New" (IFCLABEL)
  AC_Pset_RenovationAndPhasing | properties | on 349 objects (146 IFCWINDOW, 85 IFCWALLSTANDARDCASE, 52 IFCBEAM, 30 IFCCOLUMN)
    Renovation Status = "Existing" (IFCLABEL)
  Pset_DoorCommon | properties | on 34 objects (34 IFCDOOR)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_DoorCommon | properties | on 20 objects (20 IFCDOOR)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 1.393728 (IFCPOSITIVERATIOMEASURE)
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_DoorCommon | properties | on 2 objects (2 IFCDOOR)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 1.33 (IFCPOSITIVERATIOMEASURE)
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 1.38408 (IFCPOSITIVERATIOMEASURE)
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 1.30508 (IFCPOSITIVERATIOMEASURE)
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 1.059827999999999 (IFCPOSITIVERATIOMEASURE)
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 3.49376 (IFCPOSITIVERATIOMEASURE)
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 3.317688 (IFCPOSITIVERATIOMEASURE)
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_DoorCommon: 4 more contents on 4 objects not shown
  Pset_WindowCommon | properties | on 86 objects (86 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
  Pset_WindowCommon | properties | on 19 objects (19 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 0.7074599999999999 (IFCPOSITIVERATIOMEASURE)
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WindowCommon | properties | on 18 objects (18 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 0.82992 (IFCPOSITIVERATIOMEASURE)
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WindowCommon | properties | on 17 objects (17 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 0.8231579999999998 (IFCPOSITIVERATIOMEASURE)
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WindowCommon | properties | on 15 objects (15 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 0.9923579999999999 (IFCPOSITIVERATIOMEASURE)
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WindowCommon | properties | on 6 objects (6 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 0.9282 (IFCPOSITIVERATIOMEASURE)
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WindowCommon | properties | on 6 objects (6 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 0.7722 (IFCPOSITIVERATIOMEASURE)
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WindowCommon | properties | on 4 objects (4 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 1.062576 (IFCPOSITIVERATIOMEASURE)
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WindowCommon: 6 more contents on 9 objects not shown
  Pset_CoveringCommon | properties | on 28 objects (28 IFCCOVERING)
    AcousticRating = "" (IFCLABEL)
    Finish = "" (IFCTEXT)
    FireRating = "" (IFCLABEL)
    Material = "Systemhimling - 60x60" (IFCLABEL)
    TotalThickness = 30. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 15 objects (15 IFCCOVERING)
    AcousticRating = "" (IFCLABEL)
    Finish = "" (IFCTEXT)
    FireRating = "" (IFCLABEL)
    Material = "Betong" (IFCLABEL)
    TotalThickness = 30. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 5 objects (5 IFCCOVERING)
    AcousticRating = "" (IFCLABEL)
    Finish = "" (IFCTEXT)
    FireRating = "" (IFCLABEL)
    Material = "Gulvbelegg" (IFCLABEL)
    TotalThickness = 200. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 3 objects (3 IFCCOVERING)
    AcousticRating = "" (IFCLABEL)
    Finish = "" (IFCTEXT)
    FireRating = "" (IFCLABEL)
    Material = "Gulvbelegg" (IFCLABEL)
    TotalThickness = 100. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 2 objects (2 IFCCOVERING)
    AcousticRating = "" (IFCLABEL)
    Finish = "" (IFCTEXT)
    FireRating = "" (IFCLABEL)
    Material = "Betong" (IFCLABEL)
    TotalThickness = 5730.000000000002 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 2 objects (2 IFCCOVERING)
    AcousticRating = "" (IFCLABEL)
    Finish = "" (IFCTEXT)
    FireRating = "" (IFCLABEL)
    Material = "Betong" (IFCLABEL)
    TotalThickness = 5730. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 2 objects (2 IFCCOVERING)
    AcousticRating = "" (IFCLABEL)
    Finish = "" (IFCTEXT)
    FireRating = "" (IFCLABEL)
    Material = "Betong" (IFCLABEL)
    TotalThickness = 7200.000000000001 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 2 objects (2 IFCCOVERING)
    AcousticRating = "" (IFCLABEL)
    Finish = "" (IFCTEXT)
    FireRating = "" (IFCLABEL)
    Material = "Betong" (IFCLABEL)
    TotalThickness = 2309.999999999998 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon: 32 more contents on 14 objects not shown
  AC_Pset_Dimension | properties | on 9 objects (9 IFCBUILDINGELEMENTPROXY)
    Height = 2.08 (IFCABSORBEDDOSEMEASURE)
    Lenght = "925" (IFCLABEL)
    Width = "34" (IFCLABEL)
  AC_Pset_Dimension | properties | on 9 objects (9 IFCBUILDINGELEMENTPROXY)
    Height = 0.8700000000000001 (IFCABSORBEDDOSEMEASURE)
    Lenght = "925" (IFCLABEL)
    Width = "34" (IFCLABEL)
  AC_Pset_Dimension | properties | on 9 objects (9 IFCBUILDINGELEMENTPROXY)
    Height = 1.587 (IFCABSORBEDDOSEMEASURE)
    Lenght = "925" (IFCLABEL)
    Width = "34" (IFCLABEL)
  AC_Pset_Dimension | properties | on 6 objects (6 IFCBUILDINGELEMENTPROXY)
    Height = 10.78 (IFCABSORBEDDOSEMEASURE)
    Lenght = "925" (IFCLABEL)
    Width = "34" (IFCLABEL)
  AC_Pset_Dimension | properties | on 4 objects (4 IFCCOVERING)
    Area = "0,00" (IFCLABEL)
    Height = "5 730" (IFCLABEL)
    Width = "5 730" (IFCLABEL)
  AC_Pset_Dimension | properties | on 3 objects (3 IFCCOVERING)
    Area = "0,55" (IFCLABEL)
    Height = "30" (IFCLABEL)
    Width = "30" (IFCLABEL)
  AC_Pset_Dimension | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Height = 5.82 (IFCABSORBEDDOSEMEASURE)
    Lenght = "925" (IFCLABEL)
    Width = "34" (IFCLABEL)
  AC_Pset_Dimension | properties | on 3 objects (3 IFCCOVERING)
    Area = "0,78" (IFCLABEL)
    Height = "30" (IFCLABEL)
    Width = "30" (IFCLABEL)
  AC_Pset_Dimension: 75 more contents on 91 objects not shown
  Pset_ColumnCommon | properties | on 26 objects (26 IFCCOLUMN)
    FireRating = "" (IFCLABEL)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Betong 400 x 300" (IFCIDENTIFIER)
    Slope = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 2 objects (2 IFCCOLUMN)
    FireRating = "" (IFCLABEL)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Betong 300 x 300" (IFCIDENTIFIER)
    Slope = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 2 objects (2 IFCCOLUMN)
    FireRating = "" (IFCLABEL)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Limtre 150 x 150" (IFCIDENTIFIER)
    Slope = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 2 objects (2 IFCCOLUMN)
    FireRating = "" (IFCLABEL)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Tre 150 x 150" (IFCIDENTIFIER)
    Slope = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_BeamCommon | properties | on 44 objects (44 IFCBEAM)
    FireRating = "" (IFCLABEL)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "DT elementer 1180 x 500" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_BeamCommon | properties | on 7 objects (7 IFCBEAM)
    FireRating = "" (IFCLABEL)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Gesims flatt tak ny 268 x 102" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_BeamCommon | properties | on 4 objects (4 IFCBEAM)
    FireRating = "" (IFCLABEL)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Betong 400 x 400" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_BeamCommon | properties | on 2 objects (2 IFCBEAM)
    FireRating = "" (IFCLABEL)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Betong 300 x 400" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_BeamCommon | properties | on 2 objects (2 IFCBEAM)
    FireRating = "" (IFCLABEL)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Gesims flatt tak ny, påbygg 348 x 102" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    FireRating = "" (IFCLABEL)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Betong 200 x 450" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    FireRating = "" (IFCLABEL)
  Pset_ManufacturerOccurrence | properties | on 64 objects (64 IFCBUILDINGELEMENTPROXY)
    SerialNumber = "" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 64 objects (64 IFCBUILDINGELEMENTPROXY)
    Manufacturer = "" (IFCLABEL)
    ProductionYear = "" (IFCLABEL)
  Pset_SlabCommon | properties | on 4 objects (4 IFCSLAB)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 15. (IFCCOUNTMEASURE)
    NumberOfTreads = 15. (IFCCOUNTMEASURE)
    RequiredHeadroom = 2100. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    RiserHeight = 180. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 15. (IFCCOUNTMEASURE)
    NumberOfTreads = 15. (IFCCOUNTMEASURE)
    RequiredHeadroom = 2100. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    RiserHeight = 175. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 10. (IFCCOUNTMEASURE)
    NumberOfTreads = 9. (IFCCOUNTMEASURE)
    RequiredHeadroom = 2100. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    RiserHeight = 175.010001807396 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 10. (IFCCOUNTMEASURE)
    NumberOfTreads = 9. (IFCCOUNTMEASURE)
    RequiredHeadroom = 2100. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    RiserHeight = 174.989998192604 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 20. (IFCCOUNTMEASURE)
    NumberOfTreads = 20. (IFCCOUNTMEASURE)
    RequiredHeadroom = 2100. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    RiserHeight = 177.5 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]