IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0, QuantityTakeOffAddOnView, SpaceBoundary2ndLevelAddOnView]"
Description: "Option [Elements to export: Visible elements (on all stories)]"
Description: "Option [Partial Structure Display: Entire Model]"
Description: "Option [IFC Domain: All]"
Description: "Option [Structural Function: All Elements]"
Description: "Option [Convert Grid elements: On]"
Description: "Option [Convert IFC Annotations and Archicad 2D elements: Off]"
Description: "Option [Convert 2D symbols of Doors and Windows: On]"
Description: "Option [Export geometries that Participates in Collision Detection only: Off]"
Description: "Option [Split complex elements: Off]"
Description: "Option [Material Preservation: Explode where necessary]"
Description: "Option [Elements in Solid Element Operations: Extruded/revolved]"
Description: "Option [Elements with junctions: Extruded/revolved without junctions]"
Description: "Option [IFC Model position: Project Origin only]"
Description: "Option [Curtain Wall export mode: Container Element]"
Description: "Option [Railing export mode: Single Element]"
File name: "C:\Users\Sunniva\Desktop\Toppen-ARK.ifc"
Time stamp: "2024-02-08T13:01:12"
Author: "Arkitekten"
Organization: "Tun arkitektur AS"
Preprocessor: "DDS_IFC v3.0"
Originating system: "IFC file generated by Graphisoft Archicad 27.0.0 NOR FULL Windows version (IFC add-on version: 4001 NOR FULL)."
Authorization: "Arkitekten"
Application: "Archicad" version "27.0.0" identifier "IFC add-on version: 4001 NOR FULL" by Organization "Graphisoft" id "GS" description "Graphisoft"

People and organizations
  Person "Arkitekten" (roles: "Ark:"; postal address "Architect Postal Address": "Øvre Langgate 63", "Tønsberg", "3110"; telecom address "Architect Telecom Address": telephone "48 25 85 15"; e-mail "post@tunark.no"; web page "www.tunark.no") of Organization "Tun arkitektur AS" (postal address "Architect Postal Address": "Øvre Langgate 63", "Tønsberg", "3110"; telecom address "Architect Telecom Address": telephone "48 25 85 15"; e-mail "post@tunark.no"; web page "www.tunark.no")
  Owner history of Person "Arkitekten" (roles: "Ark:"; postal address "Architect Postal Address": "Øvre Langgate 63", "Tønsberg", "3110"; telecom address "Architect Telecom Address": telephone "48 25 85 15"; e-mail "post@tunark.no"; web page "www.tunark.no") of Organization "Tun arkitektur AS" (postal address "Architect Postal Address": "Øvre Langgate 63", "Tønsberg", "3110"; telecom address "Architect Telecom Address": telephone "48 25 85 15"; e-mail "post@tunark.no"; web page "www.tunark.no") | application "Archicad" version "27.0.0" identifier "IFC add-on version: 4001 NOR FULL" by Organization "Graphisoft" id "GS" description "Graphisoft" | change NOCHANGE | created 1707393656 (2024-02-08T12:00:56Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  SOLIDANGLEUNIT: SQUAREDEGREE (conversion based)
  CURRENCY: NOK
  TIMEUNIT: Year (conversion based)
  MASSUNIT: KILO GRAM
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN
  ENERGYUNIT: MEGA JOULE
  THERMALCONDUCTANCEUNIT: derived
  SPECIFICHEATCAPACITYUNIT: derived
  MASSDENSITYUNIT: derived

Spatial structure
IFCPROJECT "VOKSENTOPPEN" | phase "FORPROSJEKT" | description "PROSJEKTFASE"
  IFCSITE "Tomten" | latitude 59° 55′ 52.428″ | longitude 10° 42′ 27.972″ | elevation above sea level 0. | postal address: "Adresse", "#", "Sted", "0000", "Norge"
    IFCBUILDING "Bygningens navn" | long name "Byggnummer" | postal address: "Adresse", "#", "Sted", "0000", "Norge" | description "-"
      IFCBUILDINGSTOREY "0. Kjeller" | elevation 485700.
        contains 407 elements
          8 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Badromskabin 30 mm betong, 7 mm flislim, 8 mm flis 45" | names: "IV-04" | material: layers "Badromskabin 30 mm betong, 7 mm flislim, 8 mm flis" ("Flis - Vegg" 8., "Flislim" 7., "Betong - Prefab" 30.) | property sets: Pset_FireRatingProperties, Pset_WallCommon, AC_Pset_RenovationAndPhasing, MMI, BaseQuantities
          25 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Innervegg 175" | names: "VT-" | material: layers "Innervegg 175" ("Innervegg" 175.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities
          17 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Innervegg 200" | names: "VT-" | material: layers "Innervegg 200" ("Innervegg" 200.) | property sets: Pset_FireRatingProperties, Pset_WallCommon, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities
          14 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-", "ID-02-V", "ID-03-H" | property sets: Pset_DoorCommon, Pset_ManufacturerOccurrence, MMI, AC_Pset_RenovationAndPhasing, Pset_FireRatingProperties, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-" | property sets: Pset_FireRatingProperties, Pset_DoorCommon, AC_Pset_RenovationAndPhasing, Pset_ManufacturerOccurrence, BaseQuantities, MMI
          2 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, BaseQuantities, AC_Pset_RenovationAndPhasing, MMI
          9 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Innervegg 20" | names: "VT-" | material: layers "Innervegg 20" ("Innervegg" 20.) | property sets: MMI, Pset_WallCommon, Pset_FireRatingProperties, BaseQuantities, AC_Pset_RenovationAndPhasing
          7 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Innervegg 300" | names: "VT-" | material: layers "Innervegg 300" ("Innervegg" 300.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, MMI, BaseQuantities
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Innervegg 130" | names: "VT-" | material: layers "Innervegg 130" ("Innervegg" 130.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities
          54 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 200" | names: "VT-" | material: layers "Yttervegg 200" ("Yttervegg" 200.) | property sets: Pset_FireRatingProperties, MMI, Pset_WallCommon, AC_Pset_RenovationAndPhasing, BaseQuantities
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 240" | names: "VT-" | material: layers "Yttervegg 240" ("Yttervegg" 240.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, BaseQuantities, AC_Pset_RenovationAndPhasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 75" | names: "VT-" | material: layers "Yttervegg 75" ("Yttervegg" 75.) | property sets: Pset_FireRatingProperties, Pset_WallCommon, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities
          7 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 265" | names: "VT-" | material: layers "Yttervegg 265" ("Yttervegg" 265.) | property sets: Pset_WallCommon, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities, Pset_FireRatingProperties
          3 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 260" | names: "VT-" | material: layers "Yttervegg 260" ("Yttervegg" 260.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, MMI
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 350" | names: "VT-" | material: layers "Yttervegg 350" ("Yttervegg" 350.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, BaseQuantities, AC_Pset_RenovationAndPhasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 220" | names: "VT-" | material: layers "Yttervegg 220" ("Yttervegg" 220.) | property sets: Pset_FireRatingProperties, MMI, AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          18 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Innervegg 100" | names: "VT-" | material: layers "Innervegg 100" ("Innervegg" 100.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, MMI, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Innervegg 450" | names: "VT-" | material: layers "Innervegg 450" ("Innervegg" 450.) | property sets: Pset_WallCommon, MMI, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          2 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, MMI, BaseQuantities, AC_Pset_RenovationAndPhasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 160" | names: "VT-" | material: layers "Yttervegg 160" ("Yttervegg" 160.) | property sets: MMI, AC_Pset_RenovationAndPhasing, Pset_FireRatingProperties, BaseQuantities, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 165" | names: "VT-" | material: layers "Yttervegg 165" ("Yttervegg" 165.) | property sets: Pset_WallCommon, MMI, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 280" | names: "VT-" | material: layers "Yttervegg 280" ("Yttervegg" 280.) | property sets: Pset_WallCommon, MMI, AC_Pset_RenovationAndPhasing, Pset_FireRatingProperties, BaseQuantities
          11 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 325" | names: "VT-" | material: layers "Yttervegg 325" ("Yttervegg" 325.) | property sets: BaseQuantities, AC_Pset_RenovationAndPhasing, MMI, Pset_FireRatingProperties, Pset_WallCommon
          4 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu" | object type "WINDOW" | names: "V-" | property sets: Pset_WindowCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, BaseQuantities, AC_Pset_RenovationAndPhasing, MMI
          1 x IFCDOOR | type IFCDOORSTYLE "Skyvedør dobbel utenpåliggende" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 375" | names: "VT-" | material: layers "Yttervegg 375" ("Yttervegg" 375.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 250" | names: "VT-" | material: layers "Yttervegg 250" ("Yttervegg" 250.) | property sets: Pset_WallCommon, AC_Pset_RenovationAndPhasing, MMI, BaseQuantities, Pset_FireRatingProperties
          3 x IFCDOOR | type IFCDOORSTYLE "Leddport" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, Pset_ManufacturerOccurrence, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, MMI, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, Pset_ManufacturerOccurrence, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, MMI
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 225" | names: "VT-" | material: layers "Yttervegg 225" ("Yttervegg" 225.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, MMI
          11 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu" | object type "WINDOW" | names: "V-01", "V-02" | property sets: Pset_WindowCommon, Pset_ManufacturerOccurrence, Pset_FireRatingProperties, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 175" | names: "VT-" | material: layers "Yttervegg 175" ("Yttervegg" 175.) | property sets: Pset_WallCommon, AC_Pset_RenovationAndPhasing, Pset_FireRatingProperties, MMI, BaseQuantities
          3 x IFCDOOR | type IFCDOORSTYLE "Dør med 2 sidefelt og overlys" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Innervegg 230" | names: "VT-" | material: layers "Innervegg 230" ("Innervegg" 230.) | property sets: Pset_WallCommon, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities, Pset_FireRatingProperties
          8 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Innervegg 275" | names: "VT-" | material: layers "Innervegg 275" ("Innervegg" 275.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 255" | names: "VT-" | material: layers "Yttervegg 255" ("Yttervegg" 255.) | property sets: Pset_FireRatingProperties, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities, Pset_WallCommon
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 275" | names: "VT-" | material: layers "Yttervegg 275" ("Yttervegg" 275.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, MMI
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 150" | names: "VT-" | material: layers "Yttervegg 150" ("Yttervegg" 150.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities
          3 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu to-fags" | object type "WINDOW" | names: "V-" | property sets: Pset_WindowCommon, Pset_ManufacturerOccurrence, AC_Pset_RenovationAndPhasing, MMI, BaseQuantities, Pset_FireRatingProperties
          8 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 300" | names: "VT-" | material: layers "Yttervegg 300" ("Yttervegg" 300.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, MMI
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-" | property sets: Pset_FireRatingProperties, Pset_DoorCommon, Pset_ManufacturerOccurrence, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities
          2 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu to-fags" | object type "WINDOW" | names: "V-" | property sets: Pset_WindowCommon, Pset_ManufacturerOccurrence, MMI, BaseQuantities, AC_Pset_RenovationAndPhasing, Pset_FireRatingProperties
          11 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Innervegg 125" | names: "VT-" | material: layers "Innervegg 125" ("Innervegg" 125.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, MMI
          22 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Innervegg 150" | names: "VT-" | material: layers "Innervegg 150" ("Innervegg" 150.) | property sets: Pset_WallCommon, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities, Pset_FireRatingProperties
          3 x IFCDOOR | type IFCDOORSTYLE "Skyvedør utenpåliggende" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, AC_Pset_RenovationAndPhasing, BaseQuantities, MMI
          7 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-", "ID-02-V" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCWALL | type IFCWALLTYPE "Innervegg 200" | names: "VT-" | material: "Innervegg" | property sets: AC_Pset_RenovationAndPhasing, MMI, Pset_WallCommon, Pset_FireRatingProperties, BaseQuantities
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Innervegg 400" | names: "VT-" | material: layers "Innervegg 400" ("Innervegg" 400.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 125" | names: "VT-" | material: layers "Yttervegg 125" ("Yttervegg" 125.) | property sets: Pset_WallCommon, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities, Pset_FireRatingProperties
          2 x IFCDOOR | type IFCDOORSTYLE "Dør med 2 sidefelt" | object type "DOOR" | names: "YD-" | property sets: Pset_ManufacturerOccurrence, Pset_DoorCommon, MMI, Pset_FireRatingProperties, BaseQuantities, AC_Pset_RenovationAndPhasing
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu" | object type "WINDOW" | names: "V-" | property sets: Pset_WindowCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, MMI, BaseQuantities, Pset_ManufacturerOccurrence
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Innervegg 375" | names: "VT-" | material: layers "Innervegg 375" ("Innervegg" 375.) | property sets: MMI, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Innervegg 475" | names: "VT-" | material: layers "Innervegg 475" ("Innervegg" 475.) | property sets: Pset_WallCommon, MMI, BaseQuantities, AC_Pset_RenovationAndPhasing, Pset_FireRatingProperties
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Innervegg 550" | names: "VT-" | material: layers "Innervegg 550" ("Innervegg" 550.) | property sets: Pset_FireRatingProperties, MMI, AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 600" | names: "VT-" | material: layers "Yttervegg 600" ("Yttervegg" 600.) | property sets: Pset_FireRatingProperties, MMI, AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Innervegg 290" | names: "VT-" | material: layers "Innervegg 290" ("Innervegg" 290.) | property sets: Pset_WallCommon, MMI, AC_Pset_RenovationAndPhasing, Pset_FireRatingProperties, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, Pset_ManufacturerOccurrence, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, MMI
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu to-fags" | object type "WINDOW" | names: "V-" | property sets: Pset_FireRatingProperties, Pset_ManufacturerOccurrence, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities, Pset_WindowCommon
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, MMI, BaseQuantities, AC_Pset_RenovationAndPhasing, Pset_ManufacturerOccurrence
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall Type" | names: "CurtainWall-" | parts: 39 IFCMEMBER, 8 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_FireRatingProperties, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities
          6 x IFCSTAIR | names: "Trapp-" | parts: 32 IFCBUILDINGELEMENTPART | property sets: Pset_StairCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, MMI, BaseQuantities
          17 x IFCSLAB | type IFCSLABTYPE "Dekke 300" | BASESLAB | names: "Dekke-" | material: layers "Dekke 300" ("Dekke" 300.) | property sets: Pset_CoveringCommon, Pset_SlabCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, MMI, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "Dekke 850" | BASESLAB | names: "Dekke-" | material: layers "Dekke 850" ("Dekke" 850.0000000000227) | property sets: Pset_CoveringCommon, Pset_FireRatingProperties, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities, Pset_SlabCommon
          2 x IFCCOLUMN | type IFCCOLUMNTYPE "Betong 350 x 200" | object type "COLUMN" | names: "S-" | material: "Betong" | property sets: Pset_FireRatingProperties, MMI, Pset_ColumnCommon, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Betong 275 x 220" | object type "COLUMN" | names: "S-" | material: "Betong" | property sets: Pset_ColumnCommon, MMI, AC_Pset_RenovationAndPhasing, Pset_FireRatingProperties, BaseQuantities
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Betong 410 x 200" | object type "COLUMN" | names: "S-" | material: "Betong" | property sets: Pset_ColumnCommon, Pset_FireRatingProperties, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Betong 350 x 185" | object type "COLUMN" | names: "S-" | material: "Betong" | property sets: Pset_FireRatingProperties, Pset_ColumnCommon, MMI, BaseQuantities, AC_Pset_RenovationAndPhasing
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Betong 300 x 300" | object type "COLUMN" | names: "S-" | material: "Betong" | property sets: Pset_ColumnCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, MMI
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Betong 285 x 200" | object type "COLUMN" | names: "S-" | material: "Betong" | property sets: Pset_ColumnCommon, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities, Pset_FireRatingProperties
          1 x IFCBEAM | type IFCBEAMTYPE "Tre 350 x 200" | object type "BEAM" | names: "B-" | material: "Tre" | property sets: Pset_BeamCommon, Pset_FireRatingProperties, BaseQuantities, MMI, AC_Pset_RenovationAndPhasing
          1 x IFCBEAM | type IFCBEAMTYPE "Tre 410 x 230" | object type "BEAM" | names: "B-" | material: "Tre" | property sets: Pset_BeamCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, MMI
          2 x IFCBEAM | type IFCBEAMTYPE "Tre 410 x 240" | object type "BEAM" | names: "B-" | material: "Tre" | property sets: Pset_BeamCommon, Pset_FireRatingProperties, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "Tre 200 x 175" | object type "BEAM" | names: "B-" | material: "Tre" | property sets: Pset_BeamCommon, MMI, AC_Pset_RenovationAndPhasing, Pset_FireRatingProperties, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "YD-" | property sets: Pset_FireRatingProperties, Pset_DoorCommon, MMI, Pset_ManufacturerOccurrence, BaseQuantities, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "Skyvedør utenpåliggende" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, BaseQuantities, MMI, AC_Pset_RenovationAndPhasing
          2 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-" | property sets: Pset_FireRatingProperties, MMI, Pset_DoorCommon, AC_Pset_RenovationAndPhasing, Pset_ManufacturerOccurrence, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør metall" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, AC_Pset_RenovationAndPhasing, BaseQuantities, MMI
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Innervegg 250" | names: "VT-" | material: layers "Innervegg 250" ("Innervegg" 250.) | property sets: Pset_WallCommon, MMI, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør metall" | object type "DOOR" | names: "YD-" | property sets: Pset_ManufacturerOccurrence, Pset_DoorCommon, Pset_FireRatingProperties, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Innervegg 225" | names: "VT-" | material: layers "Innervegg 225" ("Innervegg" 225.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, MMI
          2 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-", "ID-01-H" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, MMI, BaseQuantities, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-" | property sets: Pset_FireRatingProperties, Pset_ManufacturerOccurrence, MMI, AC_Pset_RenovationAndPhasing, Pset_DoorCommon, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør med sidefelt på side 2" | object type "DOOR" | names: "YD-" | property sets: Pset_FireRatingProperties, Pset_DoorCommon, Pset_ManufacturerOccurrence, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, Pset_ManufacturerOccurrence, MMI, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-" | property sets: Pset_FireRatingProperties, MMI, Pset_ManufacturerOccurrence, AC_Pset_RenovationAndPhasing, Pset_DoorCommon, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Innervegg 220" | names: "VT-" | material: layers "Innervegg 220" ("Innervegg" 220.) | property sets: Pset_FireRatingProperties, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "ID-03-H" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCWALL | type IFCWALLTYPE "Innervegg 175" | names: "VT-" | material: "Innervegg" | property sets: Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, MMI
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør metall" | object type "DOOR" | names: "YD-" | property sets: BaseQuantities, Pset_ManufacturerOccurrence, AC_Pset_RenovationAndPhasing, MMI, Pset_FireRatingProperties, Pset_DoorCommon
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Påforingsvegg baderomskabin 70mm stålstende, 15 mm ultraboard, 15mm kryssfiner 100" | names: "IV-03" | material: layers "Påforingsvegg baderomskabin 70mm stålstende, 15 mm ultraboard, 15mm kryssfiner" ("Stenderverk stål - Isolert" 70., "Gipsplate - Hard" 15., "Finer" 15.) | property sets: Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, MMI, Pset_WallCommon
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Korridorvegg stålstendere 95 mm, isolert, 15 mm ultraboard 15 mm kryssfiner 155" | names: "IV-02" | material: layers "Korridorvegg stålstendere 95 mm, isolert, 15 mm ultraboard 15 mm kryssfiner" ("Finer" 15., "Gipsplate - Hard" 15., "Stenderverk stål - Isolert" 95., "Gipsplate - Hard" 15., "Finer" 15.) | property sets: Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities, MMI
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Skillevegg beboerrom 2 stålstendere 70 mm, isolert, 15 mm ultraboard 15 mm kryssfiner 130" | names: "IV-05" | material: layers "Skillevegg beboerrom 2 stålstendere 70 mm, isolert, 15 mm ultraboard 15 mm kryssfiner" ("Finer" 15., "Gipsplate - Hard" 15., "Stenderverk stål - Isolert" 70., "Gipsplate - Hard" 15., "Finer" 15.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities
          2 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "ID-01-V" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, MMI, BaseQuantities, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "ID-01-H" | property sets: Pset_FireRatingProperties, Pset_DoorCommon, Pset_ManufacturerOccurrence, MMI, BaseQuantities, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "Skyvedør med pocketkarm" | object type "DOOR" | names: "ID-05-V" | property sets: BaseQuantities, MMI, AC_Pset_RenovationAndPhasing, Pset_ManufacturerOccurrence, Pset_DoorCommon, Pset_FireRatingProperties
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Skillevegg avdeling 15 mm ultraboard, 15mm kryssfiner, 70mm stålstende, luftspalte 70mm, 70mm stålstende, 15 mm ultraboard, 15mm kryssfiner 270" | names: "IV-06" | material: layers "Skillevegg avdeling 15 mm ultraboard, 15mm kryssfiner, 70mm stålstende, luftspalte 70mm, 70mm stålstende, 15 mm ultraboard, 15mm kryssfiner" ("Finer" 15., "Gipsplate - Hard" 15., "Stenderverk stål - Isolert" 70., "Lufting - Vertikalt" 70., "Stenderverk stål - Isolert" 70., "Gipsplate - Hard" 15., "Finer" 15.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Stålpipe" | object type "Chimney" | names: "Pipe-" | property sets: AC_Pset_Dimension, Pset_ManufacturerOccurrence, AC_Pset_RenovationAndPhasing, MMI
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "ID-01-V" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities
      IFCBUILDINGSTOREY "1. Etasje" | long name "1. 2. Etasje" | elevation 488410.
        contains 774 elements
          60 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Korridorvegg stålstendere 95 mm, isolert, 15 mm ultraboard 15 mm kryssfiner 155" | names: "IV-02", "IV-05", "YV-02" | material: layers "Korridorvegg stålstendere 95 mm, isolert, 15 mm ultraboard 15 mm kryssfiner" ("Finer" 15., "Gipsplate - Hard" 15., "Stenderverk stål - Isolert" 95., "Gipsplate - Hard" 15., "Finer" 15.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, MMI
          5 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "ID-05-H", "ID-01-H", "ID-03-V" (+2 more) | property sets: Pset_DoorCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities
          116 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Badromskabin 30 mm betong, 7 mm flislim, 8 mm flis 45" | names: "IV-04" | material: layers "Badromskabin 30 mm betong, 7 mm flislim, 8 mm flis" ("Flis - Vegg" 8., "Flislim" 7., "Betong - Prefab" 30.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, MMI
          89 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Påforingsvegg baderomskabin 70mm stålstende, 15 mm ultraboard, 15mm kryssfiner 100" | names: "IV-03" | material: layers "Påforingsvegg baderomskabin 70mm stålstende, 15 mm ultraboard, 15mm kryssfiner" ("Stenderverk stål - Isolert" 70., "Gipsplate - Hard" 15., "Finer" 15.) | property sets: Pset_WallCommon, MMI, AC_Pset_RenovationAndPhasing, Pset_FireRatingProperties, BaseQuantities
          5 x IFCDOOR | type IFCDOORSTYLE "Skyvedør med pocketkarm" | object type "DOOR" | names: "ID-07-V", "ID-07-H" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCROOF | names: "Tak-" | material: "Tak" | property sets: Pset_FireRatingProperties, MMI, AC_Pset_RenovationAndPhasing, Pset_RoofCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "Dekke 200" | BASESLAB | names: "Dekke-" | material: layers "Dekke 200" ("Dekke" 200.) | property sets: Pset_CoveringCommon, Pset_SlabCommon, Pset_FireRatingProperties, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities
          32 x IFCSLAB | type IFCSLABTYPE "Dekke 250" | BASESLAB | names: "Dekke-" | material: layers "Dekke 250" ("Dekke" 250.) | property sets: Pset_CoveringCommon, Pset_SlabCommon, Pset_FireRatingProperties, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities
          3 x IFCSLAB | type IFCSLABTYPE "Dekke 220" | BASESLAB | names: "Dekke-" | material: layers "Dekke 220" ("Dekke" 220.) | property sets: Pset_CoveringCommon, Pset_SlabCommon, MMI, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "Dekke 310" | BASESLAB | names: "Dekke-" | material: layers "Dekke 310" ("Dekke" 310.0000000000092) | property sets: Pset_CoveringCommon, Pset_SlabCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, MMI, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "Dekke 520" | BASESLAB | names: "Dekke-" | material: layers "Dekke 520" ("Dekke" 520.) | property sets: Pset_SlabCommon, Pset_FireRatingProperties, MMI, AC_Pset_RenovationAndPhasing, Pset_CoveringCommon, BaseQuantities
          1 x IFCWALL | type IFCWALLTYPE "Yttervegg 325" | names: "VT-" | material: "Yttervegg" | property sets: Pset_FireRatingProperties, Pset_WallCommon, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 300" | names: "VT-" | material: layers "Yttervegg 300" ("Yttervegg" 300.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, BaseQuantities, AC_Pset_RenovationAndPhasing
          13 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Skillevegg avdeling 15 mm ultraboard, 15mm kryssfiner, 70mm stålstende, luftspalte 70mm, 70mm stålstende, 15 mm ultraboard, 15mm kryssfiner 270" | names: "IV-06" | material: layers "Skillevegg avdeling 15 mm ultraboard, 15mm kryssfiner, 70mm stålstende, luftspalte 70mm, 70mm stålstende, 15 mm ultraboard, 15mm kryssfiner" ("Finer" 15., "Gipsplate - Hard" 15., "Stenderverk stål - Isolert" 70., "Lufting - Vertikalt" 70., "Stenderverk stål - Isolert" 70., "Gipsplate - Hard" 15., "Finer" 15.) | property sets: Pset_FireRatingProperties, MMI, Pset_WallCommon, BaseQuantities, AC_Pset_RenovationAndPhasing
          70 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 250 mm iso, 104 mm tegl utf., 50 mm luftsjikt, 70 mm murplate, 200 mm isolasjon 499" | names: "YV-01" | material: layers "Yttervegg 250 mm iso, 104 mm tegl utf., 50 mm luftsjikt, 70 mm murplate, 200 mm isolasjon" ("Teglstein" 104., "Lufting - Vertikalt" 50., "Isolasjon - Murplate" 70., "Gipsplate - Utvendig" 9., "Isolasjon - Myk" 200., "Dampsperre" 1., "Isolasjon - Myk" 50., "Finer" 15.) | property sets: Pset_FireRatingProperties, Pset_WallCommon, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities
          130 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu" | object type "WINDOW" | names: "V-02", "V-01", "V-" | property sets: Pset_WindowCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, BaseQuantities, AC_Pset_RenovationAndPhasing, MMI
          16 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "ID-01-H", "ID-02-V", "ID-03-H" (+2 more) | property sets: Pset_DoorCommon, MMI, Pset_ManufacturerOccurrence, AC_Pset_RenovationAndPhasing, BaseQuantities, Pset_FireRatingProperties
          13 x IFCDOOR | type IFCDOORSTYLE "Dør med sidefelt på side 2" | object type "DOOR" | names: "ID-04-H", "ID-04-V", "YD-" | property sets: Pset_DoorCommon, MMI, Pset_ManufacturerOccurrence, BaseQuantities, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          3 x IFCDOOR | type IFCDOORSTYLE "Dør med 2 sidefelt og overlys" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "ID-" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, MMI, BaseQuantities, AC_Pset_RenovationAndPhasing
          32 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Stålstender 95/95 mm, isolert, 2x2 gips 147" | names: "YV-02", "IV-09" | material: layers "Stålstender 95/95 mm, isolert, 2x2 gips" ("Gips" 13., "Gips" 13., "Stenderverk stål - Isolert" 95., "Gips" 13., "Gips" 13.) | property sets: Pset_WallCommon, MMI, AC_Pset_RenovationAndPhasing, Pset_FireRatingProperties, BaseQuantities
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Brannvegg Betong 200 mm 200" | names: "IV-07" | material: layers "Brannvegg Betong 200 mm" ("Betong" 200.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, MMI
          5 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "ID-02-V", "ID-01-V", "ID-02-H" | property sets: Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_DoorCommon, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities
          25 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "ID-01-H", "ID-03-V", "ID-02-H" (+4 more) | property sets: Pset_DoorCommon, Pset_ManufacturerOccurrence, MMI, AC_Pset_RenovationAndPhasing, Pset_FireRatingProperties, BaseQuantities
          2 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "ID-01-H", "ID-01-V" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, MMI, Pset_ManufacturerOccurrence, AC_Pset_RenovationAndPhasing, BaseQuantities
          21 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "ID-01-V", "ID-02-V", "ID-03-V" (+2 more) | property sets: Pset_FireRatingProperties, Pset_DoorCommon, Pset_ManufacturerOccurrence, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities
          15 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Skillevegg beboerrom Forskutte stålstendere 95 mm, isolert, 2x13 mm gips, 6 mm kryssfiner 190" | names: "VT-", "IV-01" | material: layers "Skillevegg beboerrom Forskutte stålstendere 95 mm, isolert, 2x13 mm gips, 6 mm kryssfiner" ("Finer" 15., "Gipsplate - Hard" 15., "Stenderverk stål - Uisolert" 35., "Stenderverk stål - Isolert" 95., "Gipsplate - Hard" 15., "Finer" 15.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities
          3 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "ID-01-H", "ID-01-V", "ID-08-H" | property sets: Pset_FireRatingProperties, Pset_DoorCommon, Pset_ManufacturerOccurrence, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities
          13 x IFCDOOR | type IFCDOORSTYLE "Dør med sidefelt på side 2" | object type "DOOR" | names: "ID-04-H" | property sets: Pset_FireRatingProperties, Pset_DoorCommon, Pset_ManufacturerOccurrence, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu multi-rams horisontalt" | object type "WINDOW" | names: "MF-" | property sets: Pset_WindowCommon, Pset_FireRatingProperties, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities, Pset_ManufacturerOccurrence
          4 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "ID-06-H", "ID-01-H" | property sets: Pset_DoorCommon, Pset_ManufacturerOccurrence, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, MMI, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "ID-06-V" | property sets: Pset_FireRatingProperties, Pset_DoorCommon, AC_Pset_RenovationAndPhasing, Pset_ManufacturerOccurrence, MMI, BaseQuantities
          5 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "ID-05-V", "ID-03-V", "ID-01-V" | property sets: Pset_DoorCommon, Pset_ManufacturerOccurrence, MMI, Pset_FireRatingProperties, BaseQuantities, AC_Pset_RenovationAndPhasing
          4 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "ID-02-H" | property sets: Pset_FireRatingProperties, Pset_ManufacturerOccurrence, AC_Pset_RenovationAndPhasing, BaseQuantities, MMI, Pset_DoorCommon
          18 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Skillevegg beboerrom 2 stålstendere 70 mm, isolert, 15 mm ultraboard 15 mm kryssfiner 130" | names: "IV-05" | material: layers "Skillevegg beboerrom 2 stålstendere 70 mm, isolert, 15 mm ultraboard 15 mm kryssfiner" ("Finer" 15., "Gipsplate - Hard" 15., "Stenderverk stål - Isolert" 70., "Gipsplate - Hard" 15., "Finer" 15.) | property sets: Pset_WallCommon, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities, Pset_FireRatingProperties
          3 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "ID-01-H", "ID-02-H", "ID-03-H" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities
          11 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "ID-02-H", "ID-01-H", "ID-03-V" (+3 more) | property sets: Pset_DoorCommon, Pset_FireRatingProperties, MMI, Pset_ManufacturerOccurrence, AC_Pset_RenovationAndPhasing, BaseQuantities
          8 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 250 mm iso, 104 mm tegl utf., 20 mm luftsjikt, 250 mm isolasjon 429" | names: "YV-02" | material: layers "Yttervegg 250 mm iso, 104 mm tegl utf., 20 mm luftsjikt, 250 mm isolasjon" ("Teglstein" 104., "Lufting - Vertikalt" 50., "Gipsplate - Utvendig" 9., "Isolasjon - Myk" 200., "Dampsperre" 1., "Isolasjon - Myk" 50., "Finer" 15.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities
          2 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "ID-01-V" | property sets: Pset_FireRatingProperties, Pset_DoorCommon, MMI, Pset_ManufacturerOccurrence, BaseQuantities, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "ID-03-V" | property sets: Pset_FireRatingProperties, Pset_DoorCommon, MMI, BaseQuantities, AC_Pset_RenovationAndPhasing, Pset_ManufacturerOccurrence
          2 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu" | object type "WINDOW" | names: "V-" | property sets: Pset_WindowCommon, MMI, Pset_FireRatingProperties, BaseQuantities, Pset_ManufacturerOccurrence, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "ID-03-V" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, AC_Pset_RenovationAndPhasing, MMI, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør med 2 sidefelt" | object type "DOOR" | names: "ID-" | property sets: Pset_FireRatingProperties, Pset_DoorCommon, MMI, AC_Pset_RenovationAndPhasing, Pset_ManufacturerOccurrence, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Foldedør multipanel" | object type "DOOR" | names: "ID-" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities, Pset_ManufacturerOccurrence
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "ID-03-V" | property sets: Pset_DoorCommon, MMI, Pset_ManufacturerOccurrence, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          19 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Skillevegg internt beboerrom stålstendere 70 mm, isolert,15 mm kryssfiner 100" | names: "IV-08", "YV-02" | material: layers "Skillevegg internt beboerrom stålstendere 70 mm, isolert,15 mm kryssfiner" ("Finer" 15., "Stenderverk stål - Isolert" 70., "Finer" 15.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, MMI
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "ID-" | property sets: Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_DoorCommon, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "ID-03-V" | property sets: Pset_FireRatingProperties, Pset_ManufacturerOccurrence, MMI, AC_Pset_RenovationAndPhasing, Pset_DoorCommon, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Teglstein 300" | names: "IV-07" | material: layers "Teglstein 300" ("Teglstein" 300.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, MMI, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "ID-02-V" | property sets: Pset_DoorCommon, Pset_ManufacturerOccurrence, MMI, Pset_FireRatingProperties, BaseQuantities, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "ID-03-H" | property sets: Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_DoorCommon, AC_Pset_RenovationAndPhasing, MMI, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "ID-08-H" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, Pset_ManufacturerOccurrence, MMI, BaseQuantities
          1 x IFCGRID
      IFCBUILDINGSTOREY "Takplan" | elevation 491410.
        contains 3 elements
          1 x IFCSLAB | type IFCSLABTYPE "Tak 1400" | ROOF | names: "Tak enkelt -" | material: layers "Tak 1400" ("Tak" 1400.) | property sets: Pset_FireRatingProperties, Pset_SlabCommon, MMI, BaseQuantities, AC_Pset_RenovationAndPhasing
          1 x IFCSLAB | type IFCSLABTYPE "Dekke 250" | BASESLAB | names: "Dekke-" | material: layers "Dekke 250" ("Dekke" 250.) | property sets: Pset_SlabCommon, Pset_FireRatingProperties, Pset_CoveringCommon, AC_Pset_RenovationAndPhasing, MMI, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "Tak 900" | ROOF | names: "Tak enkelt -" | material: layers "Tak 900" ("Tak" 900.) | property sets: Pset_FireRatingProperties, Pset_SlabCommon, MMI, AC_Pset_RenovationAndPhasing, BaseQuantities

Types
  IFCWALLTYPE "Badromskabin 30 mm betong, 7 mm flislim, 8 mm flis 45" | 124 occurrences
  IFCWALLTYPE "Innervegg 175" | 26 occurrences
  IFCWALLTYPE "Innervegg 200" | 18 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 39 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 2 occurrences
  IFCWALLTYPE "Innervegg 20" | 9 occurrences
  IFCWALLTYPE "Innervegg 300" | 7 occurrences
  IFCWALLTYPE "Innervegg 130" | 3 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 3 occurrences
  IFCWALLTYPE "Yttervegg 200" | 54 occurrences
  IFCWALLTYPE "Yttervegg 240" | 2 occurrences
  IFCWALLTYPE "Yttervegg 75" | 1 occurrence
  IFCWALLTYPE "Yttervegg 265" | 7 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 3 occurrences
  IFCWALLTYPE "Yttervegg 260" | 1 occurrence
  IFCWALLTYPE "Yttervegg 350" | 4 occurrences
  IFCWALLTYPE "Yttervegg 220" | 1 occurrence
  IFCWALLTYPE "Innervegg 100" | 18 occurrences
  IFCWALLTYPE "Innervegg 450" | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 2 occurrences
  IFCWALLTYPE "Yttervegg 160" | 1 occurrence
  IFCWALLTYPE "Yttervegg 165" | 1 occurrence
  IFCWALLTYPE "Yttervegg 280" | 1 occurrence
  IFCWALLTYPE "Yttervegg 325" | 12 occurrences
  IFCWINDOWSTYLE "Vindu" | SINGLE_PANEL | 6 occurrences
  IFCDOORSTYLE "Skyvedør dobbel utenpåliggende" | DOUBLE_DOOR_SLIDING | 1 occurrence
  IFCWALLTYPE "Yttervegg 375" | 2 occurrences
  IFCWALLTYPE "Yttervegg 250" | 1 occurrence
  IFCDOORSTYLE "Leddport" | ROLLINGUP | 3 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 1 occurrence
  IFCWALLTYPE "Yttervegg 225" | 4 occurrences
  IFCWINDOWSTYLE "Vindu" | SINGLE_PANEL | 141 occurrences
  IFCWALLTYPE "Yttervegg 175" | 1 occurrence
  IFCDOORSTYLE "Dør med 2 sidefelt og overlys" | USERDEFINED | 6 occurrences
  IFCWALLTYPE "Innervegg 230" | 1 occurrence
  IFCWALLTYPE "Innervegg 275" | 8 occurrences
  IFCWALLTYPE "Yttervegg 255" | 1 occurrence
  IFCWALLTYPE "Yttervegg 275" | 3 occurrences
  IFCWALLTYPE "Yttervegg 150" | 2 occurrences
  IFCWINDOWSTYLE "Vindu to-fags" | USERDEFINED | 3 occurrences
  IFCWALLTYPE "Yttervegg 300" | 11 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCWINDOWSTYLE "Vindu to-fags" | DOUBLE_PANEL_VERTICAL | 2 occurrences
  IFCWALLTYPE "Innervegg 125" | 11 occurrences
  IFCWALLTYPE "Innervegg 150" | 22 occurrences
  IFCDOORSTYLE "Skyvedør utenpåliggende" | SLIDING_TO_RIGHT | 3 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 28 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCWALLTYPE "Innervegg 400" | 4 occurrences
  IFCWALLTYPE "Yttervegg 125" | 3 occurrences
  IFCDOORSTYLE "Dør med 2 sidefelt" | USERDEFINED | 3 occurrences
  IFCWINDOWSTYLE "Vindu" | SINGLE_PANEL | 1 occurrence
  IFCWALLTYPE "Innervegg 375" | 3 occurrences
  IFCWALLTYPE "Innervegg 475" | 1 occurrence
  IFCWALLTYPE "Innervegg 550" | 1 occurrence
  IFCWALLTYPE "Yttervegg 600" | 4 occurrences
  IFCWALLTYPE "Innervegg 290" | 1 occurrence
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCWINDOWSTYLE "Vindu to-fags" | DOUBLE_PANEL_VERTICAL | 1 occurrence
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCCURTAINWALLTYPE "Curtain Wall Type" | 1 occurrence
  IFCSLABTYPE "Dekke 300" | BASESLAB | 17 occurrences
  IFCSLABTYPE "Dekke 850" | BASESLAB | 1 occurrence
  IFCCOLUMNTYPE "Betong 350 x 200" | COLUMN | 2 occurrences
  IFCCOLUMNTYPE "Betong 275 x 220" | COLUMN | 1 occurrence
  IFCCOLUMNTYPE "Betong 410 x 200" | COLUMN | 1 occurrence
  IFCCOLUMNTYPE "Betong 350 x 185" | COLUMN | 1 occurrence
  IFCCOLUMNTYPE "Betong 300 x 300" | COLUMN | 1 occurrence
  IFCCOLUMNTYPE "Betong 285 x 200" | COLUMN | 1 occurrence
  IFCBEAMTYPE "Tre 350 x 200" | BEAM | 1 occurrence
  IFCBEAMTYPE "Tre 410 x 230" | BEAM | 1 occurrence
  IFCBEAMTYPE "Tre 410 x 240" | BEAM | 2 occurrences
  IFCBEAMTYPE "Tre 200 x 175" | BEAM | 2 occurrences
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCDOORSTYLE "Skyvedør utenpåliggende" | SLIDING_TO_LEFT | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 2 occurrences
  IFCDOORSTYLE "Dør metall" | SINGLE_SWING_LEFT | 1 occurrence
  IFCWALLTYPE "Innervegg 250" | 5 occurrences
  IFCDOORSTYLE "Dør metall" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCWALLTYPE "Innervegg 225" | 4 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 18 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 1 occurrence
  IFCDOORSTYLE "Dør med sidefelt på side 2" | SINGLE_SWING_LEFT | 14 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCWALLTYPE "Innervegg 220" | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 1 occurrence
  IFCDOORSTYLE "Dør metall" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCWALLTYPE "Påforingsvegg baderomskabin 70mm stålstende, 15 mm ultraboard, 15mm kryssfiner 100" | 95 occurrences
  IFCWALLTYPE "Korridorvegg stålstendere 95 mm, isolert, 15 mm ultraboard 15 mm kryssfiner 155" | 63 occurrences
  IFCWALLTYPE "Skillevegg beboerrom 2 stålstendere 70 mm, isolert, 15 mm ultraboard 15 mm kryssfiner 130" | 21 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 2 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 1 occurrence
  IFCDOORSTYLE "Skyvedør med pocketkarm" | USERDEFINED | 6 occurrences
  IFCWALLTYPE "Skillevegg avdeling 15 mm ultraboard, 15mm kryssfiner, 70mm stålstende, luftspalte 70mm, 70mm stålstende, 15 mm ultraboard, 15mm kryssfiner 270" | 15 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Stålpipe" | element type "Chimney" | USERDEFINED | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 6 occurrences
  IFCSLABTYPE "Dekke 200" | BASESLAB | 1 occurrence
  IFCSLABTYPE "Dekke 250" | BASESLAB | 33 occurrences
  IFCSLABTYPE "Dekke 220" | BASESLAB | 3 occurrences
  IFCSLABTYPE "Dekke 310" | BASESLAB | 1 occurrence
  IFCSLABTYPE "Dekke 520" | BASESLAB | 1 occurrence
  IFCWALLTYPE "Yttervegg 250 mm iso, 104 mm tegl utf., 50 mm luftsjikt, 70 mm murplate, 200 mm isolasjon 499" | 70 occurrences
  IFCDOORSTYLE "Dør med sidefelt på side 2" | SINGLE_SWING_RIGHT | 13 occurrences
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCWALLTYPE "Stålstender 95/95 mm, isolert, 2x2 gips 147" | 32 occurrences
  IFCWALLTYPE "Brannvegg Betong 200 mm 200" | 4 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 5 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 2 occurrences
  IFCWALLTYPE "Skillevegg beboerrom Forskutte stålstendere 95 mm, isolert, 2x13 mm gips, 6 mm kryssfiner 190" | 15 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 3 occurrences
  IFCWINDOWSTYLE "Vindu multi-rams horisontalt" | USERDEFINED | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 4 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 5 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 4 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 3 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 11 occurrences
  IFCWALLTYPE "Yttervegg 250 mm iso, 104 mm tegl utf., 20 mm luftsjikt, 250 mm isolasjon 429" | 8 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCDOORSTYLE "Foldedør multipanel" | FOLDING_TO_LEFT | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 1 occurrence
  IFCWALLTYPE "Skillevegg internt beboerrom stålstendere 70 mm, isolert,15 mm kryssfiner 100" | 19 occurrences
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 1 occurrence
  IFCWALLTYPE "Teglstein 300" | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 1 occurrence
  IFCSLABTYPE "Tak 1400" | ROOF | 1 occurrence
  IFCSLABTYPE "Tak 900" | ROOF | 1 occurrence

Property sets
  BaseQuantities | quantities | on 20 objects (20 IFCOPENINGELEMENT)
    Area = 1.304099999999998 [SQUARE_METRE]
    Depth = 499.0000000000001 [MILLI METRE]
    Height = 1610.000000000014 [MILLI METRE]
    Volume = 0.037430624 [CUBIC_METRE]
    Width = 809.9999999999881 [MILLI METRE]
  BaseQuantities | quantities | on 20 objects (20 IFCWINDOW)
    Area = 1.304099999999998 [SQUARE_METRE]
    Depth = 499.0000000000001 [MILLI METRE]
    GrossArea = 1.304099999999998 [SQUARE_METRE]
    Height = 1610.000000000014 [MILLI METRE]
    NetVolume = 0.037430624 [CUBIC_METRE]
    Perimeter = 4840.000000000004 [MILLI METRE]
    Volume = 0.037430624 [CUBIC_METRE]
    Width = 809.9999999999881 [MILLI METRE]
  BaseQuantities | quantities | on 11 objects (11 IFCOPENINGELEMENT)
    Area = 2.131100000000019 [SQUARE_METRE]
    Depth = 155. [MILLI METRE]
    Height = 2110.000000000014 [MILLI METRE]
    Volume = 0.1096357693389121 [CUBIC_METRE]
    Width = 1010.000000000005 [MILLI METRE]
  BaseQuantities | quantities | on 11 objects (11 IFCDOOR)
    Area = 2.131100000000019 [SQUARE_METRE]
    Depth = 155. [MILLI METRE]
    Height = 2110.000000000014 [MILLI METRE]
    NetVolume = 0.1096357693389121 [CUBIC_METRE]
    Perimeter = 6240.000000000037 [MILLI METRE]
    Volume = 0.1096357693389121 [CUBIC_METRE]
    Width = 1010.000000000005 [MILLI METRE]
  BaseQuantities | quantities | on 10 objects (10 IFCOPENINGELEMENT)
    Area = 1.304099999999998 [SQUARE_METRE]
    Depth = 499.0000000000001 [MILLI METRE]
    Height = 1610.000000000014 [MILLI METRE]
    Volume = 0.037430624 [CUBIC_METRE]
    Width = 810.0000000000023 [MILLI METRE]
  BaseQuantities | quantities | on 10 objects (10 IFCWINDOW)
    Area = 1.304099999999998 [SQUARE_METRE]
    Depth = 499.0000000000001 [MILLI METRE]
    GrossArea = 1.304099999999998 [SQUARE_METRE]
    Height = 1610.000000000014 [MILLI METRE]
    NetVolume = 0.037430624 [CUBIC_METRE]
    Perimeter = 4840.000000000032 [MILLI METRE]
    Volume = 0.037430624 [CUBIC_METRE]
    Width = 810.0000000000023 [MILLI METRE]
  BaseQuantities | quantities | on 8 objects (8 IFCOPENINGELEMENT)
    Area = 2.131100000000019 [SQUARE_METRE]
    Depth = 155. [MILLI METRE]
    Height = 2110.000000000014 [MILLI METRE]
    Volume = 0.1096357693389121 [CUBIC_METRE]
    Width = 1009.999999999991 [MILLI METRE]
  BaseQuantities | quantities | on 8 objects (8 IFCDOOR)
    Area = 2.131100000000019 [SQUARE_METRE]
    Depth = 155. [MILLI METRE]
    Height = 2110.000000000014 [MILLI METRE]
    NetVolume = 0.1096357693389121 [CUBIC_METRE]
    Perimeter = 6240.000000000009 [MILLI METRE]
    Volume = 0.1096357693389121 [CUBIC_METRE]
    Width = 1009.999999999991 [MILLI METRE]
  BaseQuantities: 1345 more contents on 1555 objects not shown
  Pset_FireRatingProperties | properties | on 1263 objects (725 IFCWALLSTANDARDCASE, 219 IFCDOOR, 155 IFCWINDOW, 59 IFCSLAB)
    FireResistanceRating = "" (IFCLABEL)
  Pset_WallCommon | properties | on 386 objects (383 IFCWALLSTANDARDCASE, 3 IFCWALL)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WallCommon | properties | on 336 objects (336 IFCWALLSTANDARDCASE)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WallCommon | properties | on 6 objects (6 IFCWALLSTANDARDCASE)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  AC_Pset_RenovationAndPhasing | properties | on 843 objects (479 IFCWALLSTANDARDCASE, 160 IFCDOOR, 143 IFCWINDOW, 59 IFCSLAB)
    Renovation Status = "New" (IFCLABEL)
  AC_Pset_RenovationAndPhasing | properties | on 342 objects (246 IFCWALLSTANDARDCASE, 59 IFCDOOR, 12 IFCWINDOW, 6 IFCBEAM)
    Renovation Status = "Existing" (IFCLABEL)
  AC_Pset_RenovationAndPhasing | properties | on 47 objects (39 IFCMEMBER, 8 IFCPLATE)
    Renovation Status = "Undefined" (IFCLABEL)
  MMI | properties | on 1266 objects (725 IFCWALLSTANDARDCASE, 219 IFCDOOR, 155 IFCWINDOW, 59 IFCSLAB)
    MMI = "Status ikke satt" (IFCLABEL)
    MMI dato = "-" (IFCLABEL)
    MMI signatur = "-" (IFCLABEL)
  Pset_DoorCommon | properties | on 171 objects (171 IFCDOOR)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_DoorCommon | properties | on 9 objects (9 IFCDOOR)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 2.143780000000004 (IFCPOSITIVERATIOMEASURE)
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_DoorCommon | properties | on 7 objects (7 IFCDOOR)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 2.143780000000003 (IFCPOSITIVERATIOMEASURE)
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_DoorCommon | properties | on 5 objects (5 IFCDOOR)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 2.143780000000002 (IFCPOSITIVERATIOMEASURE)
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_DoorCommon | properties | on 4 objects (4 IFCDOOR)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_DoorCommon | properties | on 2 objects (2 IFCDOOR)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 1.481962000000001 (IFCPOSITIVERATIOMEASURE)
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_DoorCommon | properties | on 2 objects (2 IFCDOOR)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 1.229718231400848 (IFCPOSITIVERATIOMEASURE)
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_DoorCommon | properties | on 2 objects (2 IFCDOOR)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 1.981089529339215 (IFCPOSITIVERATIOMEASURE)
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_DoorCommon: 17 more contents on 17 objects not shown
  Pset_ManufacturerOccurrence | properties | on 323 objects (171 IFCDOOR, 152 IFCWINDOW)
    SerialNumber = "NB! fylles ut under Classification and Properties" (IFCIDENTIFIER)
  Pset_ManufacturerOccurrence | properties | on 98 objects (48 IFCDOOR, 39 IFCMEMBER, 7 IFCPLATE, 3 IFCWINDOW)
    SerialNumber = "" (IFCIDENTIFIER)
  Pset_ManufacturerOccurrence | properties | on 1 object (1 IFCPLATE)
    SerialNumber = "Av" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 88 objects (88 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 0.8201000000000001 (IFCPOSITIVERATIOMEASURE)
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WindowCommon | properties | on 25 objects (25 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 2.2101 (IFCPOSITIVERATIOMEASURE)
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WindowCommon | properties | on 23 objects (23 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 1.7931 (IFCPOSITIVERATIOMEASURE)
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WindowCommon | properties | on 3 objects (3 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 0.7261843589456761 (IFCPOSITIVERATIOMEASURE)
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WindowCommon | properties | on 2 objects (2 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 3.656944000000109 (IFCPOSITIVERATIOMEASURE)
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WindowCommon | properties | on 2 objects (2 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 1.9321 (IFCPOSITIVERATIOMEASURE)
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 2.523133315830496 (IFCPOSITIVERATIOMEASURE)
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 2.497087777589623 (IFCPOSITIVERATIOMEASURE)
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WindowCommon: 10 more contents on 10 objects not shown
  Pset_PlateCommon | properties | on 8 objects (8 IFCPLATE)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_MemberCommon | properties | on 21 objects (21 IFCMEMBER)
    FireRating = "" (IFCLABEL)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_MemberCommon | properties | on 13 objects (13 IFCMEMBER)
    FireRating = "" (IFCLABEL)
    Slope = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_MemberCommon | properties | on 2 objects (2 IFCMEMBER)
    FireRating = "" (IFCLABEL)
    Slope = 89.99999852122066 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_MemberCommon | properties | on 1 object (1 IFCMEMBER)
    FireRating = "" (IFCLABEL)
    Slope = 1.039132686733819E-09 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_MemberCommon | properties | on 1 object (1 IFCMEMBER)
    FireRating = "" (IFCLABEL)
    Slope = 9.864637111146281E-07 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_MemberCommon | properties | on 1 object (1 IFCMEMBER)
    FireRating = "" (IFCLABEL)
    Slope = 1.039147366768655E-09 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_CoveringCommon | properties | on 57 objects (57 IFCSLAB)
    AcousticRating = "" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "" (IFCTEXT)
    FireRating = "" (IFCLABEL)
    FlammabilityRating = "" (IFCLABEL)
    FragilityRating = "" (IFCLABEL)
    Material = "" (IFCLABEL)
    Reference = "" (IFCIDENTIFIER)
    SurfaceSpreadOfFlame = "" (IFCLABEL)
  Pset_SlabCommon | properties | on 59 objects (59 IFCSLAB)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_ColumnCommon | properties | on 2 objects (2 IFCCOLUMN)
    FireRating = "" (IFCLABEL)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Betong 350 x 200" (IFCIDENTIFIER)
    Slope = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 1 object (1 IFCCOLUMN)
    FireRating = "" (IFCLABEL)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Betong 410 x 200" (IFCIDENTIFIER)
    Slope = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 1 object (1 IFCCOLUMN)
    FireRating = "" (IFCLABEL)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Betong 350 x 185" (IFCIDENTIFIER)
    Slope = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 1 object (1 IFCCOLUMN)
    FireRating = "" (IFCLABEL)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Betong 300 x 300" (IFCIDENTIFIER)
    Slope = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 1 object (1 IFCCOLUMN)
    FireRating = "" (IFCLABEL)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Betong 285 x 200" (IFCIDENTIFIER)
    Slope = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 1 object (1 IFCCOLUMN)
    FireRating = "" (IFCLABEL)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Betong 275 x 220" (IFCIDENTIFIER)
    Slope = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_BeamCommon | properties | on 2 objects (2 IFCBEAM)
    FireRating = "" (IFCLABEL)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Tre 410 x 240" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_BeamCommon | properties | on 2 objects (2 IFCBEAM)
    FireRating = "" (IFCLABEL)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Tre 200 x 175" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    FireRating = "" (IFCLABEL)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Tre 350 x 200" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    FireRating = "" (IFCLABEL)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Tre 410 x 230" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  AC_Pset_Dimension | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Height = 10000. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 930. (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 930. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
  Pset_CurtainWallCommon | properties | on 1 object (1 IFCCURTAINWALL)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_StairCommon | properties | on 2 objects (2 IFCSTAIR)
    FireRating = "" (IFCLABEL)
    NumberOfRiser = 15. (IFCCOUNTMEASURE)
    NumberOfTreads = 15. (IFCCOUNTMEASURE)
    RequiredHeadroom = 2100. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    RiserHeight = 180.6666666666653 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    FireRating = "" (IFCLABEL)
    NumberOfRiser = 3. (IFCCOUNTMEASURE)
    NumberOfTreads = 3. (IFCCOUNTMEASURE)
    RequiredHeadroom = 2100. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    RiserHeight = 180.6666666666653 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    FireRating = "" (IFCLABEL)
    NumberOfRiser = 14. (IFCCOUNTMEASURE)
    NumberOfTreads = 14. (IFCCOUNTMEASURE)
    RequiredHeadroom = 2100. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    RiserHeight = 180.6666666666653 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    FireRating = "" (IFCLABEL)
    NumberOfRiser = 16. (IFCCOUNTMEASURE)
    NumberOfTreads = 15. (IFCCOUNTMEASURE)
    RequiredHeadroom = 2100. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    RiserHeight = 180.6666666666653 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    FireRating = "" (IFCLABEL)
    NumberOfRiser = 7. (IFCCOUNTMEASURE)
    NumberOfTreads = 7. (IFCCOUNTMEASURE)
    RequiredHeadroom = 2100. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    RiserHeight = 180.6666666666653 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]