IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0, QuantityTakeOffAddOnView, SpaceBoundary2ndLevelAddOnView]"
Description: "Option [Elements to export: Visible elements (on all stories)]"
Description: "Option [Partial Structure Display: Entire Model]"
Description: "Option [IFC Domain: All]"
Description: "Option [Structural Function: All Elements]"
Description: "Option [Convert Grid elements: On]"
Description: "Option [Convert IFC Annotations and ARCHICAD 2D elements: Off]"
Description: "Option [Convert 2D symbols of Doors and Windows: Off]"
Description: "Option [Export geometries that Participates in Collision Detection only: Off]"
Description: "Option [Split complex elements: Off]"
Description: "Option [Material Preservation: Explode where necessary]"
Description: "Option [Elements in Solid Element Operations: Extruded/revolved]"
Description: "Option [Elements with junctions: Extruded/revolved without junctions]"
Description: "Option [IFC Model position: Survey Point and Project Origin]"
Description: "Option [Curtain Wall export mode: Container Element]"
Description: "Option [Railing export mode: Single Element]"
File name: "/Users/bpc91/Library/CloudStorage/OneDrive-SGArkitekterAS/NS Gprog ISY/Tester ISY Gprog/hus1.ifc"
Time stamp: "2024-02-14T15:34:29"
Author: "Arkitekten"
Organization: "Arkitektkontoret"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.09 : 18 Aug 2016"
Originating system: "IFC file generated by GRAPHISOFT ARCHICAD 25.0.0 NOR FULL Macintosh version (IFC add-on version: 6000 NOR FULL)."
Authorization: "Arkitekten"
Application: "ARCHICAD" version "25.0.0" identifier "IFC add-on version: 6000 NOR FULL" by Organization "GRAPHISOFT" id "GS" description "GRAPHISOFT"

People and organizations
  Person "Arkitekten" (roles: "Ark:"; postal address "Architect Postal Address": "Arkitektveien 19", "Arkitektbyen", "0000"; telecom address "Architect Telecom Address": telephone "000 000 00"; e-mail "arkitekt@arkitektfirma.no"; web page "www.arkitektfirma.no") of Organization "Arkitektkontoret" (postal address "Architect Postal Address": "Arkitektveien 19", "Arkitektbyen", "0000"; telecom address "Architect Telecom Address": telephone "000 000 00"; e-mail "arkitekt@arkitektfirma.no"; web page "www.arkitektfirma.no")
  Owner history of Person "Arkitekten" (roles: "Ark:"; postal address "Architect Postal Address": "Arkitektveien 19", "Arkitektbyen", "0000"; telecom address "Architect Telecom Address": telephone "000 000 00"; e-mail "arkitekt@arkitektfirma.no"; web page "www.arkitektfirma.no") of Organization "Arkitektkontoret" (postal address "Architect Postal Address": "Arkitektveien 19", "Arkitektbyen", "0000"; telecom address "Architect Telecom Address": telephone "000 000 00"; e-mail "arkitekt@arkitektfirma.no"; web page "www.arkitektfirma.no") | application "ARCHICAD" version "25.0.0" identifier "IFC add-on version: 6000 NOR FULL" by Organization "GRAPHISOFT" id "GS" description "GRAPHISOFT" | change NOCHANGE | created 1707917668 (2024-02-14T13:34:28Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  SOLIDANGLEUNIT: SQUAREDEGREE (conversion based)
  CURRENCY: NOK
  TIMEUNIT: Year (conversion based)
  MASSUNIT: KILO GRAM
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN
  ENERGYUNIT: MEGA JOULE
  THERMALCONDUCTANCEUNIT: derived
  SPECIFICHEATCAPACITYUNIT: derived
  MASSDENSITYUNIT: derived

Spatial structure
IFCPROJECT "Hus 1" | phase "Fase" | description "testpilot ISY"
  IFCSITE "Tomten" | latitude 59° 55′ 52.428″ | longitude 10° 42′ 27.972″ | elevation above sea level 0. | postal address: "Adresse", "#", "Sted", "0000", "Norge"
    IFCBUILDING "Bygningens navn" | postal address: "Adresse", "#", "Sted", "0000", "Norge" | description "Bygningstype"
      IFCBUILDINGSTOREY "1. Etasje" | elevation 1000.
        contains 16 elements
          1 x IFCSLAB | type IFCSLABTYPE "Betong påstøp, mebran, lim, flis 420" | BASESLAB | names: "Gulv på grunn, isolert" | material: layers "Betong påstøp, mebran, lim, flis" ("Flis - Gulv" 10., "Lim" 8., "Påstøp" 100., "Membran" 2., "Isolasjon - Markplate" 150., "Isolasjon - Markplate" 150.) | property sets: Pset_CoveringCommon, Pset_SlabCommon, Pset_FireRatingProperties, SKJEMADATA, AC_Pset_RenovationAndPhasing, BaseQuantities
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Trestender 198 mm stender, 48 mm Utf, 23 mm lekt, bordkl. inv.platekl. 316" | names: "VT-01" | material: layers "Trestender 198 mm stender, 48 mm Utf, 23 mm lekt, bordkl. inv.platekl." ("Bordkledning - Liggende" 22., "Lufting - Vertikalt" 23., "Vindsperre" 12., "Bindingsverk - Isolert" 198., "Dampsperre" 1., "Utforing - Isolert" 48., "Platekledning - Vegg" 12.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, SKJEMADATA, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-01" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, SKJEMADATA, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu" | object type "WINDOW" | names: "V-02" | property sets: Pset_WindowCommon, Pset_FireRatingProperties, SKJEMADATA, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu to-fags" | object type "WINDOW" | names: "V-01" | property sets: Pset_WindowCommon, Pset_FireRatingProperties, SKJEMADATA, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Innervegg 100" | names: "VT-03" | material: layers "Innervegg 100" ("Innervegg" 100.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, SKJEMADATA, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "ID-01" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, SKJEMADATA, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Trestender 73 mm, isolert, 1x platekl. to sider 97" | names: "VT-02" | material: layers "Trestender 73 mm, isolert, 1x platekl. to sider" ("Platekledning - Vegg" 12., "Stenderverk tre - Isolert" 73., "Platekledning - Vegg" 12.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, SKJEMADATA, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "ID-01" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, SKJEMADATA, AC_Pset_RenovationAndPhasing, BaseQuantities
          4 x IFCCOVERING | type IFCCOVERINGTYPE "sokkelbeslag 2 101 x 40" | names: "sokkelbeslag" | material: "Stål - Overflatebehandlet" | property sets: Pset_CoveringCommon, AC_Pset_Dimension, Pset_FireRatingProperties, SKJEMADATA, AC_Pset_RenovationAndPhasing, BaseQuantities
        IFCSPACE "101" | long name "gang" | INTERNAL
        IFCSPACE "102" | long name "rom 3" | INTERNAL
        IFCSPACE "103" | long name "rom 2" | INTERNAL

Types
  IFCSLABTYPE "Betong påstøp, mebran, lim, flis 420" | BASESLAB | 1 occurrence
  IFCWALLTYPE "Trestender 198 mm stender, 48 mm Utf, 23 mm lekt, bordkl. inv.platekl. 316" | 4 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCWINDOWSTYLE "Vindu" | DOUBLE_PANEL_HORIZONTAL | 1 occurrence
  IFCWINDOWSTYLE "Vindu to-fags" | USERDEFINED | 1 occurrence
  IFCWALLTYPE "Innervegg 100" | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 1 occurrence
  IFCWALLTYPE "Trestender 73 mm, isolert, 1x platekl. to sider 97" | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 1 occurrence
  IFCCOVERINGTYPE "sokkelbeslag 2 101 x 40" | 4 occurrences | property sets: Pset_CoveringCommon

Property sets
  BaseQuantities | quantities | on 2 objects (2 IFCCOVERING)
    GrossArea = 0.413999 [SQUARE_METRE]
    NetArea = 0.413999 [SQUARE_METRE]
  BaseQuantities | quantities | on 2 objects (2 IFCCOVERING)
    GrossArea = 0.615999 [SQUARE_METRE]
    NetArea = 0.615999 [SQUARE_METRE]
  BaseQuantities | quantities | on 1 object (1 IFCSITE)
    GrossArea = 0. [SQUARE_METRE]
    GrossPerimeter = 0. [MILLI METRE]
  BaseQuantities | quantities | on 1 object (1 IFCBUILDING)
    GrossFloorArea = 25.361403073 [SQUARE_METRE]
  BaseQuantities | quantities | on 1 object (1 IFCBUILDINGSTOREY)
    GrossFloorArea = 25.361403073 [SQUARE_METRE]
    GrossHeight = 2700. [MILLI METRE]
    Height = 2700. [MILLI METRE]
    NetHeight = 2700. [MILLI METRE]
  BaseQuantities | quantities | on 1 object (1 IFCSLAB)
    GrossArea = 24. [SQUARE_METRE]
    GrossVolume = 10.08 [CUBIC_METRE]
    NetArea = 24. [SQUARE_METRE]
    NetVolume = 10.08 [CUBIC_METRE]
    Perimeter = 20000. [MILLI METRE]
    Width = 420. [MILLI METRE]
  BaseQuantities | quantities | on 1 object (1 IFCOPENINGELEMENT)
    Area = 2.1311 [SQUARE_METRE]
    Depth = 316. [MILLI METRE]
    Height = 2110. [MILLI METRE]
    Volume = 0.109635769339 [CUBIC_METRE]
    Width = 1010. [MILLI METRE]
  BaseQuantities | quantities | on 1 object (1 IFCWALLSTANDARDCASE)
    GrossFootprintArea = 0.923818055372 [SQUARE_METRE]
    GrossSideArea = 10.284943 [SQUARE_METRE]
    GrossVolume = 3.35571592 [CUBIC_METRE]
    Height = 2700. [MILLI METRE]
    Length = 3798. [MILLI METRE]
    NetFootprintArea = 0.923818055372 [SQUARE_METRE]
    NetSideArea = 8.154348 [SQUARE_METRE]
    NetVolume = 2.6823671 [CUBIC_METRE]
    Width = 316. [MILLI METRE]
  BaseQuantities: 17 more contents on 17 objects not shown
  Pset_CoveringCommon | properties | on 4 objects (4 IFCCOVERING)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    Material = "sokkelbeslag 2" (IFCLABEL)
  Pset_CoveringCommon | properties | on 1 object (1 IFCSLAB)
    AcousticRating = "" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "" (IFCTEXT)
    FireRating = "" (IFCLABEL)
    FlammabilityRating = "" (IFCLABEL)
    FragilityRating = "" (IFCLABEL)
    Material = "" (IFCLABEL)
    Reference = "" (IFCIDENTIFIER)
    SurfaceSpreadOfFlame = "" (IFCLABEL)
  Pset_CoveringCommon | properties | on 1 type object
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_FireRatingProperties | properties | on 14 objects (5 IFCWALLSTANDARDCASE, 4 IFCCOVERING, 3 IFCDOOR, 1 IFCSLAB)
    FireResistanceRating = "" (IFCLABEL)
  Pset_FireRatingProperties | properties | on 1 object (1 IFCWINDOW)
    FireResistanceRating = "EI-30" (IFCLABEL)
    IsCombustible = TRUE (IFCBOOLEAN)
  Pset_FireRatingProperties | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    FireResistanceRating = "EI30" (IFCLABEL)
    IsCombustible = TRUE (IFCBOOLEAN)
  SKJEMADATA | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    Beskrivelse = "" (IFCLABEL)
    Brannkrav = "" (IFCLABEL)
    Etasje = "1. Etasje" (IFCLABEL)
    ID = "VT-01" (IFCLABEL)
    Linket endring = "" (IFCLABEL)
    Lydkrav = "" (IFCLABEL)
    Størrelse = "316 x 2 700" (IFCLABEL)
    U-verdi = "" (IFCLABEL)
  SKJEMADATA | properties | on 4 objects (4 IFCCOVERING)
    Beskrivelse = "" (IFCLABEL)
    Brannkrav = "" (IFCLABEL)
    Etasje = "1. Etasje" (IFCLABEL)
    ID = "sokkelbeslag" (IFCLABEL)
    Linket endring = "" (IFCLABEL)
    Lydkrav = "" (IFCLABEL)
    Størrelse = "101 x 40" (IFCLABEL)
    U-verdi = "" (IFCLABEL)
  SKJEMADATA | properties | on 1 object (1 IFCSLAB)
    Beskrivelse = "" (IFCLABEL)
    Brannkrav = "" (IFCLABEL)
    Etasje = "1. Etasje" (IFCLABEL)
    ID = "Gulv på grunn, isolert" (IFCLABEL)
    Linket endring = "" (IFCLABEL)
    Lydkrav = "" (IFCLABEL)
    Størrelse = "x 420" (IFCLABEL)
    U-verdi = "" (IFCLABEL)
  SKJEMADATA | properties | on 1 object (1 IFCDOOR)
    Annmerkning = "" (IFCLABEL)
    Brannkrav = "" (IFCLABEL)
    Dørblad = "" (IFCLABEL)
    Etasje = "1. Etasje" (IFCLABEL)
    Funksjon = "" (IFCLABEL)
    Glass = "" (IFCLABEL)
    Hengsler = "" (IFCLABEL)
    Håndtak = "" (IFCLABEL)
    Håndtaksoverflate = "" (IFCLABEL)
    ID = "YD-01" (IFCLABEL)
    Karm = "" (IFCLABEL)
    Karmoverflate = "" (IFCLABEL)
    Linket endring = "" (IFCLABEL)
    Lydkrav = "" (IFCLABEL)
    Låskasse = "" (IFCLABEL)
    Oveflate anslagside = "" (IFCLABEL)
    Ramme = "" (IFCLABEL)
    Rammeoverflate = "" (IFCLABEL)
    Slagretning = "V" (IFCLABEL)
    Størrelse = "990 x 2 090" (IFCLABEL)
    Terskel = "-" (IFCLABEL)
    Tilleggslås = "" (IFCLABEL)
    U-verdi = "" (IFCLABEL)
    Veggtykkelse = "316" (IFCLABEL)
  SKJEMADATA | properties | on 1 object (1 IFCWINDOW)
    Annmerkning = "" (IFCLABEL)
    Brannkrav = "" (IFCLABEL)
    Etasje = "1. Etasje" (IFCLABEL)
    Funksjon = "" (IFCLABEL)
    Glass = "" (IFCLABEL)
    Hengsler = "" (IFCLABEL)
    Håndtak = "" (IFCLABEL)
    Håndtaksoverflate = "" (IFCLABEL)
    ID = "V-02" (IFCLABEL)
    Karm = "" (IFCLABEL)
    Karmoverflate = "" (IFCLABEL)
    Linket endring = "" (IFCLABEL)
    Lydkrav = "" (IFCLABEL)
    Låskasse = "" (IFCLABEL)
    Oveflate anslagside = "" (IFCLABEL)
    Ramme = "" (IFCLABEL)
    Rammeoverflate = "" (IFCLABEL)
    Størrelse = "490 x 490" (IFCLABEL)
    Tilleggslås = "" (IFCLABEL)
    U-verdi = "" (IFCLABEL)
    Veggtykkelse = "316" (IFCLABEL)
  SKJEMADATA | properties | on 1 object (1 IFCWINDOW)
    Annmerkning = "anmerkning" (IFCLABEL)
    Brannkrav = "EI-30" (IFCLABEL)
    Etasje = "1. Etasje" (IFCLABEL)
    Funksjon = "funksjon" (IFCLABEL)
    Glass = "glass" (IFCLABEL)
    Hengsler = "hengsler" (IFCLABEL)
    Håndtak = "" (IFCLABEL)
    Håndtaksoverflate = "" (IFCLABEL)
    ID = "V-01" (IFCLABEL)
    Karm = "karm" (IFCLABEL)
    Karmoverflate = "overflate karm" (IFCLABEL)
    Linket endring = "" (IFCLABEL)
    Lydkrav = "33dB" (IFCLABEL)
    Låskasse = "låskasse" (IFCLABEL)
    Oveflate anslagside = "overflate anslagside" (IFCLABEL)
    Ramme = "ramme" (IFCLABEL)
    Rammeoverflate = "overflate ramme" (IFCLABEL)
    Størrelse = "1 190 x 1 190" (IFCLABEL)
    Tilleggslås = "tilleggslås" (IFCLABEL)
    U-verdi = "1,0" (IFCLABEL)
    Veggtykkelse = "316" (IFCLABEL)
  SKJEMADATA | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Beskrivelse = "" (IFCLABEL)
    Brannkrav = "" (IFCLABEL)
    Etasje = "1. Etasje" (IFCLABEL)
    ID = "VT-03" (IFCLABEL)
    Linket endring = "" (IFCLABEL)
    Lydkrav = "" (IFCLABEL)
    Størrelse = "100 x 2 400" (IFCLABEL)
    U-verdi = "" (IFCLABEL)
  SKJEMADATA | properties | on 1 object (1 IFCDOOR)
    Annmerkning = "" (IFCLABEL)
    Brannkrav = "" (IFCLABEL)
    Dørblad = "" (IFCLABEL)
    Etasje = "1. Etasje" (IFCLABEL)
    Funksjon = "" (IFCLABEL)
    Glass = "" (IFCLABEL)
    Hengsler = "" (IFCLABEL)
    Håndtak = "" (IFCLABEL)
    Håndtaksoverflate = "" (IFCLABEL)
    ID = "ID-01" (IFCLABEL)
    Karm = "" (IFCLABEL)
    Karmoverflate = "" (IFCLABEL)
    Linket endring = "" (IFCLABEL)
    Lydkrav = "" (IFCLABEL)
    Låskasse = "" (IFCLABEL)
    Oveflate anslagside = "" (IFCLABEL)
    Ramme = "" (IFCLABEL)
    Rammeoverflate = "" (IFCLABEL)
    Slagretning = "H" (IFCLABEL)
    Størrelse = "890 x 2 090" (IFCLABEL)
    Terskel = "-" (IFCLABEL)
    Tilleggslås = "" (IFCLABEL)
    U-verdi = "" (IFCLABEL)
    Veggtykkelse = "100" (IFCLABEL)
  SKJEMADATA: 2 more contents on 2 objects not shown
  AC_Pset_RenovationAndPhasing | properties | on 19 objects (6 IFCWALLSTANDARDCASE, 4 IFCCOVERING, 3 IFCDOOR, 3 IFCSPACE)
    Renovation Status = "New" (IFCLABEL)
  Pset_WallCommon | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    AcousticRating = "" (IFCLABEL)
    Combustible = TRUE (IFCBOOLEAN)
    FireRating = "EI30" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_DoorCommon | properties | on 2 objects (2 IFCDOOR)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 0.071068 (IFCPOSITIVERATIOMEASURE)
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    AcousticRating = "33dB" (IFCLABEL)
    FireExit = FALSE (IFCBOOLEAN)
    FireRating = "EI-30" (IFCLABEL)
    GlazingAreaFraction = 0.842724 (IFCPOSITIVERATIOMEASURE)
    IsExternal = TRUE (IFCBOOLEAN)
    SecurityRating = "sikkerhetsklasse" (IFCLABEL)
    SmokeStop = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  AC_Pset_Dimension | properties | on 2 objects (2 IFCCOVERING)
    Area = "1,16" (IFCLABEL)
    Height = "40" (IFCLABEL)
    Length = "4 200" (IFCLABEL)
  AC_Pset_Dimension | properties | on 2 objects (2 IFCCOVERING)
    Area = "1,72" (IFCLABEL)
    Height = "40" (IFCLABEL)
    Length = "6 200" (IFCLABEL)
  Pset_SpaceCommon | properties | on 3 objects (3 IFCSPACE)
    Category = "Opphold" (IFCLABEL)
    CeilingCovering = "" (IFCLABEL)
    ConcealedCeiling = FALSE (IFCBOOLEAN)
    ConcealedFlooring = FALSE (IFCBOOLEAN)
    FloorCovering = "" (IFCLABEL)
    GrossPlannedArea = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    NetPlannedArea = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    PubliclyAccessible = FALSE (IFCBOOLEAN)
    Reference = "Undefined" (IFCIDENTIFIER)
    SkirtingBoard = "" (IFCLABEL)
    WallCovering = "" (IFCLABEL)
  Pset_SpaceOccupancyRequirements | properties | on 3 objects (3 IFCSPACE)
    AreaPerOccupant = 0. (IFCAREAMEASURE) [SQUARE_METRE]