IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0, QuantityTakeOffAddOnView, SpaceBoundary2ndLevelAddOnView]"
Description: "Option [Elements to export: Visible elements (on all stories)]"
Description: "Option [Partial Structure Display: Entire Model]"
Description: "Option [IFC Domain: Custom]"
Description: "Option [Structural Function: All Elements]"
Description: "Option [Convert Grid elements: On]"
Description: "Option [Convert IFC Annotations and Archicad 2D elements: Off]"
Description: "Option [Convert 2D symbols of Doors and Windows: On]"
Description: "Option [Export geometries that Participates in Collision Detection only: On]"
Description: "Option [Split complex elements: Off]"
Description: "Option [Material Preservation: Explode where necessary]"
Description: "Option [Elements in Solid Element Operations: Extruded/revolved]"
Description: "Option [Elements with junctions: Extruded/revolved without junctions]"
Description: "Option [IFC Model position: Survey Point and Project Origin]"
Description: "Option [Curtain Wall export mode: Container Element]"
Description: "Option [Railing export mode: Single Element]"
File name: "/Volumes/Prosjekter i Arbeid/9520-Skeisvang vgs/5-DISTRIBUSJON/51 Publish/522-Detaljprosjekt/IFC/Skeisvang_vgs_ARK.ifc"
Time stamp: "2024-02-28T11:27:18"
Author: "Arkitekten"
Organization: "Arkitektkontoret"
Preprocessor: "DDS_IFC v3.0"
Originating system: "IFC file generated by Graphisoft Archicad 26.0.0 NOR FULL Macintosh version (IFC add-on version: 6016 NOR FULL)."
Authorization: "Arkitekten"
Application: "Archicad" version "26.0.0" identifier "IFC add-on version: 6016 NOR FULL" by Organization "Graphisoft" id "GS" description "Graphisoft"

People and organizations
  Person "Arkitekten" (roles: "Ark:"; postal address "Architect Postal Address": "Arkitektveien 19", "Arkitektbyen", "0000"; telecom address "Architect Telecom Address": telephone "000 000 00"; e-mail "arkitekt@arkitektfirma.no"; web page "www.arkitektfirma.no") of Organization "Arkitektkontoret" (postal address "Architect Postal Address": "Arkitektveien 19", "Arkitektbyen", "0000"; telecom address "Architect Telecom Address": telephone "000 000 00"; e-mail "arkitekt@arkitektfirma.no"; web page "www.arkitektfirma.no")
  Owner history of Person "Arkitekten" (roles: "Ark:"; postal address "Architect Postal Address": "Arkitektveien 19", "Arkitektbyen", "0000"; telecom address "Architect Telecom Address": telephone "000 000 00"; e-mail "arkitekt@arkitektfirma.no"; web page "www.arkitektfirma.no") of Organization "Arkitektkontoret" (postal address "Architect Postal Address": "Arkitektveien 19", "Arkitektbyen", "0000"; telecom address "Architect Telecom Address": telephone "000 000 00"; e-mail "arkitekt@arkitektfirma.no"; web page "www.arkitektfirma.no") | application "Archicad" version "26.0.0" identifier "IFC add-on version: 6016 NOR FULL" by Organization "Graphisoft" id "GS" description "Graphisoft" | change NOCHANGE | created 1709112413 (2024-02-28T09:26:53Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  SOLIDANGLEUNIT: SQUAREDEGREE (conversion based)
  CURRENCY: NOK
  TIMEUNIT: Year (conversion based)
  MASSUNIT: KILO GRAM
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN
  ENERGYUNIT: MEGA JOULE
  THERMALCONDUCTANCEUNIT: derived
  SPECIFICHEATCAPACITYUNIT: derived
  MASSDENSITYUNIT: derived

Spatial structure
IFCPROJECT "SKEISVANG VGS." | phase "Detaljprosjekt" | description "Prosjektbeskrivelse"
  IFCSITE "Tomten" | latitude 59° 55′ 52.428″ | longitude 10° 42′ 27.972″ | elevation above sea level 0. | postal address: "Rogalandgata 197,", "#", "Haugesund", "5518", "Norge"
    IFCBUILDING "Bygningens navn" | postal address: "Rogalandgata 197,", "#", "Haugesund", "5518", "Norge" | description "Bygningstype"
      IFCBUILDINGSTOREY "Hav" | long name "0. 1. Etasje" | elevation 0.
        contains 3 elements
          1 x IFCSLAB | type IFCSLABTYPE "Yttervegg HOVEDBYGG 450" | BASESLAB | names: "Dekke-" | material: layers "Yttervegg HOVEDBYGG 450" ("Yttervegg HOVEDBYGG" 449.9999999999993) | property sets: Pset_CoveringCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, TULLETE TEST, Pset_SlabCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Kart - koordinatobjekt 1" | names: "Stol-" | property sets: MMI, Skeisvang Pset: TEST 01 - ifcProject, AC_Pset_Dimension, tullball, TULLETE TEST, AC_Pset_RenovationAndPhasing
          1 x IFCSLAB | type IFCSLABTYPE "Stein - Skiferheller 300" | BASESLAB | names: "Dekke-" | material: layers "Stein - Skiferheller 300" ("Stein - Skiferheller" 299.9999999999972) | property sets: Pset_CoveringCommon, Pset_FireRatingProperties, MMI, Pset_SlabCommon, TESTTEST, TULLETE TEST
      IFCBUILDINGSTOREY "Kjellerplan Bygg C" | elevation 22900.
        contains 45 elements
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall Type" | names: "CurtainWall-" | parts: 64 IFCMEMBER, 24 IFCPLATE | property sets: Pset_CurtainWallCommon, MMI, TULLETE TEST, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg HOVEDBYGG 275" | names: "VT-" | material: layers "Yttervegg HOVEDBYGG 275" ("Yttervegg HOVEDBYGG" 275.) | property sets: Pset_FireRatingProperties, MMI, Pset_WallCommon, TESTTEST, TULLETE TEST, Skeisvang Pset: TEST 01 - ifcProject
          42 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Stål - Rustfritt 10" | names: "VT-" | material: layers "Stål - Rustfritt 10" ("Stål - Rustfritt" 10.) | property sets: Pset_WallCommon, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, MMI, TULLETE TEST
      IFCBUILDINGSTOREY "Kjellerplan Bygg A og B" | elevation 24000.
        contains 947 elements
          16 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Innervegg tegl 104" | names: "VT-" | material: layers "Innervegg tegl 104" ("Innervegg tegl" 104.) | property sets: Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, Pset_WallCommon, MMI, TULLETE TEST, TESTTEST
          15 x IFCCOVERING | type IFCCOVERINGTYPE "Systemhimling - 60x60 50" | CEILING | names: "Systemhimling 600 x 600 E-kant", "Parafon 60 x 60", "Fast himling" | material: "Systemhimling - 60x60" | property sets: Pset_CoveringCommon, AC_Pset_Dimension, MMI, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, AC_Pset_RenovationAndPhasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "*9520 - IV 02 - Stålstender 100mm, uisolert, 2x + 1x platekl. to sider 139" | names: "skjørt" | material: layers "*9520 - IV 02 - Stålstender 100mm, uisolert, 2x + 1x platekl. to sider" ("Gipsplate - Vegg" 13., "Gipsplate - Vegg" 13., "Stenderverk stål - Uisolert" 100., "Gipsplate - Vegg" 13.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "* PV03 Stålstender 100mm, påforingt, 2x platekl. en side 122" | names: "PV03" | material: layers "* PV03 Stålstender 100mm, påforingt, 2x platekl. en side" ("Platekledning - Vegg" 10., "OSB-plate" 12., "Stenderverk stål - Uisolert" 100.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, tullball
          10 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "*9520 - IV 02 - Trelekt 50mm, isolert, 1x platekl. en side 63" | names: "IV11" | material: layers "*9520 - IV 02 - Trelekt 50mm, isolert, 1x platekl. en side" ("Gipsplate - Vegg" 13., "Stenderverk tre - Isolert" 50.) | property sets: AC_Pset_RenovationAndPhasing, TULLETE TEST, BaseQuantities, tullball, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Teglstein 104" | names: "VT-" | material: layers "Teglstein 104" ("Teglstein" 104.) | property sets: Pset_FireRatingProperties, Pset_WallCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, TESTTEST
          55 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 1 150" | names: "VT-" | material: layers "Yttervegg 1 150" ("Yttervegg 1" 150.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, tullball
          18 x IFCCOVERING | type IFCCOVERINGTYPE "Stenderverk stål - Isolert 50" | CEILING | names: "fast gipshimling", "Dekke-" | material: "Stenderverk stål - Isolert" | property sets: AC_Pset_Dimension, Pset_FireRatingProperties, MMI, Pset_CoveringCommon, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST
          18 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "*9520 - IV 05 - Plate 25 mm med 50 mm luft til eletrisk 75" | names: "VT-" | material: layers "*9520 - IV 05 - Plate 25 mm med 50 mm luft til eletrisk" ("Platekledning - Vegg" 25.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST, MMI
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "*9520 - IV 05 - Plate 25 mm med 30 luft 55" | names: "VT-" | material: layers "*9520 - IV 05 - Plate 25 mm med 30 luft" ("Platekledning - Vegg" 25.) | property sets: Pset_WallCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, TESTTEST, TULLETE TEST
          9 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Aluminium" | names: "Terreng-01" | material: "Aluminium" | property sets: AC_Pset_RenovationAndPhasing, Skeisvang Pset: TEST 01 - ifcProject, AC_Pset_Dimension
          6 x IFCCOVERING | type IFCCOVERINGTYPE "Systemhimling - 60x120 50" | CEILING | names: "Spilehimling flåter 600 x 1200" | material: "Systemhimling - 60x120" | property sets: Pset_CoveringCommon, AC_Pset_Dimension, MMI, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST
          18 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 1 200" | names: "VT-" | material: layers "Yttervegg 1 200" ("Yttervegg 1" 200.) | property sets: Pset_FireRatingProperties, MMI, Pset_WallCommon, Skeisvang Pset: TEST 01 - ifcProject, BaseQuantities, tullball
          34 x IFCBEAM | type IFCBEAMTYPE "Stål 50 x 10" | object type "BEAM" | names: "B-", "håndløper hovedtrapp vestibyle" | material: "Stål" | property sets: Pset_BeamCommon, MMI, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, tullball, AC_Pset_RenovationAndPhasing
          9 x IFCSLAB | type IFCSLABTYPE "Stål 120" | BASESLAB | names: "håndløper hovedtrapp vestibyle" | material: layers "Stål 120" ("Stål" 120.000000000001) | property sets: Pset_FireRatingProperties, Pset_CoveringCommon, Pset_SlabCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST
          18 x IFCSLAB | type IFCSLABTYPE "Stål 60" | BASESLAB | names: "håndløper hovedtrapp vestibyle" | material: layers "Stål 60" ("Stål" 59.99999999999872) | property sets: Pset_SlabCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, TULLETE TEST, Pset_CoveringCommon
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "*9520 - IV 07 Lydvegg fasade 188" | names: "IV21" | material: layers "*9520 - IV 07 Lydvegg fasade" ("Gipsplate - Vegg" 13., "Stenderverk tre - Isolert" 150.) | property sets: MMI, Pset_WallCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu variabelt" | object type "WINDOW" | names: "YVC.000" | property sets: Pset_FireRatingProperties, Pset_WindowCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, tullball
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "*9520 - IV 02 - Stålstender 50mm, isolert, 1x platekl. en side 73" | names: "PV?" | material: layers "*9520 - IV 02 - Stålstender 50mm, isolert, 1x platekl. en side" ("Gipsplate - Vegg" 13., "Stenderverk stål - Isolert" 50.) | property sets: MMI, Pset_WallCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          2 x IFCWALL | type IFCWALLTYPE "* IV 05 - 60 dB : 3x13 mm gips, 2x100mm stålstender, 3x13mm gips 288" | names: "IV05" | parts: 16 IFCBUILDINGELEMENTPART | property sets: Pset_WallCommon, MMI, Pset_FireRatingProperties, TULLETE TEST, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "IDC.016" | property sets: Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, Pset_DoorCommon, TESTTEST, TULLETE TEST, tullball
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "* IV 09 - RENHOLD - 1 plate gips+1 plate OSB-plate, Stålstender 100mm, isolert, 2x platekl. gips 152" | names: "IV09" | material: layers "* IV 09 - RENHOLD - 1 plate gips+1 plate OSB-plate, Stålstender 100mm, isolert, 2x platekl. gips" ("Gipsplate - Vegg" 13., "Gipsplate - Vegg" 13., "Stenderverk stål - Isolert" 100., "Gipsplate - Vegg" 13., "Gipsplate - Vegg" 13.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, TULLETE TEST, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, MMI
          9 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "IDC.014", "IDC.001", "YD-" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, MMI, TESTTEST, BaseQuantities
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "9520 - YV 05 - 148 mm trestender 150" | names: "VT-" | material: layers "9520 - YV 05 - 148 mm trestender" ("Stenderverk tre YTTERVEGG - Isolert" 150.) | property sets: Pset_FireRatingProperties, MMI, Pset_WallCommon, AC_Pset_RenovationAndPhasing, tullball, Skeisvang Pset: TEST 01 - ifcProject
          11 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "* IV 01 - Stålstender 100mm, isolert, 1x platekl. to sider 126" | names: "IV01" | material: layers "* IV 01 - Stålstender 100mm, isolert, 1x platekl. to sider" ("Gipsplate - Vegg" 13., "Stenderverk stål - Isolert" 100., "Gipsplate - Vegg" 13.) | property sets: Pset_FireRatingProperties, Pset_WallCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "IDC.015" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, MMI, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "IDC.008" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, tullball, TULLETE TEST, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject
          16 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "*9520 - IV 07 - Teglvegg m/luft 134" | names: "VT-" | material: layers "*9520 - IV 07 - Teglvegg m/luft" ("Innervegg tegl" 104.) | property sets: Pset_WallCommon, MMI, Pset_FireRatingProperties, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, tullball
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "*9520 - IV 02 - Stålstender 100mm, isolert, 1x platekl. en side 113" | names: "VT-" | material: layers "*9520 - IV 02 - Stålstender 100mm, isolert, 1x platekl. en side" ("Gipsplate - Vegg" 13., "Stenderverk stål - Isolert" 100.) | property sets: Pset_WallCommon, MMI, Pset_FireRatingProperties, TULLETE TEST, TESTTEST, tullball
          14 x IFCCOVERING | type IFCCOVERINGTYPE "Teglstein 5" | CEILING | names: "tegl over åpning" | material: "Teglstein" | property sets: Pset_CoveringCommon, AC_Pset_Dimension, Pset_FireRatingProperties, MMI, TESTTEST, BaseQuantities
          2 x IFCWALL | type IFCWALLTYPE "*9520 - IV 07 - Dobbel Teglvegg m/luft 230" | names: "VT-" | parts: 4 IFCBUILDINGELEMENTPART | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, BaseQuantities, AC_Pset_RenovationAndPhasing
          33 x IFCCOLUMN | type IFCCOLUMNTYPE "Petal Kontur K7 600 600 x 14" | object type "COLUMN" | names: "YV09", "S-" | material: "0% 27718788" | property sets: Pset_FireRatingProperties, MMI, Pset_ColumnCommon, TULLETE TEST, TESTTEST, tullball
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "*9520 - IV 02B - Stålstender 50mm, isolert, 2x platekl. en side 86" | names: "IV18" | material: layers "*9520 - IV 02B - Stålstender 50mm, isolert, 2x platekl. en side" ("Gipsplate - Vegg" 13., "Gipsplate - Vegg" 13., "Stenderverk stål - Isolert" 50.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, MMI, TESTTEST, tullball
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Maling 10" | names: "VT-" | material: layers "Maling 10" ("Maling" 10.) | property sets: Pset_WallCommon, MMI, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, TULLETE TEST
          4 x IFCCOLUMN | type IFCCOLUMNTYPE "Petal Kontur K7 300 300 x 14" | object type "COLUMN" | names: "YV09" | material: "0% 27718788" | property sets: Skeisvang Pset: TEST 01 - ifcProject, MMI, Pset_FireRatingProperties, Pset_ColumnCommon, TULLETE TEST, AC_Pset_RenovationAndPhasing
          25 x IFCCOVERING | type IFCCOVERINGTYPE "Gulvbelegg 3" | FLOORING | names: "Banebelegg" | material: "Gulvbelegg" | property sets: Pset_FireRatingProperties, AC_Pset_Dimension, Pset_CoveringCommon, MMI, AC_Pset_RenovationAndPhasing, Skeisvang Pset: TEST 01 - ifcProject
          1 x IFCWALL | type IFCWALLTYPE "9520 - YV 03 - 200 mm trestender, , murplate, tegl 420" | names: "YV03" | parts: 4 IFCBUILDINGELEMENTPART | property sets: Pset_WallCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, MMI, TULLETE TEST, TESTTEST
          9 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "* PV 02- Påforing stålstender 100mm 2 lag gips 136" | names: "IV19", "PV02", "YV?" | material: layers "* PV 02- Påforing stålstender 100mm 2 lag gips" ("Gipsplate - Vegg" 13., "Gipsplate - Vegg" 13., "Stenderverk stål - Isolert" 100.) | property sets: Pset_WallCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, Pset_FireRatingProperties, TULLETE TEST
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "* IV 06 - dusj_Stålstender 100mm, isolert, 1x + 2x platekl. to sider (1) 135" | names: "IV06" | material: layers "* IV 06 - dusj_Stålstender 100mm, isolert, 1x + 2x platekl. to sider (1)" ("Gipsplate - Vegg" 13., "Stenderverk stål - Isolert" 100., "OSB-plate" 12., "Platekledning - Vegg" 10.) | property sets: Pset_FireRatingProperties, Pset_WallCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "IDC.002" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, MMI, AC_Pset_RenovationAndPhasing, TULLETE TEST, tullball
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "* IV 07 - dusj_Stålstender 100mm, isolert, 2x platekl. to sider 148" | names: "IV07" | material: layers "* IV 07 - dusj_Stålstender 100mm, isolert, 2x platekl. to sider" ("Gipsplate - Vegg" 13., "Gipsplate - Vegg" 13., "Stenderverk stål - Isolert" 100., "OSB-plate" 12., "Platekledning - Vegg" 10.) | property sets: Pset_FireRatingProperties, MMI, TESTTEST, Pset_WallCommon, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "*9520 - IV 02 - dusj_Stålstender 50mm, påforingt, 2x platekl. en side 72" | names: "PV04" | material: layers "*9520 - IV 02 - dusj_Stålstender 50mm, påforingt, 2x platekl. en side" ("Platekledning - Vegg" 10., "OSB-plate" 12., "Stenderverk stål - Uisolert" 50.) | property sets: Pset_FireRatingProperties, Pset_WallCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "IDC.002" | property sets: Pset_DoorCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, tullball, TESTTEST
          2 x IFCBEAM | type IFCBEAMTYPE "Kantbjelke 320-L 110 x 320" | object type "BEAM" | names: "B-" | material: "100% 3804985440" | property sets: Pset_BeamCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, MMI, TESTTEST, TULLETE TEST
          2 x IFCBEAM | type IFCBEAMTYPE "Kantbjelke rekkverk 8 x 472" | object type "BEAM" | names: "B-" | material: "100% 3804985440" | property sets: Pset_BeamCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, tullball, TESTTEST
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "*9520 - IV 05 - Plate 25 mm med 10 luft 35" | names: "VT-" | material: layers "*9520 - IV 05 - Plate 25 mm med 10 luft" ("Platekledning - Vegg" 25.) | property sets: Pset_FireRatingProperties, Pset_WallCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, TESTTEST
          11 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "* PV 01- Påforing stålstender 100mm 3 lag gips 149" | names: "PV01" | material: layers "* PV 01- Påforing stålstender 100mm 3 lag gips" ("Gipsplate - Vegg" 13., "Gipsplate - Vegg" 13., "Gipsplate - Vegg" 13., "Stenderverk stål - Isolert" 100.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, TESTTEST, MMI, tullball, Skeisvang Pset: TEST 01 - ifcProject
          2 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall Type" | names: "CurtainWall-" | parts: 375 IFCMEMBER, 110 IFCPLATE | property sets: Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, Pset_CurtainWallCommon, TULLETE TEST
          3 x IFCWALL | type IFCWALLTYPE "* PV 01- Påforing stålstender 100mm 3 lag gips 149" | names: "PV01" | parts: 12 IFCBUILDINGELEMENTPART | property sets: Pset_FireRatingProperties, MMI, Pset_WallCommon, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST
          15 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "* IV 02 - Stålstender 100mm, isolert, 2x platekl. to sider 152" | names: "IV02" | material: layers "* IV 02 - Stålstender 100mm, isolert, 2x platekl. to sider" ("Gipsplate - Vegg" 13., "Gipsplate - Vegg" 13., "Stenderverk stål - Isolert" 100., "Gipsplate - Vegg" 13., "Gipsplate - Vegg" 13.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet asymmetrisk" | object type "DOOR" | names: "IDC.003" | property sets: Pset_FireRatingProperties, MMI, Pset_DoorCommon, TESTTEST, TULLETE TEST, tullball
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Stenderverk stål - Isolert 100" | names: "skjørt" | material: layers "Stenderverk stål - Isolert 100" ("Stenderverk stål - Isolert" 100.) | property sets: MMI, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, Pset_WallCommon, TESTTEST, TULLETE TEST
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "*9520 - IV 03 - Stålstender 75mm, uisolert, 1x platekl. en side 88" | names: "VT-" | material: layers "*9520 - IV 03 - Stålstender 75mm, uisolert, 1x platekl. en side" ("Gipsplate - Vegg" 13., "Stenderverk stål - Uisolert" 75.) | property sets: tullball, TULLETE TEST, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, BaseQuantities, Pset_WallCommon
          6 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu" | object type "WINDOW" | names: "V-", "IVA.000" | property sets: Pset_WindowCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, AC_Pset_RenovationAndPhasing
          3 x IFCDOOR | type IFCDOORSTYLE "Skyvedør" | object type "DOOR" | names: "YD-", "IDA" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, TESTTEST, TULLETE TEST, tullball, AC_Pset_RenovationAndPhasing
          6 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-", "YDC.000" | property sets: Pset_DoorCommon, MMI, Pset_FireRatingProperties, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, TESTTEST, tullball
          14 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 1 250" | names: "VT-" | material: layers "Yttervegg 1 250" ("Yttervegg 1" 250.) | property sets: MMI, Pset_WallCommon, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, TULLETE TEST, TESTTEST
          3 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-", "IDA" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, Skeisvang Pset: TEST 01 - ifcProject, MMI
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, TESTTEST, tullball, TULLETE TEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "YD-" | property sets: Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, MMI, Pset_DoorCommon, TESTTEST, TULLETE TEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, MMI, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, tullball
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-" | property sets: BaseQuantities, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, tullball, TESTTEST, Pset_FireRatingProperties
          17 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 1 100" | names: "VT-" | material: layers "Yttervegg 1 100" ("Yttervegg 1" 100.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, TESTTEST, Pset_FireRatingProperties, MMI, TULLETE TEST, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, MMI, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, Pset_FireRatingProperties, tullball
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 1 170" | names: "VT-" | material: layers "Yttervegg 1 170" ("Yttervegg 1" 170.) | property sets: Pset_FireRatingProperties, Pset_WallCommon, MMI, TULLETE TEST, AC_Pset_RenovationAndPhasing, Skeisvang Pset: TEST 01 - ifcProject
          1 x IFCSLAB | type IFCSLABTYPE "Yttervegg 1 200" | BASESLAB | names: "Dekke-" | material: layers "Yttervegg 1 200" ("Yttervegg 1" 200.) | property sets: Pset_SlabCommon, Pset_FireRatingProperties, Pset_CoveringCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 1 400" | names: "VT-" | material: layers "Yttervegg 1 400" ("Yttervegg 1" 400.) | property sets: Pset_WallCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, TESTTEST, TULLETE TEST
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 1 275" | names: "VT-" | material: layers "Yttervegg 1 275" ("Yttervegg 1" 275.) | property sets: Pset_WallCommon, MMI, AC_Pset_RenovationAndPhasing, tullball, TULLETE TEST, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "YD-" | property sets: Pset_FireRatingProperties, MMI, Pset_DoorCommon, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, MMI, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Innervegg 200" | names: "VT-" | material: layers "Innervegg 200" ("Innervegg" 200.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, TESTTEST, TULLETE TEST, Skeisvang Pset: TEST 01 - ifcProject
          3 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-", "IDC.001" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-" | property sets: MMI, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, Pset_FireRatingProperties, TESTTEST, tullball
          8 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg HOVEDBYGG 200" | names: "VT-" | material: layers "Yttervegg HOVEDBYGG 200" ("Yttervegg HOVEDBYGG" 200.) | property sets: Pset_WallCommon, MMI, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, tullball
          8 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 1 120" | names: "VT-" | material: layers "Yttervegg 1 120" ("Yttervegg 1" 120.) | property sets: Pset_FireRatingProperties, Pset_WallCommon, AC_Pset_RenovationAndPhasing, Skeisvang Pset: TEST 01 - ifcProject, BaseQuantities, tullball
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-" | property sets: Pset_FireRatingProperties, MMI, TESTTEST, Pset_DoorCommon, tullball, TULLETE TEST
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 1 220" | names: "VT-" | material: layers "Yttervegg 1 220" ("Yttervegg 1" 220.) | property sets: Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, MMI, tullball, Pset_WallCommon
          7 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-", "IDC.014" | property sets: TESTTEST, tullball, BaseQuantities, AC_Pset_RenovationAndPhasing, TULLETE TEST, Pset_FireRatingProperties
          7 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 1 50" | names: "VT-" | material: layers "Yttervegg 1 50" ("Yttervegg 1" 50.) | property sets: MMI, Pset_FireRatingProperties, Pset_WallCommon, TESTTEST, TULLETE TEST, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, MMI, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, TESTTEST, TULLETE TEST
          54 x IFCSLAB | type IFCSLABTYPE "Dekke 200" | BASESLAB | names: "Dekke-" | material: layers "Dekke 200" ("Dekke" 200.) | property sets: TESTTEST, TULLETE TEST, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, Pset_SlabCommon, Pset_CoveringCommon
          8 x IFCSLAB | type IFCSLABTYPE "Dekke 600" | BASESLAB | names: "Dekke-" | material: layers "Dekke 600" ("Dekke" 600.0000000000001) | property sets: Pset_CoveringCommon, Pset_SlabCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, MMI, TESTTEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, TULLETE TEST, TESTTEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, tullball, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "YD-" | property sets: Skeisvang Pset: TEST 01 - ifcProject, MMI, Pset_FireRatingProperties, Pset_DoorCommon, TESTTEST, TULLETE TEST
          3 x IFCSTAIR | names: "Trapp-" | parts: 8 IFCBUILDINGELEMENTPART | property sets: Pset_FireRatingProperties, Pset_StairCommon, Skeisvang Pset: TEST 01 - ifcProject, MMI, TESTTEST, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, MMI, TULLETE TEST, tullball
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, MMI, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          2 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu" | object type "WINDOW" | names: "V-" | property sets: BaseQuantities, AC_Pset_RenovationAndPhasing, tullball, TULLETE TEST, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject
          1 x IFCWALL | type IFCWALLTYPE "Yttervegg 1 150" | names: "VT-" | material: "Yttervegg 1" | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, MMI, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, tullball, TESTTEST
          2 x IFCSLAB | type IFCSLABTYPE "Dekke 120" | BASESLAB | names: "Dekke-" | material: layers "Dekke 120" ("Dekke" 119.9999999999984) | property sets: Pset_CoveringCommon, Pset_SlabCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, MMI
          11 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tre" | names: "Terreng-01" | material: "Tre" | property sets: Skeisvang Pset: TEST 01 - ifcProject, AC_Pset_Dimension, AC_Pset_RenovationAndPhasing
          1 x IFCSLAB | type IFCSLABTYPE "Yttervegg 1 1250" | BASESLAB | names: "Dekke-" | material: layers "Yttervegg 1 1250" ("Yttervegg 1" 1250.000000000004) | property sets: Pset_CoveringCommon, Pset_SlabCommon, Pset_FireRatingProperties, TESTTEST, MMI, Skeisvang Pset: TEST 01 - ifcProject
          9 x IFCWALL | type IFCWALLTYPE "Bodvegger 150 x 3250" | names: "VT-" | parts: 198 IFCBUILDINGELEMENTPART | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, tullball, TULLETE TEST
          1 x IFCSLAB | type IFCSLABTYPE "Stein - Skiferheller 200" | BASESLAB | names: "Dekke-" | material: layers "Stein - Skiferheller 200" ("Stein - Skiferheller" 200.) | property sets: Pset_CoveringCommon, Pset_SlabCommon, Pset_FireRatingProperties, TULLETE TEST, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg DETALJER 550" | names: "VT-" | material: layers "Yttervegg DETALJER 550" ("Yttervegg DETALJER" 550.) | property sets: Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, Pset_WallCommon, MMI, TESTTEST, TULLETE TEST
          2 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-", "YDC.000" | property sets: Pset_DoorCommon, MMI, TULLETE TEST, tullball, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST
          2 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "YD-" | property sets: MMI, Pset_DoorCommon, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, TESTTEST, TULLETE TEST
          4 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-", "IDA" | property sets: Pset_FireRatingProperties, MMI, Pset_DoorCommon, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "YD-" | property sets: AC_Pset_RenovationAndPhasing, TULLETE TEST, tullball, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, Pset_DoorCommon
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet med overlys" | object type "DOOR" | names: "YDA.000" | property sets: Pset_DoorCommon, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, MMI, TESTTEST, tullball
          2 x IFCDOOR | type IFCDOORSTYLE "Leddport" | object type "DOOR" | names: "PA.000" | property sets: Pset_FireRatingProperties, TULLETE TEST, MMI, Pset_DoorCommon, tullball, TESTTEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet med overlys" | object type "DOOR" | names: "IDA.000" | property sets: Pset_DoorCommon, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST, tullball, MMI
          3 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "IDA" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, AC_Pset_RenovationAndPhasing
          2 x IFCSLAB | type IFCSLABTYPE "Dekke 50" | BASESLAB | names: "Dekke-" | material: layers "Dekke 50" ("Dekke" 50.) | property sets: Pset_SlabCommon, Pset_FireRatingProperties, Pset_CoveringCommon, TULLETE TEST, Skeisvang Pset: TEST 01 - ifcProject, MMI
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg HOVEDBYGG 320" | names: "VT-" | material: layers "Yttervegg HOVEDBYGG 320" ("Yttervegg HOVEDBYGG" 320.) | property sets: Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST, Pset_WallCommon
          23 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu variabelt" | object type "WINDOW" | names: "YVA.000" | property sets: Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, Pset_WindowCommon, TESTTEST, tullball
          6 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Sink" | names: "renne_nedløp_trafo_energisentral", "gesimsbeslag_trafo_energisentral" | material: "Sink" | property sets: Skeisvang Pset: TEST 01 - ifcProject, AC_Pset_RenovationAndPhasing, AC_Pset_Dimension
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Maling 3" | names: "VT-" | material: layers "Maling 3" ("Maling" 3.); layers "Maling 2.5" ("Maling" 2.5) | property sets: Pset_WallCommon, MMI, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, tullball
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg HOVEDBYGG 275" | names: "VT-" | material: layers "Yttervegg HOVEDBYGG 275" ("Yttervegg HOVEDBYGG" 275.) | property sets: Pset_WallCommon, tullball, TULLETE TEST, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, MMI
          2 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet med overlys" | object type "DOOR" | names: "IDA" | property sets: Pset_FireRatingProperties, Pset_DoorCommon, Skeisvang Pset: TEST 01 - ifcProject, MMI, TESTTEST, tullball
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 1 350" | names: "VT-" | material: layers "Yttervegg 1 350" ("Yttervegg 1" 350.) | property sets: Pset_FireRatingProperties, Pset_WallCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, TESTTEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet med overlys" | object type "DOOR" | names: "IDA" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, tullball, MMI
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 1 550" | names: "VT-" | material: layers "Yttervegg 1 550" ("Yttervegg 1" 550.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, TULLETE TEST, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST
          1 x IFCSLAB | type IFCSLABTYPE "Dekke 400" | BASESLAB | names: "Dekke-" | material: layers "Dekke 400" ("Dekke" 399.9999999999979) | property sets: Pset_CoveringCommon, Pset_SlabCommon, Pset_FireRatingProperties, MMI, TESTTEST, tullball
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "YDC.000" | property sets: MMI, Pset_FireRatingProperties, Pset_DoorCommon, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          2 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "IDC-000" | property sets: Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, Pset_DoorCommon, tullball
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "IDA" | property sets: Pset_FireRatingProperties, MMI, Pset_DoorCommon, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Curtain Wall Type" | names: "Glassvegg-" | parts: 145 IFCBUILDINGELEMENTPROXY | property sets: AC_Pset_Dimension, Skeisvang Pset: TEST 01 - ifcProject, AC_Pset_RenovationAndPhasing
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Isolasjon - Trykkfast" | names: "renne_nedløp_trafo_energisentral", "kondensisolasjon tak_trafo_energisentral" | material: "Isolasjon - Trykkfast" | property sets: AC_Pset_Dimension, AC_Pset_RenovationAndPhasing, Skeisvang Pset: TEST 01 - ifcProject
          3 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "IDA", "YD-" | property sets: Pset_DoorCommon, MMI, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          2 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-" | property sets: Pset_FireRatingProperties, Pset_DoorCommon, TESTTEST, MMI, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "YD-" | property sets: BaseQuantities, AC_Pset_RenovationAndPhasing, tullball, TULLETE TEST, Skeisvang Pset: TEST 01 - ifcProject, Pset_DoorCommon
          2 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "IDC.017" | property sets: Pset_DoorCommon, MMI, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "IDC.001" | property sets: Pset_DoorCommon, MMI, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, BaseQuantities, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "IDC.017" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, MMI, tullball
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Stål 100 x 100" | object type "COLUMN" | names: "S-" | material: "Stål" | property sets: Pset_ColumnCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, tullball, TESTTEST
          5 x IFCWALL | type IFCWALLTYPE "* YV 03 - 200 mm trestender, , murplate utvendig, sjikt for solavskjerming, tegl 464" | names: "YV01a", "YV05" | parts: 20 IFCBUILDINGELEMENTPART | property sets: Pset_FireRatingProperties, MMI, Pset_WallCommon, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, AC_Pset_RenovationAndPhasing
          4 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu vertikal multi-rams" | object type "WINDOW" | names: "YVC.000" | property sets: Pset_WindowCommon, MMI, Pset_FireRatingProperties, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST
          3 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu variabelt" | object type "WINDOW" | names: "YVC.000" | property sets: Pset_FireRatingProperties, MMI, TESTTEST, tullball, TULLETE TEST, Pset_WindowCommon
          2 x IFCWALL | type IFCWALLTYPE "9520 - YV 02 - 200 mm trestender, , murplate, tegl 394" | names: "YV02", "YV04" | parts: 8 IFCBUILDINGELEMENTPART | property sets: Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, MMI, Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu variabelt" | object type "WINDOW" | names: "YVC.000" | property sets: Pset_WindowCommon, MMI, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, tullball
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg tegl 104" | names: "VT-" | material: layers "Yttervegg tegl 104" ("Yttervegg tegl" 104.) | property sets: Pset_WallCommon, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, MMI, TULLETE TEST, Pset_FireRatingProperties
          1 x IFCWALL | type IFCWALLTYPE "Yttervegg tegl 104" | names: "VT-" | material: "Yttervegg tegl" | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, TESTTEST, TULLETE TEST, Skeisvang Pset: TEST 01 - ifcProject
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Isolasjon - Trykkfast 200" | names: "VT-" | material: layers "Isolasjon - Trykkfast 200" ("Isolasjon - Trykkfast" 200.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, TESTTEST, TULLETE TEST, MMI, tullball
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Bjelkelag148 mm tre, 9 mm GU 157" | names: "VT-" | material: layers "Bjelkelag148 mm tre, 9 mm GU" ("Gipsplate - Utvendig" 9., "Bjelkelag - Isolert" 148.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, TESTTEST, TULLETE TEST, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "IDC-000" | property sets: Pset_FireRatingProperties, MMI, TESTTEST, TULLETE TEST, Skeisvang Pset: TEST 01 - ifcProject, Pset_DoorCommon
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "IDC.001" | property sets: Pset_DoorCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST, tullball
          7 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "*9520 - IV LYD4 - 60 dB : 3x13 mm gips, 1x100mm stålstender 149" | names: "PV01" | material: layers "*9520 - IV LYD4 - 60 dB : 3x13 mm gips, 1x100mm stålstender" ("Gipsplate - Vegg" 13., "Gipsplate - Vegg" 13., "Gipsplate - Vegg" 13., "Stenderverk stål - Isolert" 100.) | property sets: MMI, Pset_WallCommon, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, tullball, AC_Pset_RenovationAndPhasing
          1 x IFCWALL | type IFCWALLTYPE "*9520 - IV LYD3 - 55 dB: 2x13 mm gips, 2x100mm stålstender, 2x13mm gips 262" | names: "IV08" | parts: 6 IFCBUILDINGELEMENTPART | property sets: MMI, Pset_WallCommon, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, TESTTEST, AC_Pset_RenovationAndPhasing
          2 x IFCDOOR | type IFCDOORSTYLE "Dør med sidefelt på side 2" | object type "DOOR" | names: "IDC.009" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, tullball, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "IDC.010" | property sets: Pset_FireRatingProperties, Pset_DoorCommon, MMI, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "IDC.004" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "9520 - IV 00 - Stålstender 100mm, isolert, 2x platekl. en side 136" | names: "VT-" | material: layers "9520 - IV 00 - Stålstender 100mm, isolert, 2x platekl. en side" ("Gipsplate - Vegg" 13., "Gipsplate - Vegg" 13., "Stenderverk stål - Isolert" 100.) | property sets: Pset_FireRatingProperties, Pset_WallCommon, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, tullball, TULLETE TEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet med 2 sidefelt" | object type "DOOR" | names: "IDC.005" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, tullball
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet asymmetrisk" | object type "DOOR" | names: "IDC.006" | property sets: Pset_FireRatingProperties, MMI, Pset_DoorCommon, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, tullball
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "IDC.002" | property sets: Pset_DoorCommon, Skeisvang Pset: TEST 01 - ifcProject, MMI, Pset_FireRatingProperties, TESTTEST, TULLETE TEST
          2 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "IDC.002", "IDC.001" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, tullball, TULLETE TEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "IDC.008" | property sets: Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, MMI, TULLETE TEST, tullball, TESTTEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "IDC.012" | property sets: Pset_FireRatingProperties, Pset_DoorCommon, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, MMI, tullball
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "IDC.012" | property sets: Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, Pset_DoorCommon, TULLETE TEST, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "* IV 04 - Stålstender 100mm, isolert, 1x + 2x platekl. to sider 139" | names: "IV04" | material: layers "* IV 04 - Stålstender 100mm, isolert, 1x + 2x platekl. to sider" ("Gipsplate - Vegg" 13., "Stenderverk stål - Isolert" 100., "Gipsplate - Vegg" 13., "Gipsplate - Vegg" 13.) | property sets: Pset_WallCommon, MMI, Pset_FireRatingProperties, TESTTEST, TULLETE TEST, tullball
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "IDC.014" | property sets: Pset_DoorCommon, MMI, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          2 x IFCWALL | type IFCWALLTYPE "* IV 08- 55 dB: 2x13 mm gips, 2x100mm stålstender, 2x13mm gips 262" | names: "IV08" | parts: 12 IFCBUILDINGELEMENTPART | property sets: MMI, Pset_WallCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, tullball
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "* PV04 Stålstender 100mm isolert, påforingt, 2x platekl. en side 122" | names: "PV04" | material: layers "* PV04 Stålstender 100mm isolert, påforingt, 2x platekl. en side" ("Platekledning - Vegg" 10., "OSB-plate" 12., "Stenderverk stål - Isolert" 100.) | property sets: Pset_FireRatingProperties, MMI, Pset_WallCommon, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, tullball
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet med overlys" | object type "DOOR" | names: "YDC-000" | property sets: Pset_FireRatingProperties, Pset_DoorCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, AC_Pset_RenovationAndPhasing
          1 x IFCCOVERING | type IFCCOVERINGTYPE "9520 - HH 00 - Fast himling gips_Sylomar Akustikk Super T60 KOPI 125" | CEILING | names: "Gipshimling m. Sylomer Akustik Super T60" | parts: 2 IFCBUILDINGELEMENTPART | property sets: AC_Pset_Dimension, MMI, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, Pset_CoveringCommon, TESTTEST
          2 x IFCSLAB | type IFCSLABTYPE "9520 - HH 00 - Fast himling gips_Sylomar Akustikk Super T60 KOPI 125" | BASESLAB | names: "Gipshimling m. Sylomer Akustik Super T60" | material: layers "9520 - HH 00 - Fast himling gips_Sylomar Akustikk Super T60 KOPI" ("Gipsplate - Tak" 13., "Gipsplate - Tak" 13.) | property sets: Pset_CoveringCommon, Pset_SlabCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, tullball
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "IDC.004" | property sets: Pset_DoorCommon, MMI, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, TESTTEST
          2 x IFCDOOR | type IFCDOORSTYLE "Dør med sidefelt på side 2" | object type "DOOR" | names: "IDC.011" | property sets: Pset_DoorCommon, MMI, TESTTEST, Pset_FireRatingProperties, TULLETE TEST, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "IDC.008" | property sets: MMI, Pset_DoorCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "IDC.007" | property sets: Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST, tullball
          1 x IFCSLAB | type IFCSLABTYPE "Dekke 5000" | BASESLAB | names: "Dekke-" | material: layers "Dekke 5000" ("Dekke" 5000.) | property sets: Pset_CoveringCommon, Pset_SlabCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, TESTTEST
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tekst 3D" | names: "Stol-" | property sets: AC_Pset_Dimension, Skeisvang Pset: TEST 01 - ifcProject, AC_Pset_RenovationAndPhasing, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Flis - Gulv 15" | names: "Banebelegg" | material: "Flis - Gulv" | property sets: Pset_CoveringCommon, AC_Pset_Dimension, AC_Pset_RenovationAndPhasing, Skeisvang Pset: TEST 01 - ifcProject
          11 x IFCCOVERING | type IFCCOVERINGTYPE "Systemhimling - 60x60 20" | CEILING | names: "Systemhimling 600 x 600 E-kant", "Systemhimling Hygiene 600 x 600 E-kant" | material: "Systemhimling - 60x60" | property sets: AC_Pset_Dimension, Pset_CoveringCommon, MMI, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør med sidefelt på side 2" | object type "DOOR" | names: "IDC.011" | property sets: Pset_DoorCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, tullball, TULLETE TEST
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "9520 - IV 00 - Stålstender 100mm, uisolert 110" | names: "VT-" | material: layers "9520 - IV 00 - Stålstender 100mm, uisolert" ("Stenderverk stål - Uisolert" 100.) | property sets: Pset_WallCommon, AC_Pset_RenovationAndPhasing, BaseQuantities, tullball, Pset_FireRatingProperties, TULLETE TEST
          5 x IFCSLAB | type IFCSLABTYPE "Tre 50" | BASESLAB | names: "Dekke-" | material: layers "Tre 50" ("Tre" 50.) | property sets: Pset_CoveringCommon, Pset_SlabCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, tullball
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Påstøp 3" | FLOORING | names: "Slipt betong" | material: "Påstøp" | property sets: AC_Pset_Dimension, MMI, Pset_CoveringCommon, Pset_FireRatingProperties, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Innervegg 45" | names: "VT-" | material: layers "Innervegg 45" ("Innervegg" 45.) | property sets: Pset_WallCommon, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, MMI, TESTTEST, TULLETE TEST
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Tre 45" | names: "VT-" | material: layers "Tre 45" ("Tre" 45.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, MMI, TESTTEST, tullball
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Bjelkelag148 mm tre, 9 mm GU , uisolert 148" | names: "IV01" | material: layers "Bjelkelag148 mm tre, 9 mm GU , uisolert" ("Bindingsverk - Uisolert" 148.) | property sets: Skeisvang Pset: TEST 01 - ifcProject, MMI, Pset_FireRatingProperties, Pset_WallCommon, TESTTEST, TULLETE TEST
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg HOVEDBYGG 125" | names: "VT-" | material: layers "Yttervegg HOVEDBYGG 125" ("Yttervegg HOVEDBYGG" 125.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Isolasjon - Trykkfast 125" | names: "VT-" | material: layers "Isolasjon - Trykkfast 125" ("Isolasjon - Trykkfast" 125.) | property sets: MMI, Pset_FireRatingProperties, Pset_WallCommon, Skeisvang Pset: TEST 01 - ifcProject, tullball, TULLETE TEST
          4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Lem rektangulær" | names: "Lufterist metall_Fagne" | property sets: AC_Pset_Dimension, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, Skeisvang Pset: TEST 01 - ifcProject, AC_Pset_RenovationAndPhasing
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Innervegg 150" | names: "VT-" | material: layers "Innervegg 150" ("Innervegg" 150.) | property sets: Pset_FireRatingProperties, Pset_WallCommon, TESTTEST, MMI, Skeisvang Pset: TEST 01 - ifcProject, tullball
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, TESTTEST, tullball
          2 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "IDC.013" | property sets: Pset_DoorCommon, MMI, Pset_FireRatingProperties, TESTTEST, TULLETE TEST, Skeisvang Pset: TEST 01 - ifcProject
          4 x IFCCOVERING | type IFCCOVERINGTYPE "Stål 50" | CEILING | names: "fotskraperist" | material: "Stål" | property sets: Pset_CoveringCommon, AC_Pset_Dimension, Skeisvang Pset: TEST 01 - ifcProject, MMI, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "IDC.002" | property sets: Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, Pset_DoorCommon, TULLETE TEST
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Innervegg tegl 230" | names: "VT-" | material: layers "Innervegg tegl 230" ("Innervegg tegl" 230.) | property sets: Pset_WallCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, tullball, Pset_FireRatingProperties
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "IDC-000" | property sets: Pset_DoorCommon, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, tullball, MMI
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "IDC.015" | property sets: MMI, Skeisvang Pset: TEST 01 - ifcProject, Pset_DoorCommon, TESTTEST, TULLETE TEST, tullball
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "IDC.015" | property sets: Pset_FireRatingProperties, Pset_DoorCommon, MMI, TULLETE TEST, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "IDC.113" | property sets: Pset_FireRatingProperties, Pset_DoorCommon, MMI, TULLETE TEST, TESTTEST, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "IDC.002" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, tullball
          4 x IFCCOVERING | type IFCCOVERINGTYPE "Gulvplanker 35" | FLOORING | names: "Parkett" | material: "Gulvplanker" | property sets: Pset_CoveringCommon, Pset_FireRatingProperties, AC_Pset_Dimension, MMI, Skeisvang Pset: TEST 01 - ifcProject, BaseQuantities
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Gulvplanker 30" | FLOORING | names: "Parkett" | material: "Gulvplanker" | property sets: AC_Pset_Dimension, Pset_CoveringCommon, MMI, Pset_FireRatingProperties, BaseQuantities, TESTTEST
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Gulvplanker 362" | FLOORING | names: "Parkett" | material: "Gulvplanker" | property sets: Pset_CoveringCommon, AC_Pset_Dimension, Pset_FireRatingProperties, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, AC_Pset_RenovationAndPhasing
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Gulvplanker 367" | FLOORING | names: "Parkett" | material: "Gulvplanker" | property sets: AC_Pset_Dimension, Pset_CoveringCommon, Pset_FireRatingProperties, MMI, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Gulvplanker 367" | FLOORING | names: "Parkett" | material: "Gulvplanker" | property sets: AC_Pset_Dimension, Pset_CoveringCommon, MMI, Pset_FireRatingProperties, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Gulvplanker 367" | FLOORING | names: "Parkett" | material: "Gulvplanker" | property sets: Pset_CoveringCommon, AC_Pset_Dimension, MMI, TESTTEST, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Tre 150" | FLOORING | names: "Parkett" | material: "Tre" | property sets: Pset_CoveringCommon, AC_Pset_Dimension, MMI, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Tre 212" | FLOORING | names: "Parkett" | material: "Tre" | property sets: Pset_CoveringCommon, Pset_FireRatingProperties, AC_Pset_Dimension, MMI, AC_Pset_RenovationAndPhasing, TESTTEST
          3 x IFCCOVERING | type IFCCOVERINGTYPE "Tre 150" | FLOORING | names: "Parkett" | material: "Tre" | property sets: Pset_CoveringCommon, AC_Pset_Dimension, Pset_FireRatingProperties, MMI, TESTTEST, AC_Pset_RenovationAndPhasing
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Tre 578" | FLOORING | names: "Parkett" | material: "Tre" | property sets: Pset_CoveringCommon, AC_Pset_Dimension, MMI, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Tre 945" | FLOORING | names: "Parkett" | material: "Tre" | property sets: Pset_FireRatingProperties, Pset_CoveringCommon, AC_Pset_Dimension, TESTTEST, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Tre 1312" | FLOORING | names: "Parkett" | material: "Tre" | property sets: Pset_CoveringCommon, TESTTEST, AC_Pset_RenovationAndPhasing, BaseQuantities, Skeisvang Pset: TEST 01 - ifcProject, AC_Pset_Dimension
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Tre 150" | names: "VT-" | material: layers "Tre 150" ("Tre" 150.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Overgangsbeslag amfi mot bygg A 270 x 2" | object type "COLUMN" | names: "S-" | material: "0% 27718788" | property sets: Pset_FireRatingProperties, Pset_ColumnCommon, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, MMI, tullball
          3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tre - Heltre" | names: "renne_nedløp_trafo_energisentral" | material: "Tre - Heltre" | property sets: Skeisvang Pset: TEST 01 - ifcProject, AC_Pset_RenovationAndPhasing, AC_Pset_Dimension
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Bjelkelag 198, isolert 216" | names: "IV01" | material: layers "Bjelkelag 198, isolert" ("Gipsplate - Utvendig" 9., "Bindingsverk - Isolert" 198., "Gipsplate - Utvendig" 9.) | property sets: Pset_WallCommon, TESTTEST, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, AC_Pset_RenovationAndPhasing
          28 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Tre 25" | names: "VT-" | material: layers "Tre 25" ("Tre" 25.) | property sets: MMI, Pset_WallCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, tullball
          12 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Tre 5" | names: "VT-" | material: layers "Tre 5" ("Tre" 5.) | property sets: Pset_WallCommon, MMI, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Isolasjon - Myk 138" | names: "VT-" | material: layers "Isolasjon - Myk 138" ("Isolasjon - Myk" 138.) | property sets: Pset_WallCommon, MMI, TESTTEST, tullball, TULLETE TEST, Skeisvang Pset: TEST 01 - ifcProject
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Isolasjon - Myk 51" | names: "VT-" | material: layers "Isolasjon - Myk 51" ("Isolasjon - Myk" 51.) | property sets: MMI, Pset_FireRatingProperties, tullball, BaseQuantities, AC_Pset_RenovationAndPhasing, TESTTEST
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Isolasjon - Myk 225" | names: "VT-" | material: layers "Isolasjon - Myk 225" ("Isolasjon - Myk" 225.) | property sets: MMI, Pset_WallCommon, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, TESTTEST, TULLETE TEST
          2 x IFCBEAM | type IFCBEAMTYPE "Overgangsbeslag amfi mot bygg A 270 x 2" | object type "BEAM" | names: "B-" | material: "0% 27718788" | property sets: MMI, Pset_BeamCommon, Pset_FireRatingProperties, TESTTEST, TULLETE TEST, tullball
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Puss 125" | names: "VT-" | material: layers "Puss 125" ("Puss" 125.) | property sets: Pset_WallCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, TULLETE TEST, tullball
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu vertikal multi-rams" | object type "WINDOW" | names: "YVC.000" | property sets: AC_Pset_RenovationAndPhasing, BaseQuantities, TESTTEST, tullball, Skeisvang Pset: TEST 01 - ifcProject, MMI
          2 x IFCSLAB | type IFCSLABTYPE "Dekke 2557" | BASESLAB | names: "hjørnebeslag" | material: layers "Dekke 2557" ("Dekke" 2557.000000000002) | property sets: Pset_CoveringCommon, Pset_SlabCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST
          1 x IFCGRID
      IFCBUILDINGSTOREY "Plan 1. Etasje" | elevation 27300.
        contains 2477 elements
          17 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "* IV 01 - Stålstender 100mm, isolert, 1x platekl. to sider 126" | names: "IV01" | material: layers "* IV 01 - Stålstender 100mm, isolert, 1x platekl. to sider" ("Gipsplate - Vegg" 13., "Stenderverk stål - Isolert" 100., "Gipsplate - Vegg" 13.) | property sets: Pset_WallCommon, MMI, Pset_FireRatingProperties, TESTTEST, TULLETE TEST, tullball
          10 x IFCCOLUMN | type IFCCOLUMNTYPE "HUP 100x100x10 100 x 100" | object type "COLUMN" | names: "S-" | material: "Stål - S355" | property sets: Pset_FireRatingProperties, Pset_ColumnCommon, MMI, TESTTEST, tullball, TULLETE TEST
          54 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "*9520 - IV 02 - Stålstender 100mm, uisolert,1x platekl. en side 113" | names: "skjørt" | material: layers "*9520 - IV 02 - Stålstender 100mm, uisolert,1x platekl. en side" ("Gipsplate - Vegg" 13., "Stenderverk stål - Uisolert" 100.) | property sets: Pset_FireRatingProperties, Pset_WallCommon, MMI, TESTTEST, TULLETE TEST, AC_Pset_RenovationAndPhasing
          6 x IFCCOVERING | type IFCCOVERINGTYPE "Platekledning - Himling 15" | CEILING | names: "Fast himling", "Spilehimling flåter 600 x 1200" | material: "Platekledning - Himling" | property sets: Pset_CoveringCommon, AC_Pset_Dimension, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "* IV 09 - RENHOLD - 1 plate gips+1 plate OSB-plate, Stålstender 100mm, isolert, 2x platekl. gips 152" | names: "IV09" | material: layers "* IV 09 - RENHOLD - 1 plate gips+1 plate OSB-plate, Stålstender 100mm, isolert, 2x platekl. gips" ("Gipsplate - Vegg" 13., "Gipsplate - Vegg" 13., "Stenderverk stål - Isolert" 100., "Gipsplate - Vegg" 13., "Gipsplate - Vegg" 13.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          6 x IFCCOVERING | type IFCCOVERINGTYPE "Systemhimling - 60x120 50" | CEILING | names: "Spilehimling flåter 600 x 1200" | material: "Systemhimling - 60x120" | property sets: Pset_CoveringCommon, Pset_FireRatingProperties, AC_Pset_Dimension, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST
          92 x IFCCOLUMN | type IFCCOLUMNTYPE "Aluminium 50 x 10" | object type "COLUMN" | names: "S-" | material: "Aluminium" | property sets: Pset_ColumnCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, tullball, TULLETE TEST
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Stål 321" | CEILING | names: "Spilehimling flåter 600 x 1200" | material: "Stål" | property sets: Pset_FireRatingProperties, Pset_CoveringCommon, AC_Pset_Dimension, MMI, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Stål 329" | CEILING | names: "Spilehimling flåter 600 x 1200" | material: "Stål" | property sets: AC_Pset_Dimension, Pset_FireRatingProperties, Pset_CoveringCommon, Skeisvang Pset: TEST 01 - ifcProject, MMI, AC_Pset_RenovationAndPhasing
          56 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "*9520 - IV 05 - Plate 25 mm med 50 mm luft til eletrisk 75" | names: "VT-", "Veggabsorbent" | material: layers "*9520 - IV 05 - Plate 25 mm med 50 mm luft til eletrisk" ("Platekledning - Vegg" 25.) | property sets: TULLETE TEST, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, MMI, Pset_FireRatingProperties, Pset_WallCommon
          15 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tre" | names: "Terreng-01" | material: "Tre" | property sets: AC_Pset_Dimension, Skeisvang Pset: TEST 01 - ifcProject, AC_Pset_RenovationAndPhasing
          8 x IFCCOVERING | type IFCCOVERINGTYPE "Platekledning - Himling 20" | CEILING | names: "Spilehimling flåter 600 x 1200", "Fast himling" | material: "Platekledning - Himling" | property sets: Pset_CoveringCommon, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, MMI, AC_Pset_Dimension, TESTTEST
          4 x IFCSLAB | type IFCSLABTYPE "Stål 120" | BASESLAB | names: "håndløper hovedtrapp vestibyle" | material: layers "Stål 120" ("Stål" 120.000000000001) | property sets: Pset_CoveringCommon, Pset_SlabCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST
          8 x IFCSLAB | type IFCSLABTYPE "Stål 60" | BASESLAB | names: "håndløper hovedtrapp vestibyle" | material: layers "Stål 60" ("Stål" 59.99999999999872) | property sets: Pset_CoveringCommon, Pset_SlabCommon, MMI, Pset_FireRatingProperties, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject
          45 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "*9520 - IV 07 - Teglvegg m/luft 134" | names: "VT-" | material: layers "*9520 - IV 07 - Teglvegg m/luft" ("Innervegg tegl" 104.) | property sets: MMI, Pset_FireRatingProperties, Pset_WallCommon, TESTTEST, AC_Pset_RenovationAndPhasing, Skeisvang Pset: TEST 01 - ifcProject
          26 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "*9520 - IV 03 - FORING NISJER Stålstender 75mm, uisolert, 1x platekl. en side 100" | names: "IV03" | material: layers "*9520 - IV 03 - FORING NISJER Stålstender 75mm, uisolert, 1x platekl. en side" ("Platekledning - Vegg" 25., "Stenderverk stål - Isolert" 75.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, TULLETE TEST, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject
          54 x IFCCOVERING | type IFCCOVERINGTYPE "Systemhimling - 60x60 50" | CEILING | names: "Systemhimling 600 x 600 E-kant", "Parafon 60 x 60" | material: "Systemhimling - 60x60" | property sets: Pset_CoveringCommon, AC_Pset_Dimension, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, TESTTEST, AC_Pset_RenovationAndPhasing
          8 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Innervegg tegl 104" | names: "VT-" | material: layers "Innervegg tegl 104" ("Innervegg tegl" 104.) | property sets: Pset_WallCommon, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, MMI, TULLETE TEST, AC_Pset_RenovationAndPhasing
          20 x IFCCOVERING | type IFCCOVERINGTYPE "9520 - HH 00 - Fast himling gips_Sylomar Akustikk Super T60 KOPI 125" | CEILING | names: "Gipshimling m. Sylomer Akustik Super T60", "Fast himling" | parts: 40 IFCBUILDINGELEMENTPART | property sets: Pset_CoveringCommon, AC_Pset_Dimension, MMI, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, TESTTEST
          16 x IFCCOVERING | type IFCCOVERINGTYPE "Systemhimling - 60x60 20" | CEILING | names: "Systemhimling 600 x 600 E-kant" | material: "Systemhimling - 60x60" | property sets: Pset_CoveringCommon, Pset_FireRatingProperties, AC_Pset_Dimension, Skeisvang Pset: TEST 01 - ifcProject, MMI, TESTTEST
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "9520 - YV 05 - 148 mm trestender 150" | names: "VT-" | material: layers "9520 - YV 05 - 148 mm trestender" ("Stenderverk tre YTTERVEGG - Isolert" 150.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "*9520 - IV 05 - Plate 25 mm med 10 luft 35" | names: "VT-" | material: layers "*9520 - IV 05 - Plate 25 mm med 10 luft" ("Platekledning - Vegg" 25.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, tullball
          25 x IFCCOVERING | type IFCCOVERINGTYPE "Teglstein 5" | CEILING | names: "tegl over åpning" | material: "Teglstein" | property sets: Pset_CoveringCommon, AC_Pset_Dimension, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet asymmetrisk" | object type "DOOR" | names: "IDC.109" | property sets: Pset_DoorCommon, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, MMI, TESTTEST, AC_Pset_RenovationAndPhasing
          12 x IFCWALL | type IFCWALLTYPE "* IV 05 - 60 dB : 3x13 mm gips, 2x100mm stålstender, 3x13mm gips 288" | names: "IV05", "VT-" | parts: 96 IFCBUILDINGELEMENTPART | property sets: MMI, Pset_WallCommon, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, TESTTEST, tullball
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "*9520 - 3x13 mm gips 39" | names: "VT-" | material: layers "*9520 - 3x13 mm gips" ("Gipsplate - Vegg" 13., "Gipsplate - Vegg" 13., "Gipsplate - Vegg" 13.) | property sets: Pset_FireRatingProperties, Pset_WallCommon, TESTTEST, MMI, TULLETE TEST, tullball
          5 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "IDC.106", "YD-" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, MMI, TESTTEST, TULLETE TEST, BaseQuantities
          4 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "IDC.106", "YD-", "IDC.113" | property sets: Pset_FireRatingProperties, MMI, Pset_DoorCommon, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, tullball
          2 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "IDC.114", "IDC.015" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, MMI, TESTTEST
          4 x IFCWALL | type IFCWALLTYPE "*9520 - IV 07 - Dobbel Teglvegg m/luft 230" | names: "VT-" | parts: 8 IFCBUILDINGELEMENTPART | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, BaseQuantities
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Isolasjon - Myk 150" | names: "IV?", "VT-" | material: layers "Isolasjon - Myk 150" ("Isolasjon - Myk" 150.) | property sets: Pset_FireRatingProperties, MMI, Pset_WallCommon, Skeisvang Pset: TEST 01 - ifcProject, tullball, TULLETE TEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet asymmetrisk" | object type "DOOR" | names: "YDC.100" | property sets: Pset_DoorCommon, MMI, Pset_FireRatingProperties, TESTTEST, TULLETE TEST, Skeisvang Pset: TEST 01 - ifcProject
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "*9520 - IV 07 Lydvegg fasade 188" | names: "IV21" | material: layers "*9520 - IV 07 Lydvegg fasade" ("Gipsplate - Vegg" 13., "Stenderverk tre - Isolert" 150.) | property sets: TESTTEST, Pset_FireRatingProperties, Pset_WallCommon, MMI, tullball, Skeisvang Pset: TEST 01 - ifcProject
          4 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu vertikal multi-rams" | object type "WINDOW" | names: "YVC.100" | property sets: Pset_FireRatingProperties, Pset_WindowCommon, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, MMI, AC_Pset_RenovationAndPhasing
          6 x IFCWALL | type IFCWALLTYPE "* IV 08- 55 dB: 2x13 mm gips, 2x100mm stålstender, 2x13mm gips 262" | names: "IV08", "YV03" | parts: 36 IFCBUILDINGELEMENTPART | property sets: Pset_WallCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, TULLETE TEST, TESTTEST
          1 x IFCSLAB | type IFCSLABTYPE "Stenderverk stål - Isolert 50" | BASESLAB | names: "fast gipshimling" | material: layers "Stenderverk stål - Isolert 50" ("Stenderverk stål - Isolert" 50.) | property sets: Pset_CoveringCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, MMI, Pset_SlabCommon
          3 x IFCRAILING | type IFCRAILINGTYPE "Railing Type" | names: "Rekkverk-" | parts: 284 IFCBUILDINGELEMENTPART | property sets: AC_Pset_Dimension, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST, tullball
          1 x IFCSLAB | type IFCSLABTYPE "Dekke 472" | BASESLAB | names: "Dekke-" | material: layers "Dekke 472" ("Dekke" 472.0000025130489) | property sets: Pset_SlabCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, Pset_CoveringCommon, TESTTEST
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "*9520 - IV 02 - Trelekt 50mm, isolert, 1x platekl. en side 63" | names: "IV11" | material: layers "*9520 - IV 02 - Trelekt 50mm, isolert, 1x platekl. en side" ("Gipsplate - Vegg" 13., "Stenderverk tre - Isolert" 50.) | property sets: Pset_WallCommon, MMI, Pset_FireRatingProperties, TESTTEST, TULLETE TEST, tullball
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "*9520 - IV 02B - Stålstender 50mm, isolert, 2x platekl. en side 86" | names: "IV18" | material: layers "*9520 - IV 02B - Stålstender 50mm, isolert, 2x platekl. en side" ("Gipsplate - Vegg" 13., "Gipsplate - Vegg" 13., "Stenderverk stål - Isolert" 50.) | property sets: MMI, Pset_WallCommon, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, Pset_FireRatingProperties, TULLETE TEST
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "9520 - YV 05 - 148 mm trestender (1) 150" | names: "VT-" | material: layers "9520 - YV 05 - 148 mm trestender (1)" ("Stenderverk tre YTTERVEGG - Isolert" 150.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, MMI, TULLETE TEST, AC_Pset_RenovationAndPhasing
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "9520 - YV 06 - 198 mm trestender 200" | names: "VT-" | material: layers "9520 - YV 06 - 198 mm trestender" ("Stenderverk tre - Isolert" 200.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, AC_Pset_RenovationAndPhasing, TESTTEST, tullball
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Teglstein 104" | names: "VT-" | material: layers "Teglstein 104" ("Teglstein" 104.) | property sets: Pset_WallCommon, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, TESTTEST, MMI, TULLETE TEST
          8 x IFCWALL | type IFCWALLTYPE "9520 - YV 02 - 200 mm trestender, , murplate, tegl 394" | names: "YV07", "YV02", "YV04" (+1 more) | parts: 32 IFCBUILDINGELEMENTPART | property sets: AC_Pset_RenovationAndPhasing, tullball, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, MMI, Pset_WallCommon
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Betong - Strukturell 200" | names: "IV?" | material: layers "Betong - Strukturell 200" ("Betong - Strukturell" 200.) | property sets: MMI, Pset_WallCommon, TESTTEST, TULLETE TEST, Skeisvang Pset: TEST 01 - ifcProject, tullball
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YDC.100" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, TULLETE TEST, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, MMI
          16 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "* PV 01- Påforing stålstender 100mm 3 lag gips 149" | names: "PV01" | material: layers "* PV 01- Påforing stålstender 100mm 3 lag gips" ("Gipsplate - Vegg" 13., "Gipsplate - Vegg" 13., "Gipsplate - Vegg" 13., "Stenderverk stål - Isolert" 100.) | property sets: MMI, Pset_WallCommon, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, tullball
          8 x IFCDOOR | type IFCDOORSTYLE "Dør med sidefelt på side 2" | object type "DOOR" | names: "IDC.110", "IDC.108" | property sets: Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, Pset_DoorCommon, MMI, TULLETE TEST, tullball
          2 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu vertikal multi-rams" | object type "WINDOW" | names: "YVC.100" | property sets: Pset_FireRatingProperties, MMI, TESTTEST, Pset_WindowCommon, TULLETE TEST, AC_Pset_RenovationAndPhasing
          8 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "* IV 02 - Stålstender 100mm, isolert, 2x platekl. to sider 152" | names: "IV02" | material: layers "* IV 02 - Stålstender 100mm, isolert, 2x platekl. to sider" ("Gipsplate - Vegg" 13., "Gipsplate - Vegg" 13., "Stenderverk stål - Isolert" 100., "Gipsplate - Vegg" 13., "Gipsplate - Vegg" 13.) | property sets: Pset_FireRatingProperties, MMI, Pset_WallCommon, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, TESTTEST
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu tre-fags" | object type "WINDOW" | names: "V-" | property sets: Pset_WindowCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, TESTTEST, tullball
          2 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet med 2 sidefelt" | object type "DOOR" | names: "IDC.105" | property sets: Pset_DoorCommon, MMI, Pset_FireRatingProperties, TESTTEST, tullball, TULLETE TEST
          1 x IFCSLAB | type IFCSLABTYPE "Dekke 65" | BASESLAB | names: "Dekke-" | material: layers "Dekke 65" ("Dekke" 65.) | property sets: Pset_SlabCommon, Pset_FireRatingProperties, Pset_CoveringCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST
          24 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Maling 3" | names: "VT-" | material: layers "Maling 2.5" ("Maling" 2.5); layers "Maling 3" ("Maling" 3.) | property sets: Pset_WallCommon, MMI, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, TESTTEST
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Overgangsbeslag amfi mot bygg A 270 x 2" | object type "COLUMN" | names: "S-" | material: "0% 27718788" | property sets: Pset_ColumnCommon, Pset_FireRatingProperties, MMI, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST
          111 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Maling 10" | names: "VT-" | material: layers "Maling 10" ("Maling" 10.) | property sets: Pset_WallCommon, MMI, Pset_FireRatingProperties, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu variabelt" | object type "WINDOW" | names: "YVC.100" | property sets: Pset_FireRatingProperties, Pset_WindowCommon, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, MMI, AC_Pset_RenovationAndPhasing
          2 x IFCSLAB | type IFCSLABTYPE ""9520 - GULV 01 - Betong Påstøp 120 mm, 50 mm trykkfast isolasjon 170" | BASESLAB | names: "Dekke-" | material: layers ""9520 - GULV 01 - Betong Påstøp 120 mm, 50 mm trykkfast isolasjon" ("Isolasjon - Trykkfast" 50.) | property sets: Pset_CoveringCommon, Pset_SlabCommon, Skeisvang Pset: TEST 01 - ifcProject, MMI, Pset_FireRatingProperties, TULLETE TEST
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "*9520 - IV 03 - Stålstender 75mm, uisolert, 1x platekl. en side 88" | names: "VT-" | material: layers "*9520 - IV 03 - Stålstender 75mm, uisolert, 1x platekl. en side" ("Gipsplate - Vegg" 13., "Stenderverk stål - Uisolert" 75.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, MMI, TULLETE TEST
          2 x IFCWALL | type IFCWALLTYPE "9520 - YV 03 - 200 mm trestender, , murplate, tegl 420" | names: "YV03", "YV03a" | parts: 8 IFCBUILDINGELEMENTPART | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, TESTTEST
          1 x IFCWALL | type IFCWALLTYPE "* PV 01- Påforing stålstender 100mm 3 lag gips 149" | names: "PV01" | parts: 4 IFCBUILDINGELEMENTPART | property sets: Pset_WallCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, MMI, TULLETE TEST
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall Type" | names: "CurtainWall-" | parts: 49 IFCMEMBER, 14 IFCPLATE | property sets: Skeisvang Pset: TEST 01 - ifcProject, AC_Pset_RenovationAndPhasing, tullball, TESTTEST, TULLETE TEST, Pset_CurtainWallCommon
          34 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Kryssfiner 25" | names: "VT-" | material: layers "Kryssfiner 25" ("Kryssfiner" 25.) | property sets: MMI, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST, AC_Pset_RenovationAndPhasing
          5 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Kryssfiner" | names: "renne_nedløp_trafo_energisentral" | material: "Kryssfiner" | property sets: AC_Pset_Dimension, Skeisvang Pset: TEST 01 - ifcProject, AC_Pset_RenovationAndPhasing
          2 x IFCCOVERING | type IFCCOVERINGTYPE "9520 - HH 00 - Fast himling gips_Sylomar Akustikk Super T60 KOPI 125" | CEILING | names: "Fast himling" | parts: 4 IFCBUILDINGELEMENTPART | property sets: Pset_CoveringCommon, Pset_FireRatingProperties, AC_Pset_Dimension, Skeisvang Pset: TEST 01 - ifcProject, MMI, TESTTEST
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "* PV03 Stålstender 100mm, påforingt, 2x platekl. en side 122" | names: "PV03" | material: layers "* PV03 Stålstender 100mm, påforingt, 2x platekl. en side" ("Platekledning - Vegg" 10., "OSB-plate" 12., "Stenderverk stål - Uisolert" 100.) | property sets: MMI, Skeisvang Pset: TEST 01 - ifcProject, Pset_WallCommon, TESTTEST, Pset_FireRatingProperties, TULLETE TEST
          6 x IFCDOOR | type IFCDOORSTYLE "Dør med sidefelt på side 2" | object type "DOOR" | names: "IDC.110", "IDC.111" | property sets: MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, Pset_DoorCommon, Pset_FireRatingProperties, TULLETE TEST
          23 x IFCCOVERING | type IFCCOVERINGTYPE "Stenderverk stål - Isolert 50" | CEILING | names: "fast gipshimling" | material: "Stenderverk stål - Isolert" | property sets: Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, Pset_CoveringCommon, AC_Pset_Dimension, TESTTEST
          2 x IFCSLAB | type IFCSLABTYPE "Systemhimling - 60x60 50" | BASESLAB | names: "Systemhimling 600 x 600 E-kant", "Dekke-" | material: layers "Systemhimling - 60x60 50" ("Systemhimling - 60x60" 50.) | property sets: Pset_CoveringCommon, MMI, Pset_SlabCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, tullball
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Stenderverk stål - Isolert 100" | names: "skjørt" | material: layers "Stenderverk stål - Isolert 100" ("Stenderverk stål - Isolert" 100.) | property sets: MMI, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, Pset_WallCommon, TULLETE TEST, tullball
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg HOVEDBYGG 350" | names: "VT-" | material: layers "Yttervegg HOVEDBYGG 350" ("Yttervegg HOVEDBYGG" 350.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          2 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu vertikal multi-rams" | object type "WINDOW" | names: "V-" | property sets: Pset_FireRatingProperties, Pset_WindowCommon, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, AC_Pset_RenovationAndPhasing, tullball
          190 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 1 150" | names: "VT-" | material: layers "Yttervegg 1 150" ("Yttervegg 1" 150.) | property sets: Pset_WallCommon, MMI, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          10 x IFCWALL | type IFCWALLTYPE "Yttervegg 1 350" | names: "VT-" | material: "Yttervegg 1" | property sets: Pset_FireRatingProperties, Pset_WallCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, TESTTEST
          3 x IFCWALL | type IFCWALLTYPE "Yttervegg HOVEDBYGG 350" | names: "VT-" | material: "Yttervegg HOVEDBYGG" | property sets: MMI, Pset_FireRatingProperties, Pset_WallCommon, TESTTEST, TULLETE TEST, Skeisvang Pset: TEST 01 - ifcProject
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          2 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "YD-" | property sets: Pset_FireRatingProperties, Pset_DoorCommon, MMI, TULLETE TEST, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject
          7 x IFCWALL | type IFCWALLTYPE "Yttervegg 1 200" | names: "VT-" | material: "Yttervegg 1" | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, tullball, TULLETE TEST
          13 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 1 200" | names: "VT-" | material: layers "Yttervegg 1 200" ("Yttervegg 1" 200.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, MMI, TULLETE TEST
          6 x IFCWALL | type IFCWALLTYPE "Yttervegg 1 300" | names: "VT-" | material: "Yttervegg 1" | property sets: Pset_WallCommon, MMI, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          1 x IFCSLAB | type IFCSLABTYPE "Dekke 220" | BASESLAB | names: "Dekke-" | material: layers "Dekke 220" ("Dekke" 220.) | property sets: Pset_CoveringCommon, Pset_SlabCommon, MMI, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-" | property sets: Pset_FireRatingProperties, MMI, Pset_DoorCommon, TULLETE TEST, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST
          3 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-", "IDB.100", "IDA.100" | property sets: Pset_FireRatingProperties, Pset_DoorCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, TESTTEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, MMI, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          4 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-", "IDA.100" | property sets: MMI, Pset_FireRatingProperties, Pset_DoorCommon, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør med overlys" | object type "DOOR" | names: "IDA.100" | property sets: Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, MMI, TESTTEST, Pset_DoorCommon, TULLETE TEST
          32 x IFCDOOR | type IFCDOORSTYLE "Dør med sidefelt på side 2" | object type "DOOR" | names: "IDA.100", "YD-", "IDB.100" (+2 more) | property sets: Pset_DoorCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST, MMI
          3 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "IDA.100", "IDB.100" | property sets: Pset_FireRatingProperties, Pset_DoorCommon, Skeisvang Pset: TEST 01 - ifcProject, MMI, TESTTEST, TULLETE TEST
          51 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 1 100" | names: "VT-" | material: layers "Yttervegg 1 100" ("Yttervegg 1" 100.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, tullball
          8 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "IDA.100", "IDB.100", "YD-" (+1 more) | property sets: MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, Pset_DoorCommon, AC_Pset_RenovationAndPhasing, Pset_FireRatingProperties
          2 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, MMI, TESTTEST, TULLETE TEST, Skeisvang Pset: TEST 01 - ifcProject
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          5 x IFCWALL | type IFCWALLTYPE "Yttervegg 1 150" | names: "VT-" | material: "Yttervegg 1" | property sets: MMI, Pset_WallCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          1 x IFCWALL | type IFCWALLTYPE "Yttervegg 1 250" | names: "VT-" | material: "Yttervegg 1" | property sets: MMI, Pset_FireRatingProperties, Pset_WallCommon, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet med overlys" | object type "DOOR" | names: "IDB.100" | property sets: Pset_DoorCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST, Pset_FireRatingProperties
          5 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu" | object type "WINDOW" | names: "V-" | property sets: Pset_WindowCommon, Skeisvang Pset: TEST 01 - ifcProject, MMI, Pset_FireRatingProperties, TESTTEST, AC_Pset_RenovationAndPhasing
          1 x IFCWALL | type IFCWALLTYPE "Yttervegg 1 100" | names: "VT-" | material: "Yttervegg 1" | property sets: Pset_WallCommon, MMI, Pset_FireRatingProperties, TULLETE TEST, TESTTEST, AC_Pset_RenovationAndPhasing
          4 x IFCDOOR | type IFCDOORSTYLE "Dør med sidefelt på side 2 og overlys" | object type "DOOR" | names: "YD-", "IDB.100", "YDB.100" | property sets: Pset_DoorCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, tullball, TESTTEST
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Maling 5" | names: "VT-" | material: layers "Maling 5" ("Maling" 5.) | property sets: MMI, Pset_WallCommon, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, TESTTEST, tullball
          13 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 1 240" | names: "VT-" | material: layers "Yttervegg 1 240" ("Yttervegg 1" 240.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, TESTTEST, TULLETE TEST, Skeisvang Pset: TEST 01 - ifcProject
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Limtre 250 x 250" | object type "COLUMN" | names: "S-" | material: "Limtre" | property sets: Pset_ColumnCommon, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, Pset_FireRatingProperties, MMI, BaseQuantities
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Gips 250 x 250" | object type "COLUMN" | names: "S-" | material: "Gips" | property sets: Pset_ColumnCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, tullball, AC_Pset_RenovationAndPhasing
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Betong - Prefab 250 x 300" | object type "COLUMN" | names: "S-" | material: "Betong - Prefab" | property sets: Pset_FireRatingProperties, MMI, Pset_ColumnCommon, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, tullball
          13 x IFCDOOR | type IFCDOORSTYLE "Dør med sidefelt på side 2" | object type "DOOR" | names: "IDA.100", "IDB.100", "YD-" (+1 more) | property sets: MMI, Pset_FireRatingProperties, Pset_DoorCommon, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, tullball
          3 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-", "IDA.100" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, TESTTEST, MMI, TULLETE TEST, tullball
          1 x IFCSLAB | type IFCSLABTYPE "Dekke 1000" | BASESLAB | names: "Dekke-" | material: layers "Dekke 1000" ("Dekke" 1000.) | property sets: Pset_CoveringCommon, Pset_FireRatingProperties, MMI, Pset_SlabCommon, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST
          4 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, MMI, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, TULLETE TEST, tullball, MMI
          3 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "IDB.100", "IDA.100" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, MMI, TESTTEST, TULLETE TEST, tullball
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "IDB.100" | property sets: Pset_FireRatingProperties, Pset_DoorCommon, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, MMI, TULLETE TEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "IDA.100" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "IDA.100" | property sets: BaseQuantities, tullball, AC_Pset_RenovationAndPhasing, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, MMI
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "IDA.100" | property sets: Pset_FireRatingProperties, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, Pset_DoorCommon, MMI, TULLETE TEST
          2 x IFCDOOR | type IFCDOORSTYLE "Dør med overlys" | object type "DOOR" | names: "IDA.100" | property sets: MMI, Pset_DoorCommon, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, tullball, Pset_FireRatingProperties
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 1 120" | names: "VT-" | material: layers "Yttervegg 1 120" ("Yttervegg 1" 120.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, AC_Pset_RenovationAndPhasing, tullball
          1 x IFCDOOR | type IFCDOORSTYLE "Dør med overlys" | object type "DOOR" | names: "IDA.100" | property sets: Pset_FireRatingProperties, MMI, Pset_DoorCommon, TESTTEST, TULLETE TEST, Skeisvang Pset: TEST 01 - ifcProject
          2 x IFCSLAB | type IFCSLABTYPE "Dekke 300" | BASESLAB | names: "Dekke-" | material: layers "Dekke 300" ("Dekke" 300.) | property sets: Pset_CoveringCommon, Pset_SlabCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, MMI, TULLETE TEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør med overlys" | object type "DOOR" | names: "IDA.100" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, tullball, TULLETE TEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, BaseQuantities, AC_Pset_RenovationAndPhasing, Pset_FireRatingProperties
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 1 75" | names: "VT-" | material: layers "Yttervegg 1 75" ("Yttervegg 1" 75.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, MMI
          5 x IFCDOOR | type IFCDOORSTYLE "Dør med sidefelt på side 2 og overlys" | object type "DOOR" | names: "IDB.100", "IDA.100", "IDA-100" | property sets: Pset_DoorCommon, MMI, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "IDB.100" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, MMI, TESTTEST, tullball
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "IDB.100" | property sets: MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST, Pset_FireRatingProperties, Pset_DoorCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu" | object type "WINDOW" | names: "V-" | property sets: Pset_FireRatingProperties, Pset_WindowCommon, BaseQuantities, AC_Pset_RenovationAndPhasing, MMI, tullball
          1 x IFCDOOR | type IFCDOORSTYLE "Dør med sidefelt på side 1" | object type "DOOR" | names: "IDA.100" | property sets: Pset_FireRatingProperties, Pset_DoorCommon, MMI, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, AC_Pset_RenovationAndPhasing
          3 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, Skeisvang Pset: TEST 01 - ifcProject, MMI, TULLETE TEST, TESTTEST, tullball
          12 x IFCSLAB | type IFCSLABTYPE "Dekke 100" | BASESLAB | names: "Dekke-" | material: layers "Dekke 100" ("Dekke" 100.) | property sets: TESTTEST, AC_Pset_RenovationAndPhasing, TULLETE TEST, Skeisvang Pset: TEST 01 - ifcProject, MMI, Pset_FireRatingProperties
          8 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Curtain Wall Type" | names: "Glassvegg-" | parts: 425 IFCBUILDINGELEMENTPROXY | property sets: AC_Pset_Dimension, Skeisvang Pset: TEST 01 - ifcProject, AC_Pset_RenovationAndPhasing
          1 x IFCBEAM | type IFCBEAMTYPE "Betong - Prefab 500 x 450" | object type "BEAM" | names: "B-" | material: "Betong - Prefab" | property sets: MMI, Pset_BeamCommon, Pset_FireRatingProperties, TULLETE TEST, TESTTEST, tullball
          2 x IFCSTAIR | names: "Trapp-" | parts: 6 IFCBUILDINGELEMENTPART | property sets: Pset_StairCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, MMI, TESTTEST, TULLETE TEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-" | property sets: Pset_FireRatingProperties, Pset_DoorCommon, MMI, TULLETE TEST, TESTTEST, tullball
          3 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "IDA.100", "YD-" | property sets: Pset_DoorCommon, tullball, TESTTEST, MMI, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST
          3 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "IDA.100", "YD-" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, MMI, TESTTEST, TULLETE TEST, BaseQuantities
          2 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "IDA.100" | property sets: MMI, Pset_DoorCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          2 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "IDA.100" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, tullball
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "IDB.100" | property sets: Pset_DoorCommon, MMI, Pset_FireRatingProperties, TESTTEST, TULLETE TEST, tullball
          94 x IFCSLAB | type IFCSLABTYPE "Dekke 200" | BASESLAB | names: "Dekke-" | material: layers "Dekke 200" ("Dekke" 200.) | property sets: Pset_SlabCommon, MMI, Pset_CoveringCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST
          1 x IFCSLAB | type IFCSLABTYPE "Dekke 270" | BASESLAB | names: "Dekke-" | material: layers "Dekke 270" ("Dekke" 270.) | property sets: Pset_SlabCommon, Pset_CoveringCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST
          1 x IFCSLAB | type IFCSLABTYPE "Dekke 600" | BASESLAB | names: "Dekke-" | material: layers "Dekke 600" ("Dekke" 600.0000000000001) | property sets: Pset_FireRatingProperties, Pset_SlabCommon, Pset_CoveringCommon, MMI, TESTTEST, tullball
          4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Aluminium" | names: "Terreng-01" | material: "Aluminium" | property sets: Skeisvang Pset: TEST 01 - ifcProject, AC_Pset_Dimension, AC_Pset_RenovationAndPhasing
          99 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu variabelt" | object type "WINDOW" | names: "YVA.100", "YVA.200", "YVB.100" | property sets: MMI, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, Pset_WindowCommon, TESTTEST, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet med overlys" | object type "DOOR" | names: "YDB.100" | property sets: Pset_DoorCommon, MMI, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, BaseQuantities
          260 x IFCSLAB | type IFCSLABTYPE "Teglstein 50" | BASESLAB | names: "Dekke-" | material: layers "Teglstein 50" ("Teglstein" 49.99999999999999) | property sets: Pset_CoveringCommon, Pset_SlabCommon, MMI, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST
          17 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg HOVEDBYGG 275" | names: "VT-" | material: layers "Yttervegg HOVEDBYGG 275" ("Yttervegg HOVEDBYGG" 275.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, MMI, TESTTEST, TULLETE TEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet med overlys" | object type "DOOR" | names: "YDA.100" | property sets: Pset_DoorCommon, MMI, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, BaseQuantities, AC_Pset_RenovationAndPhasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg HOVEDBYGG 318" | names: "VT-" | material: layers "Yttervegg HOVEDBYGG 318" ("Yttervegg HOVEDBYGG" 318.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          4 x IFCCOVERING | type IFCCOVERINGTYPE "Stål 320" | CEILING | names: "Beslag rekkverk gangbro" | material: "Stål" | property sets: AC_Pset_Dimension, Pset_CoveringCommon, MMI, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "Skyvedør med sidefelt på side 1 og overlys" | object type "DOOR" | names: "YD-" | property sets: Pset_FireRatingProperties, Pset_DoorCommon, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST, MMI
          1 x IFCDOOR | type IFCDOORSTYLE "Skyvedør med overlys" | object type "DOOR" | names: "YD-" | property sets: MMI, Pset_FireRatingProperties, Pset_DoorCommon, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, tullball
          191 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Tre 25" | names: "VT-" | material: layers "Tre 25" ("Tre" 25.) | property sets: Pset_WallCommon, tullball, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, MMI
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 1 50" | names: "VT-" | material: layers "Yttervegg 1 50" ("Yttervegg 1" 50.) | property sets: Pset_FireRatingProperties, Pset_WallCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, tullball, TULLETE TEST
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Stål - Overflatebehandlet D70" | object type "COLUMN" | names: "S-" | material: "Stål - Overflatebehandlet" | property sets: Pset_ColumnCommon, MMI, Pset_FireRatingProperties, TESTTEST, tullball, Skeisvang Pset: TEST 01 - ifcProject
          2 x IFCDOOR | type IFCDOORSTYLE "Skyvedør med pocketkarm" | object type "DOOR" | names: "YD-" | property sets: MMI, TESTTEST, AC_Pset_RenovationAndPhasing, tullball, TULLETE TEST, Skeisvang Pset: TEST 01 - ifcProject
          2 x IFCCOLUMN | type IFCCOLUMNTYPE "Stål - Overflatebehandlet D30" | object type "COLUMN" | names: "S-" | material: "Stål - Overflatebehandlet" | property sets: Pset_ColumnCommon, Pset_FireRatingProperties, MMI, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, AC_Pset_RenovationAndPhasing
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 1 250" | names: "VT-" | material: layers "Yttervegg 1 250" ("Yttervegg 1" 250.) | property sets: Pset_FireRatingProperties, MMI, Pset_WallCommon, Skeisvang Pset: TEST 01 - ifcProject, AC_Pset_RenovationAndPhasing, TESTTEST
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 1 30" | names: "VT-" | material: layers "Yttervegg 1 30" ("Yttervegg 1" 30.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, MMI
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "IDB.100" | property sets: Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, tullball, TULLETE TEST, MMI
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Innervegg 150" | names: "VT-" | material: layers "Innervegg 150" ("Innervegg" 150.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tekst 3D" | names: "Stol-" | property sets: AC_Pset_Dimension, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, Skeisvang Pset: TEST 01 - ifcProject, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "IDA.100" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, tullball
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "IDB.100" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, MMI, tullball
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 1 160" | names: "VT-" | material: layers "Yttervegg 1 160" ("Yttervegg 1" 160.) | property sets: Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, Pset_WallCommon, tullball
          1 x IFCDOOR | type IFCDOORSTYLE "Skyvedør med 2 sidefelt og overlys" | object type "DOOR" | names: "YD-" | property sets: Pset_FireRatingProperties, Pset_DoorCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, tullball, BaseQuantities
          2 x IFCSLAB | type IFCSLABTYPE "Dekke 450" | BASESLAB | names: "Dekke-" | material: layers "Dekke 450" ("Dekke" 449.9999999999602) | property sets: Pset_FireRatingProperties, Pset_SlabCommon, Pset_CoveringCommon, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, MMI
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Stål 40" | names: "VT-" | material: layers "Stål 40" ("Stål" 40.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, MMI, TESTTEST, TULLETE TEST
          27 x IFCSLAB | type IFCSLABTYPE "Stål 30" | BASESLAB | names: "Dekke-" | material: layers "Stål 30" ("Stål" 30.) | property sets: Pset_SlabCommon, Pset_CoveringCommon, AC_Pset_RenovationAndPhasing, Skeisvang Pset: TEST 01 - ifcProject, BaseQuantities, tullball
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Sink" | names: "gesimsbeslag_trafo_energisentral" | material: "Sink" | property sets: AC_Pset_Dimension, Skeisvang Pset: TEST 01 - ifcProject, AC_Pset_RenovationAndPhasing
          1 x IFCSLAB | type IFCSLABTYPE "Aluminium 3800" | BASESLAB | names: "Dekke-" | material: layers "Aluminium 3800" ("Aluminium" 3800.000031360505) | property sets: Pset_CoveringCommon, Pset_SlabCommon, MMI, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 1 275" | names: "VT-" | material: layers "Yttervegg 1 275" ("Yttervegg 1" 275.) | property sets: Pset_FireRatingProperties, MMI, Pset_WallCommon, TULLETE TEST, TESTTEST, tullball
          10 x IFCSLAB | type IFCSLABTYPE "Dekke 5980" | BASESLAB | names: "Dekke-" | material: layers "Dekke 5980" ("Dekke" 5980.000000000025) | property sets: Pset_SlabCommon, Pset_CoveringCommon, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, MMI, TULLETE TEST
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 1 10" | names: "VT-" | material: layers "Yttervegg 1 10" ("Yttervegg 1" 10.) | property sets: Pset_FireRatingProperties, Pset_WallCommon, TULLETE TEST, TESTTEST, MMI, Skeisvang Pset: TEST 01 - ifcProject
          1 x IFCSLAB | type IFCSLABTYPE "Dekke 165" | BASESLAB | names: "Dekke-" | material: layers "Dekke 165" ("Dekke" 165.0000000000347) | property sets: Pset_CoveringCommon, Pset_SlabCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, MMI, TULLETE TEST
          1 x IFCSLAB | type IFCSLABTYPE "Dekke 470" | BASESLAB | names: "Dekke-" | material: layers "Dekke 470" ("Dekke" 470.0000000000028) | property sets: Pset_SlabCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, MMI, TULLETE TEST
          2 x IFCSLAB | type IFCSLABTYPE "Dekke 385" | BASESLAB | names: "Dekke-" | material: layers "Dekke 385" ("Dekke" 385.0000000000016) | property sets: Pset_SlabCommon, Pset_CoveringCommon, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, TULLETE TEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet med overlys" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, Skeisvang Pset: TEST 01 - ifcProject, MMI, Pset_FireRatingProperties, BaseQuantities, TESTTEST
          1 x IFCSLAB | type IFCSLABTYPE "Stein - Skiferheller 150" | BASESLAB | names: "Dekke-" | material: layers "Stein - Skiferheller 150" ("Stein - Skiferheller" 150.) | property sets: Pset_SlabCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, Pset_CoveringCommon, TULLETE TEST
          3 x IFCCOLUMN | type IFCCOLUMNTYPE "Stål D300" | object type "COLUMN" | names: "S-" | material: "Stål" | property sets: Pset_ColumnCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, MMI, tullball
          4 x IFCWALL | type IFCWALLTYPE "* YV 03 - 200 mm trestender, , murplate utvendig, sjikt for solavskjerming, tegl 464" | names: "YV01a", "YV05" | parts: 16 IFCBUILDINGELEMENTPART | property sets: Pset_FireRatingProperties, TESTTEST, TULLETE TEST, Pset_WallCommon, AC_Pset_RenovationAndPhasing, MMI
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu variabelt" | object type "WINDOW" | names: "YVC.100" | property sets: Pset_WindowCommon, MMI, TESTTEST, TULLETE TEST, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties
          7 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu variabelt" | object type "WINDOW" | names: "YVC.100" | property sets: Pset_FireRatingProperties, MMI, Pset_WindowCommon, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, tullball
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu variabelt" | object type "WINDOW" | names: "YVC.100" | property sets: Pset_WindowCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, tullball
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu variabelt" | object type "WINDOW" | names: "YVC.100" | property sets: Pset_WindowCommon, MMI, AC_Pset_RenovationAndPhasing, TULLETE TEST, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg tegl 104" | names: "VT-", "YV08", "YV06" | material: layers "Yttervegg tegl 104" ("Yttervegg tegl" 104.) | property sets: MMI, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, Pset_WallCommon, TULLETE TEST, tullball
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu variabelt" | object type "WINDOW" | names: "YVC.100" | property sets: Pset_WindowCommon, tullball, MMI, Pset_FireRatingProperties, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Innervegg 200" | names: "IV?" | material: layers "Innervegg 200" ("Innervegg" 200.) | property sets: Pset_FireRatingProperties, Pset_WallCommon, MMI, TESTTEST, TULLETE TEST, Skeisvang Pset: TEST 01 - ifcProject
          2 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "IDC.101", "IDC.102" | property sets: Pset_FireRatingProperties, TULLETE TEST, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, MMI, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "IDC.101" | property sets: Pset_DoorCommon, MMI, TESTTEST, TULLETE TEST, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "*9520 - IV LYD4 - 60 dB : 3x13 mm gips, 1x100mm stålstender 149" | names: "PV01" | material: layers "*9520 - IV LYD4 - 60 dB : 3x13 mm gips, 1x100mm stålstender" ("Gipsplate - Vegg" 13., "Gipsplate - Vegg" 13., "Gipsplate - Vegg" 13., "Stenderverk stål - Isolert" 100.) | property sets: MMI, Skeisvang Pset: TEST 01 - ifcProject, Pset_WallCommon, Pset_FireRatingProperties, TULLETE TEST, TESTTEST
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "* PV 02- Påforing stålstender 100mm 2 lag gips 136" | names: "IV19" | material: layers "* PV 02- Påforing stålstender 100mm 2 lag gips" ("Gipsplate - Vegg" 13., "Gipsplate - Vegg" 13., "Stenderverk stål - Isolert" 100.) | property sets: MMI, Pset_WallCommon, Skeisvang Pset: TEST 01 - ifcProject, BaseQuantities, AC_Pset_RenovationAndPhasing, tullball
          6 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu" | object type "WINDOW" | names: "IVC.100", "YVC.200" | property sets: Pset_WindowCommon, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, MMI, tullball, TESTTEST
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "*9520 - IV LYD1 - 35/37 dB: 1x13 mm gips, 1x100mm stålstender, 1x13mm gips 126" | names: "IV01?" | material: layers "*9520 - IV LYD1 - 35/37 dB: 1x13 mm gips, 1x100mm stålstender, 1x13mm gips" ("Gipsplate - Vegg" 13., "Stenderverk stål - Isolert" 100., "Gipsplate - Vegg" 13.) | property sets: TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, Pset_WallCommon, MMI, Pset_FireRatingProperties, TULLETE TEST
          2 x IFCSLAB | type IFCSLABTYPE "Dekke 50" | BASESLAB | names: "Dekke-" | material: layers "Dekke 50" ("Dekke" 50.) | property sets: Pset_CoveringCommon, Pset_SlabCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, TESTTEST
          5 x IFCSLAB | type IFCSLABTYPE "Tre 50" | BASESLAB | names: "Dekke-" | material: layers "Tre 50" ("Tre" 50.) | property sets: Pset_CoveringCommon, Pset_SlabCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, tullball, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "Isolasjon - Trykkfast 200" | BASESLAB | names: "Dekke-" | material: layers "Isolasjon - Trykkfast 200" ("Isolasjon - Trykkfast" 200.) | property sets: Skeisvang Pset: TEST 01 - ifcProject, Pset_CoveringCommon, MMI, Pset_FireRatingProperties, Pset_SlabCommon, TULLETE TEST
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "* IV 03- 48/50 dB: 3x13 mm gips, 1X100mm stålstender, 3x13mm gips 178" | names: "IV03" | material: layers "* IV 03- 48/50 dB: 3x13 mm gips, 1X100mm stålstender, 3x13mm gips" ("Gipsplate - Vegg" 13., "Gipsplate - Vegg" 13., "Gipsplate - Vegg" 13., "Stenderverk stål - Isolert" 100., "Gipsplate - Vegg" 13., "Gipsplate - Vegg" 13., "Gipsplate - Vegg" 13.) | property sets: MMI, Pset_WallCommon, BaseQuantities, AC_Pset_RenovationAndPhasing, TULLETE TEST, Skeisvang Pset: TEST 01 - ifcProject
          1 x IFCWALL | type IFCWALLTYPE "*9520 - IV LYD6 - 70 dB: 3x13mm gips, 100mm stålstender, 250mmleca lydblokk, 100mm stålstender, 3x13mm gips 548" | names: "PV01" | parts: 9 IFCBUILDINGELEMENTPART | property sets: MMI, Pset_WallCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, tullball, TULLETE TEST
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Innervegg 100" | names: "VT-" | material: layers "Innervegg 100" ("Innervegg" 100.) | property sets: MMI, Pset_FireRatingProperties, tullball, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, Pset_WallCommon
          24 x IFCSLAB | type IFCSLABTYPE "Gulvplanker 183" | BASESLAB | names: "Dekke-" | material: layers "Gulvplanker 183.333" ("Gulvplanker" 183.333309984409) | property sets: Pset_CoveringCommon, Pset_SlabCommon, MMI, Pset_FireRatingProperties, TULLETE TEST, TESTTEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet asymmetrisk" | object type "DOOR" | names: "IDC.103" | property sets: Pset_FireRatingProperties, Pset_DoorCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet asymmetrisk" | object type "DOOR" | names: "IDC.103" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, AC_Pset_RenovationAndPhasing
          1 x IFCSLAB | type IFCSLABTYPE "Platekledning - Vegg 50" | BASESLAB | names: "fast gipshimling" | material: layers "Platekledning - Vegg 50" ("Platekledning - Vegg" 50.) | property sets: Pset_CoveringCommon, Pset_FireRatingProperties, Pset_SlabCommon, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Kart - koordinatobjekt 1" | names: "Stol-" | property sets: AC_Pset_Dimension, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, MMI, TULLETE TEST, tullball
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Tre 15" | names: "VT-" | material: layers "Tre 15" ("Tre" 15.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, TULLETE TEST, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Tre 45" | names: "VT-" | material: layers "Tre 45" ("Tre" 45.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu tre-fags" | object type "WINDOW" | names: "V-" | property sets: Pset_WindowCommon, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, MMI, Pset_FireRatingProperties, TULLETE TEST
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Gulvbelegg 5" | FLOORING | names: "Banebelegg" | material: "Gulvbelegg" | property sets: AC_Pset_Dimension, Pset_CoveringCommon, Pset_FireRatingProperties, MMI, AC_Pset_RenovationAndPhasing, TESTTEST
          14 x IFCCOVERING | type IFCCOVERINGTYPE "Gulvbelegg 3" | FLOORING | names: "Banebelegg" | material: "Gulvbelegg" | property sets: Pset_CoveringCommon, Pset_FireRatingProperties, MMI, AC_Pset_Dimension, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST
          2 x IFCCOVERING | type IFCCOVERINGTYPE "Gulvplanker 20" | FLOORING | names: "Parkett" | material: "Gulvplanker" | property sets: Pset_CoveringCommon, Pset_FireRatingProperties, AC_Pset_Dimension, MMI, TESTTEST, AC_Pset_RenovationAndPhasing
          40 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Tre 5" | names: "VT-" | material: layers "Tre 5" ("Tre" 5.) | property sets: Pset_WallCommon, Skeisvang Pset: TEST 01 - ifcProject, MMI, TULLETE TEST, Pset_FireRatingProperties, TESTTEST
          90 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Isolasjon - Myk 225" | names: "VT-" | material: layers "Isolasjon - Myk 225" ("Isolasjon - Myk" 225.) | property sets: Pset_WallCommon, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, MMI, Pset_FireRatingProperties, tullball
          4 x IFCSLAB | type IFCSLABTYPE "Tre 460" | BASESLAB | names: "Dekke-" | material: layers "Tre 460" ("Tre" 460.0000000000009) | property sets: Pset_CoveringCommon, Pset_SlabCommon, MMI, Pset_FireRatingProperties, tullball, TESTTEST
          10 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Tre 225" | names: "VT-" | material: layers "Tre 225" ("Tre" 225.) | property sets: Pset_WallCommon, MMI, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          1 x IFCSLAB | type IFCSLABTYPE "Aluminium 3110" | BASESLAB | names: "Dekke-" | material: layers "Aluminium 3110" ("Aluminium" 3110.) | property sets: Pset_CoveringCommon, Pset_SlabCommon, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, MMI, Pset_FireRatingProperties
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Panel innvendig - Liggende m/gliper 25" | names: "VT-" | material: layers "Panel innvendig - Liggende m/gliper 25" ("Panel innvendig - Liggende m/gliper" 25.) | property sets: MMI, Pset_WallCommon, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, tullball, AC_Pset_RenovationAndPhasing
          3 x IFCCOLUMN | type IFCCOLUMNTYPE "Aluminium D60" | object type "COLUMN" | names: "S-" | material: "Aluminium" | property sets: Pset_ColumnCommon, Pset_FireRatingProperties, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, MMI, tullball
          5 x IFCSLAB | type IFCSLABTYPE "Tre 150" | BASESLAB | names: "Dekke-" | material: layers "Tre 150" ("Tre" 150.) | property sets: Pset_CoveringCommon, Pset_SlabCommon, MMI, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST
          5 x IFCSLAB | type IFCSLABTYPE "Tre 300" | BASESLAB | names: "Dekke-" | material: layers "Tre 300" ("Tre" 300.0000000000043) | property sets: Pset_CoveringCommon, Pset_FireRatingProperties, TULLETE TEST, Pset_SlabCommon, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject
          4 x IFCSLAB | type IFCSLABTYPE "Tre 450" | BASESLAB | names: "Dekke-" | material: layers "Tre 450" ("Tre" 450.0000000000028) | property sets: Pset_FireRatingProperties, Pset_SlabCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          5 x IFCSLAB | type IFCSLABTYPE "Tre 307" | BASESLAB | names: "Dekke-" | material: layers "Tre 306.667" ("Tre" 306.6666666666684) | property sets: Pset_FireRatingProperties, Pset_SlabCommon, Pset_CoveringCommon, MMI, TESTTEST, tullball
          5 x IFCSLAB | type IFCSLABTYPE "Tre 153" | BASESLAB | names: "Dekke-" | material: layers "Tre 153.333" ("Tre" 153.3333333333324) | property sets: Pset_CoveringCommon, Pset_FireRatingProperties, Pset_SlabCommon, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, tullball
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Påstøp 17" | FLOORING | names: "Slipt betong" | material: "Påstøp" | property sets: AC_Pset_RenovationAndPhasing, BaseQuantities, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, MMI, Pset_FireRatingProperties
          1 x IFCSLAB | type IFCSLABTYPE "Tre 200" | BASESLAB | names: "Dekke-" | material: layers "Tre 200" ("Tre" 199.9999999999993) | property sets: Pset_CoveringCommon, Pset_SlabCommon, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, MMI, TULLETE TEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet asymmetrisk" | object type "DOOR" | names: "IDC.109" | property sets: Pset_FireRatingProperties, MMI, Pset_DoorCommon, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          2 x IFCCOVERING | type IFCCOVERINGTYPE "Stål 50" | CEILING | names: "fotskraperist" | material: "Stål" | property sets: Pset_CoveringCommon, AC_Pset_Dimension, Pset_FireRatingProperties, MMI, AC_Pset_RenovationAndPhasing, TESTTEST
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Panel innvendig - Liggende 25" | names: "VT-" | material: layers "Panel innvendig - Liggende 25" ("Panel innvendig - Liggende" 25.) | property sets: Pset_FireRatingProperties, Pset_WallCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, AC_Pset_RenovationAndPhasing
          9 x IFCCOVERING | type IFCCOVERINGTYPE "Gulvplanker 35" | FLOORING | names: "Parkett" | material: "Gulvplanker" | property sets: Pset_CoveringCommon, AC_Pset_Dimension, MMI, Skeisvang Pset: TEST 01 - ifcProject, AC_Pset_RenovationAndPhasing, BaseQuantities
          6 x IFCCOVERING | type IFCCOVERINGTYPE "Gulvplanker 367" | FLOORING | names: "Parkett" | material: "Gulvplanker" | property sets: Pset_CoveringCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, AC_Pset_Dimension, BaseQuantities
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Gulvplanker 366" | FLOORING | names: "Parkett" | material: "Gulvplanker" | property sets: AC_Pset_Dimension, Pset_CoveringCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, MMI, BaseQuantities
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Gulvplanker 367" | FLOORING | names: "Parkett" | material: "Gulvplanker" | property sets: Pset_CoveringCommon, Pset_FireRatingProperties, MMI, AC_Pset_RenovationAndPhasing, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Gulvplanker 367" | FLOORING | names: "Parkett" | material: "Gulvplanker" | property sets: Pset_CoveringCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, MMI, TESTTEST, AC_Pset_RenovationAndPhasing
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Gulvplanker 367" | FLOORING | names: "Parkett" | material: "Gulvplanker" | property sets: Pset_CoveringCommon, AC_Pset_Dimension, MMI, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Gulvplanker 733" | FLOORING | names: "Parkett" | material: "Gulvplanker" | property sets: Pset_CoveringCommon, AC_Pset_Dimension, Pset_FireRatingProperties, MMI, TESTTEST, AC_Pset_RenovationAndPhasing
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Tre 135" | FLOORING | names: "Parkett" | material: "Tre" | property sets: Pset_CoveringCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, MMI, AC_Pset_RenovationAndPhasing, AC_Pset_Dimension
          8 x IFCCOVERING | type IFCCOVERINGTYPE "Tre 150" | FLOORING | names: "Parkett" | material: "Tre" | property sets: Pset_CoveringCommon, AC_Pset_Dimension, MMI, TESTTEST, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Tre 2045" | FLOORING | names: "Parkett" | material: "Tre" | property sets: Pset_CoveringCommon, Pset_FireRatingProperties, MMI, AC_Pset_Dimension, Skeisvang Pset: TEST 01 - ifcProject, BaseQuantities
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Tre 2412" | FLOORING | names: "Parkett" | material: "Tre" | property sets: TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, AC_Pset_Dimension, Pset_CoveringCommon, MMI
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Tre 636" | FLOORING | names: "Parkett" | material: "Tre" | property sets: Pset_CoveringCommon, AC_Pset_Dimension, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Tre 627" | FLOORING | names: "Parkett" | material: "Tre" | property sets: Pset_CoveringCommon, AC_Pset_Dimension, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, MMI, AC_Pset_RenovationAndPhasing
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Tre 532" | FLOORING | names: "Parkett" | material: "Tre" | property sets: Pset_CoveringCommon, AC_Pset_Dimension, MMI, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, AC_Pset_RenovationAndPhasing
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Tre 1678" | FLOORING | names: "Parkett" | material: "Tre" | property sets: Pset_FireRatingProperties, AC_Pset_Dimension, Pset_CoveringCommon, MMI, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject
          3 x IFCCOVERING | type IFCCOVERINGTYPE "Tre 1280" | FLOORING | names: "Parkett" | material: "Tre" | property sets: AC_Pset_Dimension, Pset_CoveringCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, MMI, AC_Pset_RenovationAndPhasing
          2 x IFCCOVERING | type IFCCOVERINGTYPE "Tre 1280" | FLOORING | names: "Parkett" | material: "Tre" | property sets: Pset_CoveringCommon, Pset_FireRatingProperties, AC_Pset_Dimension, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, AC_Pset_RenovationAndPhasing
          2 x IFCCOVERING | type IFCCOVERINGTYPE "Tre 898" | FLOORING | names: "Parkett" | material: "Tre" | property sets: Pset_FireRatingProperties, Pset_CoveringCommon, AC_Pset_Dimension, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST
          15 x IFCCOVERING | type IFCCOVERINGTYPE "Platekledning - Himling 30" | CEILING | names: "Trolltekt el. tilsv." | material: "Platekledning - Himling" | property sets: Pset_CoveringCommon, AC_Pset_Dimension, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "Tre 410" | BASESLAB | names: "Dekke-" | material: layers "Tre 410" ("Tre" 410.0000000000001) | property sets: Pset_SlabCommon, Pset_CoveringCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, TESTTEST
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Bordkledning - Stående 12" | names: "VT-" | material: layers "Bordkledning - Stående 12" ("Bordkledning - Stående" 12.) | property sets: Pset_WallCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, TESTTEST, TULLETE TEST
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "*9520 - MDD - Bassabsorbent vegg 262" | names: "VT-" | material: layers "*9520 - MDD - Bassabsorbent vegg" ("Panel innvendig - Liggende" 12., "Bjelkelag - Isolert" 200.) | property sets: MMI, Pset_WallCommon, TULLETE TEST, TESTTEST, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject
          3 x IFCCOVERING | type IFCCOVERINGTYPE "Dekke 20" | CEILING | names: "tegl over åpning" | material: "Dekke" | property sets: AC_Pset_Dimension, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, AC_Pset_RenovationAndPhasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Tre 50" | names: "VT-" | material: layers "Tre 50" ("Tre" 50.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, MMI, TESTTEST, TULLETE TEST
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Aluminium 65" | names: "VT-" | material: layers "Aluminium 65" ("Aluminium" 65.) | property sets: Pset_WallCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, TESTTEST, Pset_FireRatingProperties
          9 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Puss 125" | names: "VT-" | material: layers "Puss 125" ("Puss" 125.) | property sets: Pset_WallCommon, MMI, Pset_FireRatingProperties, TULLETE TEST, TESTTEST, tullball
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Stenderverk stål - Isolert 15" | CEILING | names: "fast gipshimling" | material: "Stenderverk stål - Isolert" | property sets: AC_Pset_Dimension, Pset_CoveringCommon, Pset_FireRatingProperties, MMI, TESTTEST, AC_Pset_RenovationAndPhasing
          57 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Solid Fill 3804854498 5" | names: "VT-" | material: layers "Solid Fill 3804854498 5" ("Solid Fill 3804854498" 5.) | property sets: MMI, Pset_WallCommon, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, Pset_FireRatingProperties, TULLETE TEST
          10 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Kryssfiner stående 2 25" | names: "VT-" | material: layers "Kryssfiner stående 2 25" ("Kryssfiner stående 2" 25.) | property sets: MMI, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, Pset_WallCommon, TESTTEST, tullball
          2 x IFCSLAB | type IFCSLABTYPE "Dekke 700" | BASESLAB | names: "Dekke-" | material: layers "Dekke 700" ("Dekke" 700.) | property sets: Pset_FireRatingProperties, Pset_CoveringCommon, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, MMI, Pset_SlabCommon
          2 x IFCBEAM | type IFCBEAMTYPE "Overgangsbeslag amfi mot bygg A 270 x 2" | object type "BEAM" | names: "B-" | material: "0% 27718788" | property sets: AC_Pset_RenovationAndPhasing, BaseQuantities, tullball, TULLETE TEST, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Innervegg 125" | names: "VT-" | material: layers "Innervegg 125" ("Innervegg" 125.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, tullball
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg HOVEDBYGG 320" | names: "VT-" | material: layers "Yttervegg HOVEDBYGG 320" ("Yttervegg HOVEDBYGG" 320.) | property sets: Pset_FireRatingProperties, Pset_WallCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, tullball
          2 x IFCCOVERING | type IFCCOVERINGTYPE "Stål 767" | CEILING | names: "Beslag rekkverk gangbro" | material: "Stål" | property sets: Pset_CoveringCommon, Pset_FireRatingProperties, AC_Pset_Dimension, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Bjelkelag148 mm tre, 9 mm GU, 50 mm murplate 207" | names: "YV08" | material: layers "Bjelkelag148 mm tre, 9 mm GU, 50 mm murplate" ("Isolasjon - Murplate" 50., "Gipsplate - Utvendig" 9., "Bjelkelag - Isolert" 148.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          2 x IFCGRID
      IFCBUILDINGSTOREY "Plan 2. Etasje" | long name "1. 2. Etasje" | elevation 30600.
        contains 761 elements
          35 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Innervegg 100" | names: "VT-" | material: layers "Innervegg 100" ("Innervegg" 100.) | property sets: Pset_FireRatingProperties, MMI, TESTTEST, Pset_WallCommon, TULLETE TEST, tullball
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "* PV 01- Påforing stålstender 100mm 3 lag gips 149" | names: "VT-" | material: layers "* PV 01- Påforing stålstender 100mm 3 lag gips" ("Gipsplate - Vegg" 13., "Gipsplate - Vegg" 13., "Gipsplate - Vegg" 13., "Stenderverk stål - Isolert" 100.) | property sets: MMI, Pset_WallCommon, Pset_FireRatingProperties, TESTTEST, TULLETE TEST, Skeisvang Pset: TEST 01 - ifcProject
          2 x IFCBEAM | type IFCBEAMTYPE "Stål 50 x 10" | object type "BEAM" | names: "B-" | material: "Stål" | property sets: Pset_BeamCommon, MMI, Pset_FireRatingProperties, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST
          8 x IFCBEAM | type IFCBEAMTYPE "HEA 340 330 x 300" | object type "BEAM" | names: "B-" | material: "Stål - S355" | property sets: Pset_BeamCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, TESTTEST
          6 x IFCSLAB | type IFCSLABTYPE "Ukjent 450" | BASESLAB | names: "Dekke-" | material: layers "Ukjent 450" ("Ukjent" 449.9999999999993) | property sets: Pset_CoveringCommon, Pset_SlabCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST
          3 x IFCSLAB | type IFCSLABTYPE "Stenderverk tre - Isolert 650" | BASESLAB | names: "Dekke-" | material: layers "Stenderverk tre - Isolert 650" ("Stenderverk tre - Isolert" 649.999999999995) | property sets: Pset_CoveringCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, Pset_SlabCommon
          2 x IFCSLAB | type IFCSLABTYPE "Glass - Herdet 40" | BASESLAB | names: "Dekke-" | material: layers "Glass - Herdet 40" ("Glass - Herdet" 39.99999999999915) | property sets: Pset_FireRatingProperties, Pset_SlabCommon, Pset_CoveringCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Isolasjon - Myk 200" | names: "VT-" | material: layers "Isolasjon - Myk 200" ("Isolasjon - Myk" 200.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, tullball, TULLETE TEST
          8 x IFCWALL | type IFCWALLTYPE "9520 - YV 02 - 200 mm trestender, , murplate, tegl 394" | names: "VT-" | parts: 32 IFCBUILDINGELEMENTPART | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, TESTTEST
          5 x IFCSLAB | type IFCSLABTYPE "Tak DETALJER 50" | BASESLAB | names: "Dekke-" | material: layers "Tak DETALJER 50" ("Tak DETALJER" 49.99999999999716) | property sets: Pset_SlabCommon, Pset_FireRatingProperties, MMI, Pset_CoveringCommon, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST
          12 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 1 150" | names: "VT-" | material: layers "Yttervegg 1 150" ("Yttervegg 1" 150.) | property sets: Pset_WallCommon, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, MMI, Pset_FireRatingProperties, tullball
          1 x IFCSLAB | type IFCSLABTYPE "Dekke 225" | BASESLAB | names: "Dekke-" | material: layers "Dekke 225" ("Dekke" 225.) | property sets: Pset_CoveringCommon, MMI, Pset_FireRatingProperties, TULLETE TEST, Skeisvang Pset: TEST 01 - ifcProject, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "IDA.200" | property sets: Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST, Pset_DoorCommon
          11 x IFCDOOR | type IFCDOORSTYLE "Dør med sidefelt på side 2" | object type "DOOR" | names: "IDA.200" | property sets: Pset_FireRatingProperties, Pset_DoorCommon, Skeisvang Pset: TEST 01 - ifcProject, MMI, TULLETE TEST, tullball
          9 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "IDA.200" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, MMI, TESTTEST, TULLETE TEST
          30 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 1 100" | names: "VT-" | material: layers "Yttervegg 1 100" ("Yttervegg 1" 100.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, TESTTEST, MMI, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST
          50 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Innervegg 150" | names: "VT-" | material: layers "Innervegg 150" ("Innervegg" 150.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, TESTTEST, MMI, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "YD-" | property sets: Pset_FireRatingProperties, Pset_DoorCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, tullball, TESTTEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "YD-" | property sets: Pset_FireRatingProperties, Pset_DoorCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, tullball
          1 x IFCSLAB | type IFCSLABTYPE "Dekke 420" | BASESLAB | names: "Dekke-" | material: layers "Dekke 420" ("Dekke" 420.) | property sets: Pset_CoveringCommon, MMI, Pset_FireRatingProperties, Pset_SlabCommon, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject
          4 x IFCBEAM | type IFCBEAMTYPE "Betong - Prefab 300 x 580" | object type "BEAM" | names: "B-", "B-D2-6", "B-D2-7" | material: "Betong - Prefab" | property sets: Pset_FireRatingProperties, MMI, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, tullball, Pset_BeamCommon
          2 x IFCBEAM | type IFCBEAMTYPE "Betong - Prefab 250 x 450" | object type "BEAM" | names: "B-" | material: "Betong - Prefab" | property sets: Pset_BeamCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, Pset_FireRatingProperties, TULLETE TEST
          2 x IFCSLAB | type IFCSLABTYPE "Dekke 50" | BASESLAB | names: "Dekke-" | material: layers "Dekke 50" ("Dekke" 50.) | property sets: Pset_CoveringCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, Pset_SlabCommon, TESTTEST
          3 x IFCSTAIR | names: "Trapp-" | parts: 23 IFCBUILDINGELEMENTPART | property sets: BaseQuantities, AC_Pset_RenovationAndPhasing, tullball, TULLETE TEST, TESTTEST, Pset_FireRatingProperties
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 1 200" | names: "VT-" | material: layers "Yttervegg 1 200" ("Yttervegg 1" 200.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          2 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "IDA.200" | property sets: MMI, Pset_FireRatingProperties, Pset_DoorCommon, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          5 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "IDA.200" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, tullball, TESTTEST, TULLETE TEST
          1 x IFCSLAB | type IFCSLABTYPE "Dekke 650" | BASESLAB | names: "Dekke-" | material: layers "Dekke 650" ("Dekke" 649.999999999998) | property sets: Pset_CoveringCommon, Pset_FireRatingProperties, Pset_SlabCommon, MMI, tullball, TULLETE TEST
          2 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "IDA.200" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST, MMI
          4 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "IDA.200", "YD-" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, MMI, TESTTEST, TULLETE TEST, BaseQuantities
          2 x IFCDOOR | type IFCDOORSTYLE "Skyvedør med pocketkarm" | object type "DOOR" | names: "IDA.200" | property sets: Pset_FireRatingProperties, MMI, Pset_DoorCommon, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST
          10 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg HOVEDBYGG 200" | names: "VT-" | material: layers "Yttervegg HOVEDBYGG 200" ("Yttervegg HOVEDBYGG" 200.) | property sets: Pset_FireRatingProperties, Pset_WallCommon, MMI, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST
          35 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 1 240" | names: "VT-" | material: layers "Yttervegg 1 240" ("Yttervegg 1" 240.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, TESTTEST, tullball, TULLETE TEST
          2 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "IDA.200" | property sets: Pset_FireRatingProperties, Pset_DoorCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, tullball, AC_Pset_RenovationAndPhasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 1 120" | names: "VT-" | material: layers "Yttervegg 1 120" ("Yttervegg 1" 120.) | property sets: MMI, Skeisvang Pset: TEST 01 - ifcProject, Pset_WallCommon, Pset_FireRatingProperties, TESTTEST, TULLETE TEST
          1 x IFCSLAB | type IFCSLABTYPE "Yttervegg tegl 900" | BASESLAB | names: "Dekke-" | material: layers "Yttervegg tegl 900" ("Yttervegg tegl" 899.9999999999986) | property sets: Pset_FireRatingProperties, Pset_SlabCommon, Pset_CoveringCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST
          2 x IFCDOOR | type IFCDOORSTYLE "Dør med sidefelt på side 1" | object type "DOOR" | names: "IDA.200" | property sets: Pset_DoorCommon, MMI, Pset_FireRatingProperties, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, AC_Pset_RenovationAndPhasing
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Isolasjon - Myk 100" | names: "VT-" | material: layers "Isolasjon - Myk 100" ("Isolasjon - Myk" 100.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, TULLETE TEST, Skeisvang Pset: TEST 01 - ifcProject, tullball
          1 x IFCSLAB | type IFCSLABTYPE "Gulvbelegg 700" | BASESLAB | names: "Dekke-" | material: layers "Gulvbelegg 700" ("Gulvbelegg" 700.0000000000006) | property sets: Pset_CoveringCommon, Pset_SlabCommon, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, TULLETE TEST
          8 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-" | property sets: Pset_FireRatingProperties, Pset_DoorCommon, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST, MMI
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Isolasjon - Myk 150" | names: "VT-" | material: layers "Isolasjon - Myk 150" ("Isolasjon - Myk" 150.) | property sets: Pset_FireRatingProperties, Pset_WallCommon, Skeisvang Pset: TEST 01 - ifcProject, MMI, TULLETE TEST, TESTTEST
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Aluminium 35" | names: "VT-" | material: layers "Aluminium 35" ("Aluminium" 35.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, TESTTEST, tullball, TULLETE TEST
          8 x IFCSLAB | type IFCSLABTYPE "Dekke 100" | BASESLAB | names: "Dekke-" | material: layers "Dekke 100" ("Dekke" 100.) | property sets: Pset_CoveringCommon, Pset_SlabCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, MMI, TESTTEST
          5 x IFCDOOR | type IFCDOORSTYLE "Dør med sidefelt på side 2" | object type "DOOR" | names: "IDA.200", "YD-" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, MMI, TULLETE TEST, AC_Pset_RenovationAndPhasing
          2 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "IDA.200", "YD-" | property sets: MMI, Pset_FireRatingProperties, TESTTEST, TULLETE TEST, Skeisvang Pset: TEST 01 - ifcProject, tullball
          1 x IFCDOOR | type IFCDOORSTYLE "Dør med sidefelt på side 1" | object type "DOOR" | names: "IDA.200" | property sets: Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, Pset_DoorCommon, TESTTEST, TULLETE TEST, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "Dør med 2 sidefelt og overlys" | object type "DOOR" | names: "IDA.200" | property sets: MMI, Pset_DoorCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          6 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-" | property sets: MMI, Skeisvang Pset: TEST 01 - ifcProject, Pset_DoorCommon, TESTTEST, TULLETE TEST, Pset_FireRatingProperties
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, MMI, Pset_FireRatingProperties, TULLETE TEST, TESTTEST, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, MMI, TESTTEST, TULLETE TEST
          1 x IFCSLAB | type IFCSLABTYPE "Tak 50" | BASESLAB | names: "Dekke-" | material: layers "Tak 50" ("Tak" 49.99999999999716) | property sets: Pset_CoveringCommon, Pset_SlabCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet" | object type "DOOR" | names: "D-" | property sets: Pset_FireRatingProperties, MMI, Pset_DoorCommon, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          65 x IFCSLAB | type IFCSLABTYPE "Dekke 200" | BASESLAB | names: "Dekke-" | material: layers "Dekke 200" ("Dekke" 200.) | property sets: Pset_CoveringCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, Pset_SlabCommon, TESTTEST
          8 x IFCROOF | names: "Tak-" | material: "Tak"; "Betong - Prefab"; "Isolasjon - Trykkfast" | property sets: Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, tullball, TESTTEST, AC_Pset_RenovationAndPhasing
          2 x IFCWALL | type IFCWALLTYPE "Yttervegg 1 150" | names: "VT-" | material: "Yttervegg 1" | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, TESTTEST
          6 x IFCSLAB | type IFCSLABTYPE "Isolasjon - Trykkfast 400" | BASESLAB | names: "Dekke-" | material: layers "Isolasjon - Trykkfast 400" ("Isolasjon - Trykkfast" 400.0000000000008) | property sets: Pset_CoveringCommon, Pset_FireRatingProperties, MMI, Pset_SlabCommon, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST
          1 x IFCSLAB | type IFCSLABTYPE "Isolasjon - Trykkfast 250" | BASESLAB | names: "Dekke-" | material: layers "Isolasjon - Trykkfast 250" ("Isolasjon - Trykkfast" 250.) | property sets: Pset_CoveringCommon, Pset_SlabCommon, Pset_FireRatingProperties, MMI, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject
          1 x IFCSLAB | type IFCSLABTYPE "Dekke 36" | BASESLAB | names: "Dekke-" | material: layers "Dekke 35.7834" ("Dekke" 35.78344897402064) | property sets: Pset_CoveringCommon, Pset_SlabCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST
          16 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg HOVEDBYGG 275" | names: "VT-" | material: layers "Yttervegg HOVEDBYGG 275" ("Yttervegg HOVEDBYGG" 275.) | property sets: Pset_FireRatingProperties, Pset_WallCommon, TESTTEST, TULLETE TEST, Skeisvang Pset: TEST 01 - ifcProject, MMI
          63 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu variabelt" | object type "WINDOW" | names: "YVA.200" | property sets: Pset_FireRatingProperties, Pset_WindowCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør tofløyet med overlys" | object type "DOOR" | names: "YDA.200" | property sets: MMI, Pset_DoorCommon, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, TULLETE TEST, tullball
          4 x IFCCOVERING | type IFCCOVERINGTYPE "Platekledning - Himling 30" | CEILING | names: "Trolltekt el. tilsv." | material: "Platekledning - Himling" | property sets: Pset_CoveringCommon, AC_Pset_Dimension, Pset_FireRatingProperties, TESTTEST, MMI, Skeisvang Pset: TEST 01 - ifcProject
          1 x IFCSLAB | type IFCSLABTYPE "Yttervegg HOVEDBYGG 400" | BASESLAB | names: "Dekke-" | material: layers "Yttervegg HOVEDBYGG 400" ("Yttervegg HOVEDBYGG" 400.0000000000022) | property sets: Pset_CoveringCommon, Pset_FireRatingProperties, Pset_SlabCommon, MMI, TESTTEST, TULLETE TEST
          1 x IFCSLAB | type IFCSLABTYPE "Stål 80" | BASESLAB | names: "Dekke-" | material: layers "Stål 80" ("Stål" 79.99999999999918) | property sets: Pset_CoveringCommon, Pset_SlabCommon, Pset_FireRatingProperties, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST
          3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Earth 4222173438" | names: "Terreng-01" | material: "Earth 4222173438" | property sets: Skeisvang Pset: TEST 01 - ifcProject, AC_Pset_RenovationAndPhasing
          2 x IFCCOLUMN | type IFCCOLUMNTYPE "SKEISVANGsoyleraula_2etg" | object type "COLUMN" | names: "Stol-" | material: "Earth 4222173438" | property sets: Pset_ColumnCommon, Pset_FireRatingProperties, MMI, TESTTEST, TULLETE TEST, Skeisvang Pset: TEST 01 - ifcProject
          2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "SKEISVANGsoyleraula_2etg" | names: "Stol-" | material: "Earth 4222173438" | property sets: AC_Pset_Dimension, MMI, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, tullball, TULLETE TEST
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Tre 50" | names: "VT-" | material: layers "Tre 50" ("Tre" 50.) | property sets: MMI, Pset_WallCommon, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, tullball, TULLETE TEST
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Glass 20" | names: "VT-" | material: layers "Glass 20" ("Glass" 20.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, TESTTEST
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Tre 100" | names: "VT-" | material: layers "Tre 100" ("Tre" 100.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          2 x IFCRAILING | type IFCRAILINGTYPE "Railing Type" | names: "Rekkverk-" | parts: 196 IFCBUILDINGELEMENTPART | property sets: AC_Pset_Dimension, TESTTEST, TULLETE TEST, MMI, Skeisvang Pset: TEST 01 - ifcProject, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "Isolasjon - Trykkfast 300" | BASESLAB | names: "Dekke-" | material: layers "Isolasjon - Trykkfast 300" ("Isolasjon - Trykkfast" 300.) | property sets: Pset_CoveringCommon, Pset_FireRatingProperties, Pset_SlabCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST
          1 x IFCSLAB | type IFCSLABTYPE "Isolasjon - Trykkfast 100" | BASESLAB | names: "Dekke-" | material: layers "Isolasjon - Trykkfast 100" ("Isolasjon - Trykkfast" 100.0000000000005) | property sets: Pset_CoveringCommon, Pset_SlabCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 1 10" | names: "VT-" | material: layers "Yttervegg 1 10" ("Yttervegg 1" 10.) | property sets: Pset_FireRatingProperties, MMI, Pset_WallCommon, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, tullball
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg HOVEDBYGG 300" | names: "VT-" | material: layers "Yttervegg HOVEDBYGG 300" ("Yttervegg HOVEDBYGG" 300.) | property sets: Pset_FireRatingProperties, Pset_WallCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, tullball
          2 x IFCSLAB | type IFCSLABTYPE "Dekke 580" | BASESLAB | names: "Dekke-" | material: layers "Dekke 580" ("Dekke" 579.9999229042072) | property sets: Pset_CoveringCommon, Pset_FireRatingProperties, Pset_SlabCommon, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          1 x IFCSLAB | type IFCSLABTYPE "Betong - Prefab 400" | BASESLAB | names: "Dekke-" | material: layers "Betong - Prefab 400" ("Betong - Prefab" 400.) | property sets: Pset_CoveringCommon, MMI, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, Pset_SlabCommon
          2 x IFCSLAB | type IFCSLABTYPE "Betong - Prefab 265" | BASESLAB | names: "Dekke-" | material: layers "Betong - Prefab 265" ("Betong - Prefab" 265.) | property sets: Pset_CoveringCommon, MMI, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, Pset_SlabCommon, tullball
          9 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg tegl 104" | names: "VT-" | material: layers "Yttervegg tegl 104" ("Yttervegg tegl" 104.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, TESTTEST, TULLETE TEST, Skeisvang Pset: TEST 01 - ifcProject
          4 x IFCWALL | type IFCWALLTYPE "* YV 03 - 200 mm trestender, , murplate utvendig, sjikt for solavskjerming, tegl 464" | names: "VT-" | parts: 16 IFCBUILDINGELEMENTPART | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, TESTTEST
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Innervegg 200" | names: "VT-" | material: layers "Innervegg 200" ("Innervegg" 200.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          1 x IFCSLAB | type IFCSLABTYPE "Stål - Strukturell 130" | BASESLAB | names: "Dekke-" | material: layers "Stål - Strukturell 130" ("Stål - Strukturell" 130.) | property sets: Pset_CoveringCommon, Pset_SlabCommon, MMI, Pset_FireRatingProperties, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Stål 40" | names: "VT-" | material: layers "Stål 40" ("Stål" 40.) | property sets: Pset_FireRatingProperties, MMI, Pset_WallCommon, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST
          102 x IFCSLAB | type IFCSLABTYPE "Stål 30" | BASESLAB | names: "Dekke-" | material: layers "Stål 30" ("Stål" 30.) | property sets: MMI, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, Pset_SlabCommon, Pset_CoveringCommon
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "*9520 - IV LYD4 - 60 dB : 3x13 mm gips, 1x100mm stålstender 149" | names: "VT-" | material: layers "*9520 - IV LYD4 - 60 dB : 3x13 mm gips, 1x100mm stålstender" ("Gipsplate - Vegg" 13., "Gipsplate - Vegg" 13., "Gipsplate - Vegg" 13., "Stenderverk stål - Isolert" 100.) | property sets: MMI, Pset_WallCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "9520 - YV 04 - 98 mm trestender, gips inv, GU utv 233" | names: "VT-" | material: layers "9520 - YV 04 - 98 mm trestender, gips inv, GU utv" ("Vindsperre" 0., "Gipsplate - Utvendig" 9., "Stenderverk tre - Isolert" 198., "Dampsperre" 0., "Gipsplate - Vegg" 13., "Gipsplate - Vegg" 13.) | property sets: MMI, Pset_WallCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, BaseQuantities, TESTTEST
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Kart - koordinatobjekt 1" | names: "Stol-" | property sets: AC_Pset_Dimension, MMI, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, TESTTEST, tullball
          3 x IFCWALL | type IFCWALLTYPE "* IV 05 - 60 dB : 3x13 mm gips, 2x100mm stålstender, 3x13mm gips 288" | names: "VT-" | parts: 24 IFCBUILDINGELEMENTPART | property sets: MMI, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST, BaseQuantities
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Isolasjon - Murplate 100" | names: "VT-" | material: layers "Isolasjon - Murplate 100" ("Isolasjon - Murplate" 100.) | property sets: Pset_WallCommon, tullball, TULLETE TEST, Pset_FireRatingProperties, MMI, TESTTEST
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Tre 125" | names: "VT-" | material: layers "Tre 125" ("Tre" 125.) | property sets: MMI, Pset_FireRatingProperties, Pset_WallCommon, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, tullball
          10 x IFCBEAM | type IFCBEAMTYPE "HE 180 A (1) 180 x 171" | object type "BEAM" | names: "B-" | material: "100% 3804985440" | property sets: Pset_BeamCommon, Skeisvang Pset: TEST 01 - ifcProject, MMI, TESTTEST, tullball, Pset_FireRatingProperties
          1 x IFCSLAB | type IFCSLABTYPE "Isolasjon - Murplate 540" | BASESLAB | names: "Dekke-" | material: layers "Isolasjon - Murplate 540" ("Isolasjon - Murplate" 540.0000000000041) | property sets: Pset_CoveringCommon, Pset_SlabCommon, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, TESTTEST, MMI
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YDC.200" | property sets: Pset_DoorCommon, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, TULLETE TEST, tullball, TESTTEST
          29 x IFCCOVERING | type IFCCOVERINGTYPE "Systemhimling - 60x60 20" | CEILING | names: "Systemhimling 600 x 600 E-kant" | material: "Systemhimling - 60x60" | property sets: Pset_CoveringCommon, Pset_FireRatingProperties, TESTTEST, MMI, AC_Pset_Dimension, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "Dekke 264" | BASESLAB | names: "Dekke-" | material: layers "Dekke 264.217" ("Dekke" 264.2165510259794) | property sets: Pset_CoveringCommon, Pset_SlabCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST
          20 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "*9520 - IV 02 - Stålstender 100mm, uisolert,1x platekl. en side 113" | names: "skjørt" | material: layers "*9520 - IV 02 - Stålstender 100mm, uisolert,1x platekl. en side" ("Gipsplate - Vegg" 13., "Stenderverk stål - Uisolert" 100.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, MMI, TESTTEST, TULLETE TEST
          2 x IFCBEAM | type IFCBEAMTYPE "UPE-300 100 x 300" | object type "BEAM" | names: "B-" | material: "Bindingsverk - Uisolert" | property sets: Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, Pset_BeamCommon, tullball, TULLETE TEST
          16 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Maling 10" | names: "VT-" | material: layers "Maling 10" ("Maling" 10.) | property sets: MMI, Pset_WallCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, tullball
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Puss 125" | names: "VT-" | material: layers "Puss 125" ("Puss" 125.) | property sets: Pset_WallCommon, MMI, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST
          9 x IFCCOVERING | type IFCCOVERINGTYPE "Stenderverk stål - Isolert 50" | CEILING | names: "fast gipshimling" | material: "Stenderverk stål - Isolert" | property sets: Pset_CoveringCommon, AC_Pset_Dimension, MMI, Pset_FireRatingProperties, TESTTEST, AC_Pset_RenovationAndPhasing
      IFCBUILDINGSTOREY "Loftplan / 3. Etasje" | elevation 33900.
        contains 168 elements
          16 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 1 150" | names: "VT-" | material: layers "Yttervegg 1 150" ("Yttervegg 1" 150.) | property sets: Pset_WallCommon, MMI, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, tullball
          53 x IFCWINDOW | type IFCWINDOWSTYLE "Vindu" | object type "WINDOW" | names: "V-" | property sets: Pset_WindowCommon, MMI, Pset_FireRatingProperties, TESTTEST, tullball, Skeisvang Pset: TEST 01 - ifcProject
          5 x IFCSLAB | type IFCSLABTYPE "Dekke 170" | BASESLAB | names: "Dekke-" | material: layers "Dekke 170" ("Dekke" 170.) | property sets: Pset_CoveringCommon, Pset_SlabCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST
          6 x IFCWALL | type IFCWALLTYPE "Yttervegg 1 150" | names: "VT-" | material: "Yttervegg 1" | property sets: Pset_WallCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, TESTTEST, TULLETE TEST
          2 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-" | property sets: Pset_DoorCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, MMI, TESTTEST, tullball
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg DETALJER 325" | names: "VT-" | material: layers "Yttervegg DETALJER 325" ("Yttervegg DETALJER" 325.) | property sets: Pset_WallCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, MMI, tullball, TESTTEST
          1 x IFCDOOR | type IFCDOORSTYLE "Dør" | object type "DOOR" | names: "YD-" | property sets: MMI, Pset_DoorCommon, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, Pset_FireRatingProperties, TULLETE TEST
          1 x IFCSTAIR | names: "Trapp-" | parts: 1 IFCBUILDINGELEMENTPART | property sets: Pset_StairCommon, Pset_FireRatingProperties, MMI, TULLETE TEST, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject
          3 x IFCSLAB | type IFCSLABTYPE "Dekke 200" | BASESLAB | names: "Dekke-" | material: layers "Dekke 200" ("Dekke" 200.) | property sets: Pset_SlabCommon, Skeisvang Pset: TEST 01 - ifcProject, Pset_CoveringCommon, Pset_FireRatingProperties, TESTTEST, TULLETE TEST
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg HOVEDBYGG 275" | names: "VT-" | material: layers "Yttervegg HOVEDBYGG 275" ("Yttervegg HOVEDBYGG" 275.) | property sets: MMI, Pset_FireRatingProperties, Pset_WallCommon, TULLETE TEST, tullball, TESTTEST
          10 x IFCROOF | names: "Tak-" | material: "Isolasjon - Trykkfast" | property sets: Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST, MMI, AC_Pset_RenovationAndPhasing
          4 x IFCWALL | type IFCWALLTYPE "Yttervegg DETALJER 100" | names: "VT-" | material: "Yttervegg DETALJER" | property sets: Pset_WallCommon, Pset_FireRatingProperties, MMI, TULLETE TEST, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg DETALJER 150" | names: "VT-" | material: layers "Yttervegg DETALJER 150" ("Yttervegg DETALJER" 150.) | property sets: Pset_WallCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, TESTTEST, TULLETE TEST
          1 x IFCSLAB | type IFCSLABTYPE "Stål 80" | BASESLAB | names: "Dekke-" | material: layers "Stål 80" ("Stål" 79.99999999999918) | property sets: BaseQuantities, tullball, AC_Pset_RenovationAndPhasing, TULLETE TEST, MMI, Pset_CoveringCommon
          6 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Earth 4222173438" | names: "Terreng-01" | material: "Earth 4222173438" | property sets: Skeisvang Pset: TEST 01 - ifcProject, AC_Pset_RenovationAndPhasing
          2 x IFCSLAB | type IFCSLABTYPE "Isolasjon - Trykkfast 400" | BASESLAB | names: "Dekke-" | material: layers "Isolasjon - Trykkfast 400" ("Isolasjon - Trykkfast" 400.0000000000008) | property sets: Pset_CoveringCommon, Pset_FireRatingProperties, Pset_SlabCommon, TULLETE TEST, TESTTEST, MMI
          1 x IFCBEAM | type IFCBEAMTYPE "Innervegg 150 x 1065" | object type "BEAM" | names: "B-" | material: "Innervegg" | property sets: Pset_BeamCommon, MMI, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, TESTTEST, TULLETE TEST
          24 x IFCSLAB | type IFCSLABTYPE "Dekke 1677" | BASESLAB | names: "Dekke-" | material: layers "Dekke 1676.6" ("Dekke" 1676.603703177662) | property sets: Pset_SlabCommon, Pset_CoveringCommon, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, Pset_FireRatingProperties, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "Dekke 1634" | BASESLAB | names: "Dekke-" | material: layers "Dekke 1633.89" ("Dekke" 1633.887056192975) | property sets: Pset_CoveringCommon, Pset_SlabCommon, Pset_FireRatingProperties, MMI, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST
          4 x IFCSLAB | type IFCSLABTYPE "Stål" | BASESLAB | names: "Dekke-" | material: "Stål" | property sets: Pset_CoveringCommon, Pset_FireRatingProperties, Pset_SlabCommon, Skeisvang Pset: TEST 01 - ifcProject, MMI, TESTTEST
          2 x IFCSLAB | type IFCSLABTYPE "Dekke 100" | BASESLAB | names: "Dekke-" | material: layers "Dekke 100" ("Dekke" 100.) | property sets: Pset_CoveringCommon, Pset_SlabCommon, Pset_FireRatingProperties, MMI, TESTTEST, Skeisvang Pset: TEST 01 - ifcProject
          3 x IFCWALL | type IFCWALLTYPE "Yttervegg DETALJER 150" | names: "VT-" | material: "Yttervegg DETALJER" | property sets: Pset_WallCommon, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, tullball, MMI
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Yttervegg 1 200" | names: "VT-" | material: layers "Yttervegg 1 200" ("Yttervegg 1" 200.) | property sets: Pset_WallCommon, MMI, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, AC_Pset_RenovationAndPhasing
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Kart - koordinatobjekt 1" | names: "Stol-" | property sets: AC_Pset_Dimension, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST, TULLETE TEST, MMI, tullball
          1 x IFCSLAB | type IFCSLABTYPE "Tak DETALJER 50" | BASESLAB | names: "Dekke-" | material: layers "Tak DETALJER 50" ("Tak DETALJER" 49.99999999999716) | property sets: Pset_CoveringCommon, Pset_SlabCommon, MMI, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TESTTEST
      IFCBUILDINGSTOREY "Takplan" | long name "Level 1" | elevation 37200.
        contains 5 elements
          1 x IFCSLAB | type IFCSLABTYPE "Yttervegg DETALJER 500" | BASESLAB | names: "Dekke-" | material: layers "Yttervegg DETALJER 500" ("Yttervegg DETALJER" 500.) | property sets: Pset_SlabCommon, MMI, Pset_CoveringCommon, Skeisvang Pset: TEST 01 - ifcProject, Pset_FireRatingProperties, TESTTEST
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Kart - koordinatobjekt 1" | names: "Stol-" | property sets: AC_Pset_Dimension, Skeisvang Pset: TEST 01 - ifcProject, MMI, TESTTEST, AC_Pset_RenovationAndPhasing, tullball
          3 x IFCCOLUMN | type IFCCOLUMNTYPE "Aluminium D100" | object type "COLUMN" | names: "S-" | material: "Aluminium" | property sets: Pset_ColumnCommon, MMI, Pset_FireRatingProperties, Skeisvang Pset: TEST 01 - ifcProject, TULLETE TEST, TESTTEST

Types
  IFCSLABTYPE "Yttervegg HOVEDBYGG 450" | BASESLAB | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Kart - koordinatobjekt 1" | 5 occurrences
  IFCSLABTYPE "Stein - Skiferheller 300" | BASESLAB | 1 occurrence
  IFCCURTAINWALLTYPE "Curtain Wall Type" | 4 occurrences
  IFCWALLTYPE "Yttervegg HOVEDBYGG 275" | 46 occurrences
  IFCWALLTYPE "Stål - Rustfritt 10" | 42 occurrences
  IFCWALLTYPE "Innervegg tegl 104" | 24 occurrences
  IFCCOVERINGTYPE "Systemhimling - 60x60 50" | CEILING | 69 occurrences | property sets: Pset_CoveringCommon
  IFCWALLTYPE "*9520 - IV 02 - Stålstender 100mm, uisolert, 2x + 1x platekl. to sider 139" | 1 occurrence
  IFCWALLTYPE "* PV03 Stålstender 100mm, påforingt, 2x platekl. en side 122" | 7 occurrences
  IFCWALLTYPE "*9520 - IV 02 - Trelekt 50mm, isolert, 1x platekl. en side 63" | 12 occurrences
  IFCWALLTYPE "Teglstein 104" | 3 occurrences
  IFCWALLTYPE "Yttervegg 1 150" | 287 occurrences
  IFCCOVERINGTYPE "Stenderverk stål - Isolert 50" | CEILING | 50 occurrences | property sets: Pset_CoveringCommon
  IFCWALLTYPE "*9520 - IV 05 - Plate 25 mm med 50 mm luft til eletrisk 75" | 74 occurrences
  IFCWALLTYPE "*9520 - IV 05 - Plate 25 mm med 30 luft 55" | 2 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Aluminium" | 13 occurrences
  IFCCOVERINGTYPE "Systemhimling - 60x120 50" | CEILING | 12 occurrences | property sets: Pset_CoveringCommon
  IFCWALLTYPE "Yttervegg 1 200" | 46 occurrences
  IFCBEAMTYPE "Stål 50 x 10" | BEAM | 36 occurrences
  IFCSLABTYPE "Stål 120" | BASESLAB | 13 occurrences
  IFCSLABTYPE "Stål 60" | BASESLAB | 26 occurrences
  IFCWALLTYPE "*9520 - IV 07 Lydvegg fasade 188" | 4 occurrences
  IFCWINDOWSTYLE "Vindu variabelt" | TRIPLE_PANEL_TOP | 1 occurrence
  IFCWALLTYPE "*9520 - IV 02 - Stålstender 50mm, isolert, 1x platekl. en side 73" | 3 occurrences
  IFCWALLTYPE "* IV 05 - 60 dB : 3x13 mm gips, 2x100mm stålstender, 3x13mm gips 288" | 17 occurrences
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCWALLTYPE "* IV 09 - RENHOLD - 1 plate gips+1 plate OSB-plate, Stålstender 100mm, isolert, 2x platekl. gips 152" | 6 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 26 occurrences
  IFCWALLTYPE "9520 - YV 05 - 148 mm trestender 150" | 6 occurrences
  IFCWALLTYPE "* IV 01 - Stålstender 100mm, isolert, 1x platekl. to sider 126" | 28 occurrences
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 3 occurrences
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCWALLTYPE "*9520 - IV 07 - Teglvegg m/luft 134" | 61 occurrences
  IFCWALLTYPE "*9520 - IV 02 - Stålstender 100mm, isolert, 1x platekl. en side 113" | 2 occurrences
  IFCCOVERINGTYPE "Teglstein 5" | CEILING | 39 occurrences | property sets: Pset_CoveringCommon
  IFCWALLTYPE "*9520 - IV 07 - Dobbel Teglvegg m/luft 230" | 6 occurrences
  IFCCOLUMNTYPE "Petal Kontur K7 600 600 x 14" | COLUMN | 33 occurrences
  IFCWALLTYPE "*9520 - IV 02B - Stålstender 50mm, isolert, 2x platekl. en side 86" | 2 occurrences
  IFCWALLTYPE "Maling 10" | 132 occurrences
  IFCCOLUMNTYPE "Petal Kontur K7 300 300 x 14" | COLUMN | 4 occurrences
  IFCCOVERINGTYPE "Gulvbelegg 3" | FLOORING | 39 occurrences | property sets: Pset_CoveringCommon
  IFCWALLTYPE "9520 - YV 03 - 200 mm trestender, , murplate, tegl 420" | 3 occurrences
  IFCWALLTYPE "* PV 02- Påforing stålstender 100mm 2 lag gips 136" | 15 occurrences
  IFCWALLTYPE "* IV 06 - dusj_Stålstender 100mm, isolert, 1x + 2x platekl. to sider (1) 135" | 6 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCWALLTYPE "* IV 07 - dusj_Stålstender 100mm, isolert, 2x platekl. to sider 148" | 2 occurrences
  IFCWALLTYPE "*9520 - IV 02 - dusj_Stålstender 50mm, påforingt, 2x platekl. en side 72" | 2 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 1 occurrence
  IFCBEAMTYPE "Kantbjelke 320-L 110 x 320" | BEAM | 2 occurrences
  IFCBEAMTYPE "Kantbjelke rekkverk 8 x 472" | BEAM | 2 occurrences
  IFCWALLTYPE "*9520 - IV 05 - Plate 25 mm med 10 luft 35" | 8 occurrences
  IFCWALLTYPE "* PV 01- Påforing stålstender 100mm 3 lag gips 149" | 37 occurrences
  IFCWALLTYPE "* IV 02 - Stålstender 100mm, isolert, 2x platekl. to sider 152" | 23 occurrences
  IFCDOORSTYLE "Dør tofløyet asymmetrisk" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCWALLTYPE "Stenderverk stål - Isolert 100" | 2 occurrences
  IFCWALLTYPE "*9520 - IV 03 - Stålstender 75mm, uisolert, 1x platekl. en side 88" | 2 occurrences
  IFCWINDOWSTYLE "Vindu" | SINGLE_PANEL | 12 occurrences
  IFCDOORSTYLE "Skyvedør" | USERDEFINED | 3 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 7 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCWALLTYPE "Yttervegg 1 250" | 18 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 3 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 2 occurrences
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 3 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 1 occurrence
  IFCWALLTYPE "Yttervegg 1 100" | 99 occurrences
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 4 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 4 occurrences
  IFCWALLTYPE "Yttervegg 1 170" | 2 occurrences
  IFCSLABTYPE "Yttervegg 1 200" | BASESLAB | 1 occurrence
  IFCWALLTYPE "Yttervegg 1 400" | 4 occurrences
  IFCWALLTYPE "Yttervegg 1 275" | 8 occurrences
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCWALLTYPE "Innervegg 200" | 9 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 3 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCWALLTYPE "Yttervegg HOVEDBYGG 200" | 18 occurrences
  IFCWALLTYPE "Yttervegg 1 120" | 10 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCWALLTYPE "Yttervegg 1 220" | 3 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 15 occurrences
  IFCWALLTYPE "Yttervegg 1 50" | 9 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 2 occurrences
  IFCSLABTYPE "Dekke 200" | BASESLAB | 216 occurrences
  IFCSLABTYPE "Dekke 600" | BASESLAB | 9 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 1 occurrence
  IFCWINDOWSTYLE "Vindu" | SINGLE_PANEL | 60 occurrences
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCSLABTYPE "Dekke 120" | BASESLAB | 2 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Tre" | 26 occurrences
  IFCSLABTYPE "Yttervegg 1 1250" | BASESLAB | 1 occurrence
  IFCWALLTYPE "Bodvegger 150 x 3250" | 9 occurrences
  IFCSLABTYPE "Stein - Skiferheller 200" | BASESLAB | 1 occurrence
  IFCWALLTYPE "Yttervegg DETALJER 550" | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 2 occurrences
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 2 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 4 occurrences
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCDOORSTYLE "Dør tofløyet med overlys" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCDOORSTYLE "Leddport" | ROLLINGUP | 2 occurrences
  IFCDOORSTYLE "Dør tofløyet med overlys" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 3 occurrences
  IFCSLABTYPE "Dekke 50" | BASESLAB | 6 occurrences
  IFCWALLTYPE "Yttervegg HOVEDBYGG 320" | 2 occurrences
  IFCWINDOWSTYLE "Vindu variabelt" | DOUBLE_PANEL_HORIZONTAL | 185 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Sink" | 8 occurrences
  IFCWALLTYPE "Maling 3" | 27 occurrences
  IFCDOORSTYLE "Dør tofløyet med overlys" | DOUBLE_DOOR_SINGLE_SWING | 2 occurrences
  IFCWALLTYPE "Yttervegg 1 350" | 14 occurrences
  IFCDOORSTYLE "Dør tofløyet med overlys" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCWALLTYPE "Yttervegg 1 550" | 1 occurrence
  IFCSLABTYPE "Dekke 400" | BASESLAB | 1 occurrence
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 2 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 2 occurrences
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Curtain Wall Type" | 9 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Isolasjon - Trykkfast" | 2 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 3 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 2 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 6 occurrences
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 2 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCCOLUMNTYPE "Stål 100 x 100" | COLUMN | 1 occurrence
  IFCWALLTYPE "* YV 03 - 200 mm trestender, , murplate utvendig, sjikt for solavskjerming, tegl 464" | 13 occurrences
  IFCWINDOWSTYLE "Vindu vertikal multi-rams" | DOUBLE_PANEL_HORIZONTAL | 4 occurrences
  IFCWINDOWSTYLE "Vindu variabelt" | TRIPLE_PANEL_TOP | 3 occurrences
  IFCWALLTYPE "9520 - YV 02 - 200 mm trestender, , murplate, tegl 394" | 18 occurrences
  IFCWINDOWSTYLE "Vindu variabelt" | TRIPLE_PANEL_TOP | 1 occurrence
  IFCWALLTYPE "Yttervegg tegl 104" | 19 occurrences
  IFCWALLTYPE "Isolasjon - Trykkfast 200" | 5 occurrences
  IFCWALLTYPE "Bjelkelag148 mm tre, 9 mm GU 157" | 3 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 2 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 1 occurrence
  IFCWALLTYPE "*9520 - IV LYD4 - 60 dB : 3x13 mm gips, 1x100mm stålstender 149" | 17 occurrences
  IFCWALLTYPE "*9520 - IV LYD3 - 55 dB: 2x13 mm gips, 2x100mm stålstender, 2x13mm gips 262" | 1 occurrence
  IFCDOORSTYLE "Dør med sidefelt på side 2" | SINGLE_SWING_LEFT | 8 occurrences
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCWALLTYPE "9520 - IV 00 - Stålstender 100mm, isolert, 2x platekl. en side 136" | 3 occurrences
  IFCDOORSTYLE "Dør tofløyet med 2 sidefelt" | USERDEFINED | 3 occurrences
  IFCDOORSTYLE "Dør tofløyet asymmetrisk" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 2 occurrences
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCWALLTYPE "* IV 04 - Stålstender 100mm, isolert, 1x + 2x platekl. to sider 139" | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCWALLTYPE "* IV 08- 55 dB: 2x13 mm gips, 2x100mm stålstender, 2x13mm gips 262" | 8 occurrences
  IFCWALLTYPE "* PV04 Stålstender 100mm isolert, påforingt, 2x platekl. en side 122" | 2 occurrences
  IFCDOORSTYLE "Dør tofløyet med overlys" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCCOVERINGTYPE "9520 - HH 00 - Fast himling gips_Sylomar Akustikk Super T60 KOPI 125" | CEILING | 21 occurrences | property sets: Pset_CoveringCommon
  IFCSLABTYPE "9520 - HH 00 - Fast himling gips_Sylomar Akustikk Super T60 KOPI 125" | BASESLAB | 2 occurrences
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCDOORSTYLE "Dør med sidefelt på side 2" | SINGLE_SWING_RIGHT | 10 occurrences
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 1 occurrence
  IFCSLABTYPE "Dekke 5000" | BASESLAB | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Tekst 3D" | 3 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Flis - Gulv 15" | 2 occurrences
  IFCCOVERINGTYPE "Systemhimling - 60x60 20" | CEILING | 56 occurrences | property sets: Pset_CoveringCommon
  IFCDOORSTYLE "Dør med sidefelt på side 2" | SINGLE_SWING_RIGHT | 25 occurrences
  IFCWALLTYPE "9520 - IV 00 - Stålstender 100mm, uisolert 110" | 3 occurrences
  IFCSLABTYPE "Tre 50" | BASESLAB | 10 occurrences
  IFCCOVERINGTYPE "Påstøp 3" | FLOORING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCWALLTYPE "Innervegg 45" | 4 occurrences
  IFCWALLTYPE "Tre 45" | 4 occurrences
  IFCWALLTYPE "Bjelkelag148 mm tre, 9 mm GU , uisolert 148" | 1 occurrence
  IFCWALLTYPE "Yttervegg HOVEDBYGG 125" | 2 occurrences
  IFCWALLTYPE "Isolasjon - Trykkfast 125" | 2 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Lem rektangulær" | 4 occurrences
  IFCWALLTYPE "Innervegg 150" | 53 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 1 occurrence
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 2 occurrences
  IFCCOVERINGTYPE "Stål 50" | CEILING | 6 occurrences | property sets: Pset_CoveringCommon
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCWALLTYPE "Innervegg tegl 230" | 3 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 1 occurrence
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 6 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 1 occurrence
  IFCCOVERINGTYPE "Gulvplanker 35" | FLOORING | 13 occurrences | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Gulvplanker 30" | FLOORING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Gulvplanker 362" | FLOORING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Gulvplanker 367" | FLOORING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Gulvplanker 367" | FLOORING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Gulvplanker 367" | FLOORING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Tre 150" | FLOORING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Tre 212" | FLOORING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Tre 150" | FLOORING | 11 occurrences | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Tre 578" | FLOORING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Tre 945" | FLOORING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Tre 1312" | FLOORING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCWALLTYPE "Tre 150" | 1 occurrence
  IFCCOLUMNTYPE "Overgangsbeslag amfi mot bygg A 270 x 2" | COLUMN | 2 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Tre - Heltre" | 3 occurrences
  IFCWALLTYPE "Bjelkelag 198, isolert 216" | 1 occurrence
  IFCWALLTYPE "Tre 25" | 219 occurrences
  IFCWALLTYPE "Tre 5" | 52 occurrences
  IFCWALLTYPE "Isolasjon - Myk 138" | 6 occurrences
  IFCWALLTYPE "Isolasjon - Myk 51" | 2 occurrences
  IFCWALLTYPE "Isolasjon - Myk 225" | 94 occurrences
  IFCBEAMTYPE "Overgangsbeslag amfi mot bygg A 270 x 2" | BEAM | 4 occurrences
  IFCWALLTYPE "Puss 125" | 18 occurrences
  IFCWINDOWSTYLE "Vindu vertikal multi-rams" | DOUBLE_PANEL_HORIZONTAL | 1 occurrence
  IFCSLABTYPE "Dekke 2557" | BASESLAB | 2 occurrences
  IFCCOLUMNTYPE "HUP 100x100x10 100 x 100" | COLUMN | 10 occurrences
  IFCWALLTYPE "*9520 - IV 02 - Stålstender 100mm, uisolert,1x platekl. en side 113" | 74 occurrences
  IFCCOVERINGTYPE "Platekledning - Himling 15" | CEILING | 6 occurrences | property sets: Pset_CoveringCommon
  IFCCOLUMNTYPE "Aluminium 50 x 10" | COLUMN | 92 occurrences
  IFCCOVERINGTYPE "Stål 321" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Stål 329" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Platekledning - Himling 20" | CEILING | 8 occurrences | property sets: Pset_CoveringCommon
  IFCWALLTYPE "*9520 - IV 03 - FORING NISJER Stålstender 75mm, uisolert, 1x platekl. en side 100" | 26 occurrences
  IFCDOORSTYLE "Dør tofløyet asymmetrisk" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCWALLTYPE "*9520 - 3x13 mm gips 39" | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 4 occurrences
  IFCWALLTYPE "Isolasjon - Myk 150" | 4 occurrences
  IFCDOORSTYLE "Dør tofløyet asymmetrisk" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCWINDOWSTYLE "Vindu vertikal multi-rams" | SINGLE_PANEL | 4 occurrences
  IFCSLABTYPE "Stenderverk stål - Isolert 50" | BASESLAB | 1 occurrence
  IFCRAILINGTYPE "Railing Type" | 5 occurrences
  IFCSLABTYPE "Dekke 472" | BASESLAB | 1 occurrence
  IFCWALLTYPE "9520 - YV 05 - 148 mm trestender (1) 150" | 3 occurrences
  IFCWALLTYPE "9520 - YV 06 - 198 mm trestender 200" | 4 occurrences
  IFCWALLTYPE "Betong - Strukturell 200" | 2 occurrences
  IFCWINDOWSTYLE "Vindu vertikal multi-rams" | SINGLE_PANEL | 2 occurrences
  IFCWINDOWSTYLE "Vindu tre-fags" | TRIPLE_PANEL_VERTICAL | 1 occurrence
  IFCSLABTYPE "Dekke 65" | BASESLAB | 1 occurrence
  IFCWINDOWSTYLE "Vindu variabelt" | DOUBLE_PANEL_VERTICAL | 1 occurrence
  IFCSLABTYPE ""9520 - GULV 01 - Betong Påstøp 120 mm, 50 mm trykkfast isolasjon 170" | BASESLAB | 2 occurrences
  IFCWALLTYPE "Kryssfiner 25" | 34 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Kryssfiner" | 5 occurrences
  IFCCOVERINGTYPE "9520 - HH 00 - Fast himling gips_Sylomar Akustikk Super T60 KOPI 125" | CEILING | 2 occurrences | property sets: Pset_CoveringCommon
  IFCSLABTYPE "Systemhimling - 60x60 50" | BASESLAB | 2 occurrences
  IFCWALLTYPE "Yttervegg HOVEDBYGG 350" | 5 occurrences
  IFCWINDOWSTYLE "Vindu vertikal multi-rams" | DOUBLE_PANEL_HORIZONTAL | 2 occurrences
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 2 occurrences
  IFCWALLTYPE "Yttervegg 1 300" | 6 occurrences
  IFCSLABTYPE "Dekke 220" | BASESLAB | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 2 occurrences
  IFCDOORSTYLE "Dør med overlys" | SINGLE_SWING_LEFT | 1 occurrence
  IFCDOORSTYLE "Dør med sidefelt på side 2" | SINGLE_SWING_LEFT | 37 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 3 occurrences
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 2 occurrences
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCDOORSTYLE "Dør tofløyet med overlys" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCDOORSTYLE "Dør med sidefelt på side 2 og overlys" | SINGLE_SWING_LEFT | 4 occurrences
  IFCWALLTYPE "Maling 5" | 2 occurrences
  IFCWALLTYPE "Yttervegg 1 240" | 48 occurrences
  IFCCOLUMNTYPE "Limtre 250 x 250" | COLUMN | 1 occurrence
  IFCCOLUMNTYPE "Gips 250 x 250" | COLUMN | 1 occurrence
  IFCCOLUMNTYPE "Betong - Prefab 250 x 300" | COLUMN | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 3 occurrences
  IFCSLABTYPE "Dekke 1000" | BASESLAB | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 12 occurrences
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 4 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 3 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 3 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 6 occurrences
  IFCDOORSTYLE "Dør med overlys" | SINGLE_SWING_LEFT | 2 occurrences
  IFCDOORSTYLE "Dør med overlys" | SINGLE_SWING_LEFT | 1 occurrence
  IFCSLABTYPE "Dekke 300" | BASESLAB | 2 occurrences
  IFCDOORSTYLE "Dør med overlys" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCWALLTYPE "Yttervegg 1 75" | 2 occurrences
  IFCDOORSTYLE "Dør med sidefelt på side 2 og overlys" | SINGLE_SWING_RIGHT | 5 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 3 occurrences
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCWINDOWSTYLE "Vindu" | SINGLE_PANEL | 1 occurrence
  IFCDOORSTYLE "Dør med sidefelt på side 1" | SINGLE_SWING_RIGHT | 3 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 9 occurrences
  IFCSLABTYPE "Dekke 100" | BASESLAB | 22 occurrences
  IFCBEAMTYPE "Betong - Prefab 500 x 450" | BEAM | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 2 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 2 occurrences
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCSLABTYPE "Dekke 270" | BASESLAB | 1 occurrence
  IFCDOORSTYLE "Dør tofløyet med overlys" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCSLABTYPE "Teglstein 50" | BASESLAB | 260 occurrences
  IFCDOORSTYLE "Dør tofløyet med overlys" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCWALLTYPE "Yttervegg HOVEDBYGG 318" | 1 occurrence
  IFCCOVERINGTYPE "Stål 320" | CEILING | 4 occurrences | property sets: Pset_CoveringCommon
  IFCDOORSTYLE "Skyvedør med sidefelt på side 1 og overlys" | USERDEFINED | 1 occurrence
  IFCDOORSTYLE "Skyvedør med overlys" | USERDEFINED | 1 occurrence
  IFCCOLUMNTYPE "Stål - Overflatebehandlet D70" | COLUMN | 1 occurrence
  IFCDOORSTYLE "Skyvedør med pocketkarm" | USERDEFINED | 4 occurrences
  IFCCOLUMNTYPE "Stål - Overflatebehandlet D30" | COLUMN | 2 occurrences
  IFCWALLTYPE "Yttervegg 1 30" | 2 occurrences
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCWALLTYPE "Yttervegg 1 160" | 1 occurrence
  IFCDOORSTYLE "Skyvedør med 2 sidefelt og overlys" | USERDEFINED | 1 occurrence
  IFCSLABTYPE "Dekke 450" | BASESLAB | 2 occurrences
  IFCWALLTYPE "Stål 40" | 4 occurrences
  IFCSLABTYPE "Stål 30" | BASESLAB | 129 occurrences
  IFCSLABTYPE "Aluminium 3800" | BASESLAB | 1 occurrence
  IFCSLABTYPE "Dekke 5980" | BASESLAB | 10 occurrences
  IFCWALLTYPE "Yttervegg 1 10" | 6 occurrences
  IFCSLABTYPE "Dekke 165" | BASESLAB | 1 occurrence
  IFCSLABTYPE "Dekke 470" | BASESLAB | 1 occurrence
  IFCSLABTYPE "Dekke 385" | BASESLAB | 2 occurrences
  IFCDOORSTYLE "Dør tofløyet med overlys" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCSLABTYPE "Stein - Skiferheller 150" | BASESLAB | 1 occurrence
  IFCCOLUMNTYPE "Stål D300" | COLUMN | 3 occurrences
  IFCWINDOWSTYLE "Vindu variabelt" | DOUBLE_PANEL_VERTICAL | 1 occurrence
  IFCWINDOWSTYLE "Vindu variabelt" | DOUBLE_PANEL_VERTICAL | 7 occurrences
  IFCWINDOWSTYLE "Vindu variabelt" | DOUBLE_PANEL_VERTICAL | 1 occurrence
  IFCWINDOWSTYLE "Vindu variabelt" | DOUBLE_PANEL_VERTICAL | 1 occurrence
  IFCWINDOWSTYLE "Vindu variabelt" | DOUBLE_PANEL_VERTICAL | 1 occurrence
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 2 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 1 occurrence
  IFCWALLTYPE "*9520 - IV LYD1 - 35/37 dB: 1x13 mm gips, 1x100mm stålstender, 1x13mm gips 126" | 1 occurrence
  IFCSLABTYPE "Isolasjon - Trykkfast 200" | BASESLAB | 1 occurrence
  IFCWALLTYPE "* IV 03- 48/50 dB: 3x13 mm gips, 1X100mm stålstender, 3x13mm gips 178" | 2 occurrences
  IFCWALLTYPE "*9520 - IV LYD6 - 70 dB: 3x13mm gips, 100mm stålstender, 250mmleca lydblokk, 100mm stålstender, 3x13mm gips 548" | 1 occurrence
  IFCWALLTYPE "Innervegg 100" | 36 occurrences
  IFCSLABTYPE "Gulvplanker 183" | BASESLAB | 24 occurrences
  IFCDOORSTYLE "Dør tofløyet asymmetrisk" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCDOORSTYLE "Dør tofløyet asymmetrisk" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCSLABTYPE "Platekledning - Vegg 50" | BASESLAB | 1 occurrence
  IFCWALLTYPE "Tre 15" | 2 occurrences
  IFCWINDOWSTYLE "Vindu tre-fags" | TRIPLE_PANEL_VERTICAL | 1 occurrence
  IFCCOVERINGTYPE "Gulvbelegg 5" | FLOORING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Gulvplanker 20" | FLOORING | 2 occurrences | property sets: Pset_CoveringCommon
  IFCSLABTYPE "Tre 460" | BASESLAB | 4 occurrences
  IFCWALLTYPE "Tre 225" | 10 occurrences
  IFCSLABTYPE "Aluminium 3110" | BASESLAB | 1 occurrence
  IFCWALLTYPE "Panel innvendig - Liggende m/gliper 25" | 1 occurrence
  IFCCOLUMNTYPE "Aluminium D60" | COLUMN | 3 occurrences
  IFCSLABTYPE "Tre 150" | BASESLAB | 5 occurrences
  IFCSLABTYPE "Tre 300" | BASESLAB | 5 occurrences
  IFCSLABTYPE "Tre 450" | BASESLAB | 4 occurrences
  IFCSLABTYPE "Tre 307" | BASESLAB | 5 occurrences
  IFCSLABTYPE "Tre 153" | BASESLAB | 5 occurrences
  IFCCOVERINGTYPE "Påstøp 17" | FLOORING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCSLABTYPE "Tre 200" | BASESLAB | 1 occurrence
  IFCDOORSTYLE "Dør tofløyet asymmetrisk" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCWALLTYPE "Panel innvendig - Liggende 25" | 1 occurrence
  IFCCOVERINGTYPE "Gulvplanker 367" | FLOORING | 6 occurrences | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Gulvplanker 366" | FLOORING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Gulvplanker 367" | FLOORING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Gulvplanker 367" | FLOORING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Gulvplanker 367" | FLOORING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Gulvplanker 733" | FLOORING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Tre 135" | FLOORING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Tre 2045" | FLOORING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Tre 2412" | FLOORING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Tre 636" | FLOORING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Tre 627" | FLOORING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Tre 532" | FLOORING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Tre 1678" | FLOORING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Tre 1280" | FLOORING | 3 occurrences | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Tre 1280" | FLOORING | 2 occurrences | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Tre 898" | FLOORING | 2 occurrences | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Platekledning - Himling 30" | CEILING | 19 occurrences | property sets: Pset_CoveringCommon
  IFCSLABTYPE "Tre 410" | BASESLAB | 1 occurrence
  IFCWALLTYPE "Bordkledning - Stående 12" | 2 occurrences
  IFCWALLTYPE "*9520 - MDD - Bassabsorbent vegg 262" | 3 occurrences
  IFCCOVERINGTYPE "Dekke 20" | CEILING | 3 occurrences | property sets: Pset_CoveringCommon
  IFCWALLTYPE "Tre 50" | 6 occurrences
  IFCWALLTYPE "Aluminium 65" | 4 occurrences
  IFCCOVERINGTYPE "Stenderverk stål - Isolert 15" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCWALLTYPE "Solid Fill 3804854498 5" | 57 occurrences
  IFCWALLTYPE "Kryssfiner stående 2 25" | 10 occurrences
  IFCSLABTYPE "Dekke 700" | BASESLAB | 2 occurrences
  IFCWALLTYPE "Innervegg 125" | 3 occurrences
  IFCCOVERINGTYPE "Stål 767" | CEILING | 2 occurrences | property sets: Pset_CoveringCommon
  IFCWALLTYPE "Bjelkelag148 mm tre, 9 mm GU, 50 mm murplate 207" | 3 occurrences
  IFCBEAMTYPE "HEA 340 330 x 300" | BEAM | 8 occurrences
  IFCSLABTYPE "Ukjent 450" | BASESLAB | 6 occurrences
  IFCSLABTYPE "Stenderverk tre - Isolert 650" | BASESLAB | 3 occurrences
  IFCSLABTYPE "Glass - Herdet 40" | BASESLAB | 2 occurrences
  IFCWALLTYPE "Isolasjon - Myk 200" | 2 occurrences
  IFCSLABTYPE "Tak DETALJER 50" | BASESLAB | 6 occurrences
  IFCSLABTYPE "Dekke 225" | BASESLAB | 1 occurrence
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCDOORSTYLE "Dør tofløyet" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCSLABTYPE "Dekke 420" | BASESLAB | 1 occurrence
  IFCBEAMTYPE "Betong - Prefab 300 x 580" | BEAM | 4 occurrences
  IFCBEAMTYPE "Betong - Prefab 250 x 450" | BEAM | 2 occurrences
  IFCSLABTYPE "Dekke 650" | BASESLAB | 1 occurrence
  IFCSLABTYPE "Yttervegg tegl 900" | BASESLAB | 1 occurrence
  IFCWALLTYPE "Isolasjon - Myk 100" | 4 occurrences
  IFCSLABTYPE "Gulvbelegg 700" | BASESLAB | 1 occurrence
  IFCWALLTYPE "Aluminium 35" | 2 occurrences
  IFCDOORSTYLE "Dør med sidefelt på side 1" | SINGLE_SWING_LEFT | 1 occurrence
  IFCDOORSTYLE "Dør med 2 sidefelt og overlys" | USERDEFINED | 1 occurrence
  IFCSLABTYPE "Tak 50" | BASESLAB | 1 occurrence
  IFCSLABTYPE "Isolasjon - Trykkfast 400" | BASESLAB | 8 occurrences
  IFCSLABTYPE "Isolasjon - Trykkfast 250" | BASESLAB | 1 occurrence
  IFCSLABTYPE "Dekke 36" | BASESLAB | 1 occurrence
  IFCDOORSTYLE "Dør tofløyet med overlys" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCSLABTYPE "Yttervegg HOVEDBYGG 400" | BASESLAB | 1 occurrence
  IFCSLABTYPE "Stål 80" | BASESLAB | 2 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Earth 4222173438" | 9 occurrences
  IFCCOLUMNTYPE "SKEISVANGsoyleraula_2etg" | COLUMN | 2 occurrences
  IFCFURNITURETYPE "SKEISVANGsoyleraula_2etg" | 2 occurrences
  IFCWALLTYPE "Glass 20" | 5 occurrences
  IFCWALLTYPE "Tre 100" | 5 occurrences
  IFCSLABTYPE "Isolasjon - Trykkfast 300" | BASESLAB | 1 occurrence
  IFCSLABTYPE "Isolasjon - Trykkfast 100" | BASESLAB | 1 occurrence
  IFCWALLTYPE "Yttervegg HOVEDBYGG 300" | 4 occurrences
  IFCSLABTYPE "Dekke 580" | BASESLAB | 2 occurrences
  IFCSLABTYPE "Betong - Prefab 400" | BASESLAB | 1 occurrence
  IFCSLABTYPE "Betong - Prefab 265" | BASESLAB | 2 occurrences
  IFCSLABTYPE "Stål - Strukturell 130" | BASESLAB | 1 occurrence
  IFCWALLTYPE "9520 - YV 04 - 98 mm trestender, gips inv, GU utv 233" | 2 occurrences
  IFCWALLTYPE "Isolasjon - Murplate 100" | 2 occurrences
  IFCWALLTYPE "Tre 125" | 6 occurrences
  IFCBEAMTYPE "HE 180 A (1) 180 x 171" | BEAM | 10 occurrences
  IFCSLABTYPE "Isolasjon - Murplate 540" | BASESLAB | 1 occurrence
  IFCSLABTYPE "Dekke 264" | BASESLAB | 1 occurrence
  IFCBEAMTYPE "UPE-300 100 x 300" | BEAM | 2 occurrences
  IFCSLABTYPE "Dekke 170" | BASESLAB | 5 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_RIGHT | 2 occurrences
  IFCWALLTYPE "Yttervegg DETALJER 325" | 4 occurrences
  IFCDOORSTYLE "Dør" | SINGLE_SWING_LEFT | 1 occurrence
  IFCWALLTYPE "Yttervegg DETALJER 100" | 4 occurrences
  IFCWALLTYPE "Yttervegg DETALJER 150" | 9 occurrences
  IFCBEAMTYPE "Innervegg 150 x 1065" | BEAM | 1 occurrence
  IFCSLABTYPE "Dekke 1677" | BASESLAB | 24 occurrences
  IFCSLABTYPE "Dekke 1634" | BASESLAB | 1 occurrence
  IFCSLABTYPE "Stål" | BASESLAB | 4 occurrences
  IFCSLABTYPE "Yttervegg DETALJER 500" | BASESLAB | 1 occurrence
  IFCCOLUMNTYPE "Aluminium D100" | COLUMN | 3 occurrences

Property sets
  TESTTEST | properties | on 3199 objects (874 IFCSLAB, 656 IFCBUILDINGELEMENTPART, 488 IFCMEMBER, 403 IFCCOVERING)
    testtesttetstetstst = "100" (IFCLABEL)
  TESTTEST | properties | on 2876 objects (1914 IFCWALLSTANDARDCASE, 465 IFCBUILDINGELEMENTPART, 287 IFCDOOR, 107 IFCWALL)
    testtesttetstetstst = "300" (IFCLABEL)
  TESTTEST | properties | on 5 objects (4 IFCBUILDINGELEMENTPART, 1 IFCWALL)
    testtesttetstetstst = "250" (IFCLABEL)
  TESTTEST | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    testtesttetstetstst = "" (IFCLABEL)
  tullball | properties | on 2876 objects (1914 IFCWALLSTANDARDCASE, 465 IFCBUILDINGELEMENTPART, 287 IFCDOOR, 107 IFCWALL)
    fredag = "300" (IFCLABEL)
  tullball | properties | on 2796 objects (874 IFCSLAB, 656 IFCBUILDINGELEMENTPART, 488 IFCMEMBER, 187 IFCWINDOW)
    fredag = "100" (IFCLABEL)
  tullball | properties | on 5 objects (4 IFCBUILDINGELEMENTPART, 1 IFCWALL)
    fredag = "250" (IFCLABEL)
  tullball | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    fredag = "" (IFCLABEL)
  TULLETE TEST | properties | on 2876 objects (1914 IFCWALLSTANDARDCASE, 465 IFCBUILDINGELEMENTPART, 287 IFCDOOR, 107 IFCWALL)
    tull og ball = "300" (IFCLABEL)
  TULLETE TEST | properties | on 2796 objects (874 IFCSLAB, 656 IFCBUILDINGELEMENTPART, 488 IFCMEMBER, 187 IFCWINDOW)
    tull og ball = "100" (IFCLABEL)
  TULLETE TEST | properties | on 5 objects (4 IFCBUILDINGELEMENTPART, 1 IFCWALL)
    tull og ball = "250" (IFCLABEL)
  TULLETE TEST | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    tull og ball = "" (IFCLABEL)
  Skeisvang Pset: TEST 01 - ifcProject | properties | on 1320 objects (1285 IFCWALLSTANDARDCASE, 35 IFCWALL)
    Test AA = "VT-" (IFCLABEL)
    Test BB = "300" (IFCLABEL)
    Test CC = "New" (IFCLABEL)
  Skeisvang Pset: TEST 01 - ifcProject | properties | on 756 objects (753 IFCSLAB, 3 IFCCOVERING)
    Test AA = "Dekke-" (IFCLABEL)
    Test BB = "100" (IFCLABEL)
    Test CC = "New" (IFCLABEL)
  Skeisvang Pset: TEST 01 - ifcProject | properties | on 656 objects (656 IFCBUILDINGELEMENTPART)
    Test BB = "100" (IFCLABEL)
  Skeisvang Pset: TEST 01 - ifcProject | properties | on 465 objects (465 IFCBUILDINGELEMENTPART)
    Test BB = "300" (IFCLABEL)
  Skeisvang Pset: TEST 01 - ifcProject | properties | on 413 objects (367 IFCWALLSTANDARDCASE, 46 IFCWALL)
    Test AA = "VT-" (IFCLABEL)
    Test BB = "300" (IFCLABEL)
    Test CC = "Existing" (IFCLABEL)
  Skeisvang Pset: TEST 01 - ifcProject | properties | on 119 objects (119 IFCCOLUMN)
    Test AA = "S-" (IFCLABEL)
    Test BB = "100" (IFCLABEL)
    Test CC = "New" (IFCLABEL)
  Skeisvang Pset: TEST 01 - ifcProject | properties | on 109 objects (108 IFCCOVERING, 1 IFCSLAB)
    Test AA = "Systemhimling 600 x 600 E-kant" (IFCLABEL)
    Test BB = "100" (IFCLABEL)
    Test CC = "New" (IFCLABEL)
  Skeisvang Pset: TEST 01 - ifcProject | properties | on 81 objects (81 IFCDOOR)
    Test AA = "YD-" (IFCLABEL)
    Test BB = "300" (IFCLABEL)
    Test CC = "Existing" (IFCLABEL)
  Skeisvang Pset: TEST 01 - ifcProject: 525 more contents on 2817 objects not shown
  BaseQuantities | quantities | on 181 objects (181 IFCSLAB)
    GrossArea = 0.01999999999999602 [SQUARE_METRE]
    GrossVolume = 0.0009999999999998027 [CUBIC_METRE]
    NetArea = 0.002500000000001279 [SQUARE_METRE]
    NetVolume = 0.0001250000000000657 [CUBIC_METRE]
    Perimeter = 659.9999999999682 [MILLI METRE]
    Width = 49.99999999999999 [MILLI METRE]
  BaseQuantities | quantities | on 81 objects (81 IFCWINDOW)
    Area = 3.481499999999951 [SQUARE_METRE]
    Depth = 275. [MILLI METRE]
    GrossArea = 3.481499999999951 [SQUARE_METRE]
    Height = 2110. [MILLI METRE]
    NetVolume = 0.1051884727918922 [CUBIC_METRE]
    Perimeter = 7519.999999999954 [MILLI METRE]
    Volume = 0.1051884727918922 [CUBIC_METRE]
    Width = 1649.999999999977 [MILLI METRE]
  BaseQuantities | quantities | on 64 objects (64 IFCSLAB)
    GrossArea = 0.1860000000000084 [SQUARE_METRE]
    GrossVolume = 0.005580000000000464 [CUBIC_METRE]
    NetArea = 0.1860000000000084 [SQUARE_METRE]
    NetVolume = 0.005580000000000464 [CUBIC_METRE]
    Perimeter = 3340.000000000032 [MILLI METRE]
    Width = 30. [MILLI METRE]
  BaseQuantities | quantities | on 58 objects (58 IFCWINDOW)
    Area = 3.481500000000011 [SQUARE_METRE]
    Depth = 275. [MILLI METRE]
    GrossArea = 3.481500000000011 [SQUARE_METRE]
    Height = 2110. [MILLI METRE]
    NetVolume = 0.1051884727918922 [CUBIC_METRE]
    Perimeter = 7520.00000000001 [MILLI METRE]
    Volume = 0.1051884727918922 [CUBIC_METRE]
    Width = 1650.000000000006 [MILLI METRE]
  BaseQuantities | quantities | on 53 objects (53 IFCSLAB)
    GrossArea = 0.0179999999999971 [SQUARE_METRE]
    GrossVolume = 0.0008999999999998564 [CUBIC_METRE]
    NetArea = 0.002250000000001236 [SQUARE_METRE]
    NetVolume = 0.0001125000000000634 [CUBIC_METRE]
    Perimeter = 609.9999999999852 [MILLI METRE]
    Width = 49.99999999999999 [MILLI METRE]
  BaseQuantities | quantities | on 47 objects (47 IFCWINDOW)
    Area = 1.5 [SQUARE_METRE]
    Depth = 150. [MILLI METRE]
    GrossArea = 1.5 [SQUARE_METRE]
    Height = 1500. [MILLI METRE]
    NetVolume = 0.03707949200000001 [CUBIC_METRE]
    Perimeter = 5000. [MILLI METRE]
    Volume = 0.03707949200000001 [CUBIC_METRE]
    Width = 1000. [MILLI METRE]
  BaseQuantities | quantities | on 44 objects (44 IFCMEMBER)
    CrossSectionArea = 0.0075 [SQUARE_METRE]
    GrossSurfaceArea = 0.6702000000000009 [SQUARE_METRE]
    GrossVolume = 0.008775000000000012 [CUBIC_METRE]
    Length = 1170.000000000002 [MILLI METRE]
    NetVolume = 0.008775000000000012 [CUBIC_METRE]
    OuterSurfaceArea = 0.6552000000000009 [SQUARE_METRE]
    TotalSurfaceArea = 0.6702000000000009 [SQUARE_METRE]
  BaseQuantities | quantities | on 39 objects (39 IFCSLAB)
    GrossArea = 0.04950000000000204 [SQUARE_METRE]
    GrossVolume = 0.009900000000000374 [CUBIC_METRE]
    NetArea = 0.04950000000000204 [SQUARE_METRE]
    NetVolume = 0.009900000000000374 [CUBIC_METRE]
    Perimeter = 3360.000000000014 [MILLI METRE]
    Width = 200. [MILLI METRE]
  BaseQuantities: 3218 more contents on 4383 objects not shown
  Pset_CoveringCommon | properties | on 1274 objects (874 IFCSLAB, 398 IFCCOVERING, 2 IFCBUILDINGELEMENTPROXY)
    AcousticRating = "" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "" (IFCTEXT)
    FireRating = "" (IFCLABEL)
    FlammabilityRating = "" (IFCLABEL)
    FragilityRating = "" (IFCLABEL)
    Material = "" (IFCLABEL)
    Reference = "" (IFCIDENTIFIER)
    SurfaceSpreadOfFlame = "" (IFCLABEL)
  Pset_CoveringCommon | properties | on 5 objects (5 IFCCOVERING)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    Material = "9520 - HH 00 - Fast himling gips_Sylomar Akustikk Super T60 KOPI" (IFCLABEL)
    TotalThickness = 125. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 4 type objects
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    TotalThickness = 50. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 4 type objects
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    TotalThickness = 20. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 2 type objects
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    TotalThickness = 5. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 2 type objects
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    TotalThickness = 3. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 2 type objects
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    TotalThickness = 125. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 2 type objects
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    TotalThickness = 30. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon: 33 more contents on 0 objects not shown
  MMI | properties | on 3198 objects (874 IFCSLAB, 656 IFCBUILDINGELEMENTPART, 488 IFCMEMBER, 403 IFCCOVERING)
    MMI = "100" (IFCLABEL)
  MMI | properties | on 2092 objects (1156 IFCWALLSTANDARDCASE, 465 IFCBUILDINGELEMENTPART, 287 IFCDOOR, 103 IFCWINDOW)
    MMI = "300" (IFCLABEL)
  MMI | properties | on 785 objects (758 IFCWALLSTANDARDCASE, 27 IFCWALL)
    MMI = "400" (IFCLABEL)
  MMI | properties | on 5 objects (4 IFCBUILDINGELEMENTPART, 1 IFCWALL)
    MMI = "250" (IFCLABEL)
  Pset_FireRatingProperties | properties | on 5202 objects (1920 IFCWALLSTANDARDCASE, 874 IFCSLAB, 553 IFCBUILDINGELEMENTPART, 488 IFCMEMBER)
    FireResistanceRating = "" (IFCLABEL)
  Pset_FireRatingProperties | properties | on 164 objects (92 IFCBUILDINGELEMENTPART, 57 IFCWALLSTANDARDCASE, 15 IFCWALL)
    FireResistanceRating = "EI-60" (IFCLABEL)
  Pset_FireRatingProperties | properties | on 137 objects (122 IFCDOOR, 15 IFCWINDOW)
    FireResistanceRating = "B" (IFCLABEL)
  Pset_FireRatingProperties | properties | on 36 objects (36 IFCDOOR)
    FireResistanceRating = "EI30" (IFCLABEL)
  Pset_FireRatingProperties | properties | on 17 objects (16 IFCDOOR, 1 IFCWALLSTANDARDCASE)
    FireResistanceRating = "EI60" (IFCLABEL)
  Pset_FireRatingProperties | properties | on 12 objects (5 IFCWALLSTANDARDCASE, 4 IFCDOOR, 3 IFCWINDOW)
    FireResistanceRating = "EI..." (IFCLABEL)
  Pset_FireRatingProperties | properties | on 10 objects (10 IFCDOOR)
    FireResistanceRating = "b" (IFCLABEL)
  Pset_FireRatingProperties | properties | on 4 objects (4 IFCDOOR)
    FireResistanceRating = "E30C" (IFCLABEL)
  Pset_FireRatingProperties: 3 more contents on 6 objects not shown
  Pset_SlabCommon | properties | on 813 objects (813 IFCSLAB)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_SlabCommon | properties | on 44 objects (44 IFCSLAB)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_SlabCommon | properties | on 15 objects (15 IFCSLAB)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  AC_Pset_RenovationAndPhasing | properties | on 3697 objects (1611 IFCWALLSTANDARDCASE, 799 IFCSLAB, 402 IFCCOVERING, 257 IFCDOOR)
    Renovation Status = "New" (IFCLABEL)
  AC_Pset_RenovationAndPhasing | properties | on 1206 objects (570 IFCBUILDINGELEMENTPROXY, 488 IFCMEMBER, 148 IFCPLATE)
    Renovation Status = "Undefined" (IFCLABEL)
  AC_Pset_RenovationAndPhasing | properties | on 706 objects (375 IFCWALLSTANDARDCASE, 105 IFCDOOR, 75 IFCSLAB, 63 IFCWINDOW)
    Renovation Status = "Existing" (IFCLABEL)
  AC_Pset_Dimension | properties | on 14 objects (14 IFCCOVERING)
    Area = "0,2" (IFCLABEL)
    Height = "5" (IFCLABEL)
    Width = "5" (IFCLABEL)
  AC_Pset_Dimension | properties | on 11 objects (11 IFCBUILDINGELEMENTPROXY)
    Height = 0.3 (IFCABSORBEDDOSEMEASURE)
  AC_Pset_Dimension | properties | on 10 objects (10 IFCCOVERING)
    Area = "2,0" (IFCLABEL)
    Height = "50" (IFCLABEL)
    Width = "50" (IFCLABEL)
  AC_Pset_Dimension | properties | on 10 objects (10 IFCCOVERING)
    Area = "0,5" (IFCLABEL)
    Height = "5" (IFCLABEL)
    Width = "5" (IFCLABEL)
  AC_Pset_Dimension | properties | on 10 objects (10 IFCBUILDINGELEMENTPROXY)
    Height = 2.074980836993674 (IFCABSORBEDDOSEMEASURE)
  AC_Pset_Dimension | properties | on 10 objects (10 IFCBUILDINGELEMENTPROXY)
    Height = 2.075000028255265 (IFCABSORBEDDOSEMEASURE)
  AC_Pset_Dimension | properties | on 9 objects (9 IFCBUILDINGELEMENTPROXY)
    Height = 1.0750095835444 (IFCABSORBEDDOSEMEASURE)
  AC_Pset_Dimension | properties | on 8 objects (8 IFCCOVERING)
    Area = "0,3" (IFCLABEL)
    Height = "367" (IFCLABEL)
    Width = "367" (IFCLABEL)
  AC_Pset_Dimension: 337 more contents on 524 objects not shown
  Pset_PlateCommon | properties | on 148 objects (148 IFCPLATE)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WallCommon | properties | on 832 objects (756 IFCWALLSTANDARDCASE, 76 IFCWALL)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WallCommon | properties | on 708 objects (697 IFCWALLSTANDARDCASE, 11 IFCWALL)
    AcousticRating = "R'w 60 dB" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WallCommon | properties | on 349 objects (341 IFCWALLSTANDARDCASE, 8 IFCWALL)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WallCommon | properties | on 50 objects (37 IFCWALLSTANDARDCASE, 13 IFCWALL)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WallCommon | properties | on 39 objects (39 IFCWALLSTANDARDCASE)
    AcousticRating = "R'w 50 dB" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WallCommon | properties | on 19 objects (19 IFCWALLSTANDARDCASE)
    AcousticRating = "" (IFCLABEL)
    FireRating = "EI-60" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WallCommon | properties | on 12 objects (12 IFCWALLSTANDARDCASE)
    AcousticRating = "" (IFCLABEL)
    FireRating = "EI-60" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WallCommon | properties | on 11 objects (10 IFCWALLSTANDARDCASE, 1 IFCWALL)
    AcousticRating = "R'w 70 dB" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WallCommon: 24 more contents on 96 objects not shown
  Pset_WindowCommon | properties | on 150 objects (150 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 2.832024 (IFCPOSITIVERATIOMEASURE)
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WindowCommon | properties | on 57 objects (57 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 1.078124 (IFCPOSITIVERATIOMEASURE)
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WindowCommon | properties | on 17 objects (17 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 3.301523999999997 (IFCPOSITIVERATIOMEASURE)
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WindowCommon | properties | on 11 objects (11 IFCWINDOW)
    AcousticRating = "L" (IFCLABEL)
    FireRating = "B" (IFCLABEL)
    GlazingAreaFraction = 2.832024 (IFCPOSITIVERATIOMEASURE)
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WindowCommon | properties | on 7 objects (7 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 3.619703999999999 (IFCPOSITIVERATIOMEASURE)
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WindowCommon | properties | on 4 objects (4 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 12.00422 (IFCPOSITIVERATIOMEASURE)
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WindowCommon | properties | on 3 objects (3 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 4.189283999999999 (IFCPOSITIVERATIOMEASURE)
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WindowCommon | properties | on 2 objects (2 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 1.747584 (IFCPOSITIVERATIOMEASURE)
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WindowCommon: 32 more contents on 39 objects not shown
  Pset_DoorCommon | properties | on 46 objects (46 IFCDOOR)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_DoorCommon | properties | on 37 objects (37 IFCDOOR)
    AcousticRating = "L" (IFCLABEL)
    FireRating = "B" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_DoorCommon | properties | on 22 objects (22 IFCDOOR)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 1.080882 (IFCPOSITIVERATIOMEASURE)
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_DoorCommon | properties | on 19 objects (19 IFCDOOR)
    AcousticRating = "L" (IFCLABEL)
    FireRating = "B" (IFCLABEL)
    GlazingAreaFraction = 1.0653 (IFCPOSITIVERATIOMEASURE)
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_DoorCommon | properties | on 17 objects (17 IFCDOOR)
    AcousticRating = "L" (IFCLABEL)
    FireRating = "B" (IFCLABEL)
    GlazingAreaFraction = 0.8437519999999997 (IFCPOSITIVERATIOMEASURE)
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_DoorCommon | properties | on 15 objects (15 IFCDOOR)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_DoorCommon | properties | on 14 objects (14 IFCDOOR)
    AcousticRating = "L" (IFCLABEL)
    FireRating = "B" (IFCLABEL)
    GlazingAreaFraction = 1.064524911641186 (IFCPOSITIVERATIOMEASURE)
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_DoorCommon | properties | on 10 objects (10 IFCDOOR)
    AcousticRating = "43 dB" (IFCLABEL)
    FireRating = "EI30" (IFCLABEL)
    GlazingAreaFraction = 0.6355 (IFCPOSITIVERATIOMEASURE)
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_DoorCommon: 78 more contents on 182 objects not shown
  Pset_MemberCommon | properties | on 222 objects (222 IFCMEMBER)
    FireRating = "" (IFCLABEL)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_MemberCommon | properties | on 168 objects (168 IFCMEMBER)
    FireRating = "" (IFCLABEL)
    Slope = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_MemberCommon | properties | on 9 objects (9 IFCMEMBER)
    FireRating = "" (IFCLABEL)
    Slope = 69.8141969905362 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_MemberCommon | properties | on 6 objects (6 IFCMEMBER)
    FireRating = "" (IFCLABEL)
    Slope = 88.48811738971428 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_MemberCommon | properties | on 5 objects (5 IFCMEMBER)
    FireRating = "" (IFCLABEL)
    Slope = 88.6093022115804 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_MemberCommon | properties | on 5 objects (5 IFCMEMBER)
    FireRating = "" (IFCLABEL)
    Slope = 88.61729798631046 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_MemberCommon | properties | on 5 objects (5 IFCMEMBER)
    FireRating = "" (IFCLABEL)
    Slope = 84.54586745867338 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_MemberCommon | properties | on 2 objects (2 IFCMEMBER)
    FireRating = "" (IFCLABEL)
    Slope = 88.48811738971403 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_MemberCommon: 63 more contents on 66 objects not shown
  Pset_BeamCommon | properties | on 31 objects (31 IFCBEAM)
    FireRating = "" (IFCLABEL)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Stål 50 x 10" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_BeamCommon | properties | on 10 objects (10 IFCBEAM)
    FireRating = "" (IFCLABEL)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "HE 180 A (1) 180 x 171" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_BeamCommon | properties | on 8 objects (8 IFCBEAM)
    FireRating = "" (IFCLABEL)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "HEA 340 330 x 300" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_BeamCommon | properties | on 4 objects (4 IFCBEAM)
    FireRating = "" (IFCLABEL)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Betong - Prefab 300 x 580" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_BeamCommon | properties | on 2 objects (2 IFCBEAM)
    FireRating = "" (IFCLABEL)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Kantbjelke 320-L 110 x 320" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_BeamCommon | properties | on 2 objects (2 IFCBEAM)
    FireRating = "" (IFCLABEL)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Kantbjelke rekkverk 8 x 472" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_BeamCommon | properties | on 2 objects (2 IFCBEAM)
    FireRating = "" (IFCLABEL)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Overgangsbeslag amfi mot bygg A 270 x 2" (IFCIDENTIFIER)
    Slope = 26.561 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_BeamCommon | properties | on 2 objects (2 IFCBEAM)
    FireRating = "" (IFCLABEL)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Overgangsbeslag amfi mot bygg A 270 x 2" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_BeamCommon: 8 more contents on 11 objects not shown
  Pset_ColumnCommon | properties | on 92 objects (92 IFCCOLUMN)
    FireRating = "" (IFCLABEL)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Aluminium 50 x 10" (IFCIDENTIFIER)
    Slope = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 33 objects (33 IFCCOLUMN)
    FireRating = "" (IFCLABEL)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Petal Kontur K7 600 600 x 14" (IFCIDENTIFIER)
    Slope = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 10 objects (10 IFCCOLUMN)
    FireRating = "" (IFCLABEL)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "HUP 100x100x10 100 x 100" (IFCIDENTIFIER)
    Slope = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 4 objects (4 IFCCOLUMN)
    FireRating = "" (IFCLABEL)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Petal Kontur K7 300 300 x 14" (IFCIDENTIFIER)
    Slope = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 3 objects (3 IFCCOLUMN)
    FireRating = "" (IFCLABEL)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Stål D300" (IFCIDENTIFIER)
    Slope = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 3 objects (3 IFCCOLUMN)
    FireRating = "" (IFCLABEL)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Aluminium D60" (IFCIDENTIFIER)
    Slope = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 3 objects (3 IFCCOLUMN)
    FireRating = "" (IFCLABEL)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Aluminium D100" (IFCIDENTIFIER)
    Slope = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 2 objects (2 IFCCOLUMN)
    FireRating = "" (IFCLABEL)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Overgangsbeslag amfi mot bygg A 270 x 2" (IFCIDENTIFIER)
    Slope = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon: 7 more contents on 9 objects not shown
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Pset_ManufacturerOccurrence | properties | on 566 objects (566 IFCBUILDINGELEMENTPROXY)
    SerialNumber = "" (IFCIDENTIFIER)
  Pset_ManufacturerOccurrence | properties | on 11 objects (11 IFCBUILDINGELEMENTPROXY)
    SerialNumber = "Av" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 577 objects (577 IFCBUILDINGELEMENTPROXY)
    Manufacturer = "" (IFCLABEL)
    ProductionYear = "" (IFCLABEL)
  Pset_RoofCommon | properties | on 18 objects (18 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
  Pset_CurtainWallCommon | properties | on 4 objects (4 IFCCURTAINWALL)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_StairCommon | properties | on 3 objects (3 IFCSTAIR)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 18. (IFCCOUNTMEASURE)
    NumberOfTreads = 17. (IFCCOUNTMEASURE)
    RequiredHeadroom = 2200. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    RiserHeight = 183.3333333333333 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairCommon | properties | on 2 objects (2 IFCSTAIR)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 18. (IFCCOUNTMEASURE)
    NumberOfTreads = 17. (IFCCOUNTMEASURE)
    RequiredHeadroom = 2200. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    RiserHeight = 150. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 16. (IFCCOUNTMEASURE)
    NumberOfTreads = 15. (IFCCOUNTMEASURE)
    RequiredHeadroom = 2200. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    RiserHeight = 220.3543436170465 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 13. (IFCCOUNTMEASURE)
    NumberOfTreads = 12. (IFCCOUNTMEASURE)
    RequiredHeadroom = 2200. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    RiserHeight = 253.8461538461538 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 19. (IFCCOUNTMEASURE)
    NumberOfTreads = 18. (IFCCOUNTMEASURE)
    RequiredHeadroom = 2200. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    RiserHeight = 173.6842105263158 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 5. (IFCCOUNTMEASURE)
    NumberOfTreads = 4. (IFCCOUNTMEASURE)
    RequiredHeadroom = 2200. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    RiserHeight = 124. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]